IPECS-SWITCH3000-MIB DEFINITIONS ::= BEGIN

IMPORTS

        MODULE-IDENTITY, OBJECT-TYPE, Unsigned32, Integer32, Counter32,
        IpAddress, NOTIFICATION-TYPE, enterprises, TimeTicks
                FROM SNMPv2-SMI
        DisplayString, RowStatus, MacAddress, TruthValue
                FROM SNMPv2-TC
        PortList, VlanIndex
                FROM Q-BRIDGE-MIB
        InetAddressType, InetAddress
                FROM INET-ADDRESS-MIB
        InterfaceIndex, ifIndex
                FROM IF-MIB
        EnabledStatus
                FROM P-BRIDGE-MIB
		BridgeId, Timeout, dot1dStpPort, dot1dStpPortEntry
                FROM BRIDGE-MIB
        pethPsePortEntry
                FROM POWER-ETHERNET-MIB
        dot1xAuthConfigEntry
                FROM IEEE8021-PAE-MIB;

ericssonLg             OBJECT IDENTIFIER ::= { enterprises 572 }
ipecsSwitchMgt         OBJECT IDENTIFIER ::= { ericssonLg 17389 }

ipecsEs3000MIB MODULE-IDENTITY
        LAST-UPDATED "201110190000Z"
        ORGANIZATION "Ericsson-LG Co., Ltd."
        CONTACT-INFO
                ""
        DESCRIPTION
                ""
        REVISION "200909300000Z"
        DESCRIPTION
                "Initial version of this MIB."
        ::= { ipecsSwitchMgt 13000 }

ipecsEs3000MIBObjects       OBJECT IDENTIFIER ::= { ipecsEs3000MIB 1 }
ipecsEs3000Notifications    OBJECT IDENTIFIER ::= { ipecsEs3000MIB 2 }

--supported groups

switchMgt           OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 1 }
portMgt             OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 2 }
trunkMgt            OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 3 }
lacpMgt             OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 4 }
staMgt              OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 5 }
restartMgt          OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 7 }
mirrorMgt           OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 8 }
igmpSnoopMgt        OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 9 }
ipMgt               OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 10 }
vlanMgt             OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 12 }
priorityMgt         OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 13 }
trapDestMgt         OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 14 }
qosMgt              OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 16 }
securityMgt         OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 17 }
sysLogMgt           OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 19 }
lineMgt             OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 20 }
sysTimeMgt          OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 23 }
fileMgt             OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 24 }
dnsMgt              OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 26 }
poeMgt              OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 28 }
stormMgt            OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 33 }
sysResourceMgt      OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 39 }
mvrMgt              OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 44 }
dhcpSnoopMgt        OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 46 }
clusterMgt          OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 47 }
ipSrcGuardMgt       OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 48 }
upnpMgt             OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 49 }
dynamicArpInspectionMgt     OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 56 }
timeRangeMgt                OBJECT IDENTIFIER ::= { ipecsEs3000MIBObjects 61 }

--
-- Product sysObjectID values
--

es3024GP  OBJECT IDENTIFIER ::= { ipecsSwitchMgt 101 }
es3024G   OBJECT IDENTIFIER ::= { ipecsSwitchMgt 102 }
es3026P   OBJECT IDENTIFIER ::= { ipecsSwitchMgt 103 }
es3026    OBJECT IDENTIFIER ::= { ipecsSwitchMgt 104 }

-- -------------------------------------------------------------
-- Textual Conventions
-- -------------------------------------------------------------

KeySegment ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The total length of the key is 1024 characters,
         it is divided into 8 parts and stored in 8 separated mib
         variables as below:

             Key1: part 1 of the key (1-128)
             Key2: part 2 of the key (129-256)
             Key3: part 3 of the key (257-384)
             Key4: part 4 of the key (385-512)
             Key5: part 5 of the key (513-640)
             Key6: part 6 of the key (641-768)
             Key7: part 7 of the key (769-896)
             Key8: part 8 of the key (897-1024)

         Please note that if the key string is less then 1024 characters,
         the remaining part of the string will be filled by a zero-length string.
         For example, if the length of the key is 129,
         we will get a string of length 128 in Key1, and
         a string of length 1 in Key2,
         moreover, Key3 to Key8 will all be zero-length strings."
    SYNTAX      DisplayString(SIZE(0..128))

ValidStatus ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "A simple status value for the object to create and destroy
         a table entry. This is a simplified variant of RowStatus as it
         supports only two values. Setting it to valid(1) creates an entry.
         Setting it to invalid(2) destroys an entry."
    SYNTAX      INTEGER { valid(1), invalid(2) }

StaPathCostMode ::= TEXTUAL-CONVENTION
     STATUS  current
     DESCRIPTION
         "The path cost mode of a spanning tree algorithm, short(1) indicates
          that we retrieve/configure the spanning tree path cost as a 16 bit
          value and long(2) indicates that we retrieve/configure the spanning
          tree path cost as a 32 bit value."
     SYNTAX      INTEGER { short(1), long(2) }

--
-- switchMgt
--

-- Management for the switch system, or individual units
-- in a stackable switch system. For a non-stackable system,
-- only unit 1 exists.

switchNumber OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The total number of switches present on this system."
        ::= { switchMgt 2 }

switchInfoTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF SwitchInfoEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     the switch units in this system."
        ::= { switchMgt 3 }

switchInfoEntry OBJECT-TYPE
        SYNTAX      SwitchInfoEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table providing descriptions and status information for
                     switch units."
        INDEX       { swUnitIndex }
        ::= { switchInfoTable 1 }

SwitchInfoEntry ::= SEQUENCE
{
    swUnitIndex             Integer32,
    swHardwareVer           DisplayString,
    swMicrocodeVer          DisplayString,
    swLoaderVer             DisplayString,
    swOpCodeVer             DisplayString,
    swPortNumber            Integer32,
    swPowerStatus           INTEGER,
    swRoleInSystem          INTEGER,
    swSerialNumber          DisplayString,
    swServiceTag            DisplayString,
    swModelNumber           DisplayString,
    swCpldVer               DisplayString
}

swUnitIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This object identifies the switch within the system
                     for which this entry contains information. This
                     value can never be greater than switchNumber."
        ::= { switchInfoEntry 1 }

swHardwareVer OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..20))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Hardware version of the main board."
        ::= { switchInfoEntry 2 }

swMicrocodeVer OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..20))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Microcode version of the main board."
        ::= { switchInfoEntry 3 }

swLoaderVer OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..20))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Loader version of the main board."
        ::= { switchInfoEntry 4 }

swOpCodeVer OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..20))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Operation code version of the main board."
        ::= { switchInfoEntry 6 }

swPortNumber OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The number of ports on this switch."
        ::= { switchInfoEntry 7 }

swPowerStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        internalPower(1),
                        redundantPower(2),
                        internalAndRedundantPower(3)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the switch using internalPower(1),
                     redundantPower(2) or both(3)"
        ::= { switchInfoEntry 8 }

swRoleInSystem OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        master(1),
                        backupMaster(2),
                        slave(3)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the switch is master(1), backupMaster(2)
                     or slave(3) in this system."
        ::= { switchInfoEntry 9 }

swSerialNumber OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..80))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Serial number of the switch."
        ::= { switchInfoEntry 10 }

swServiceTag OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..80))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Service tag serial-number of the switch."
        ::= { switchInfoEntry 13 }

swModelNumber OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..15))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Model number of the switch."
        ::= { switchInfoEntry 14 }

swCpldVer OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..20))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The CPLD version of the switch."
        ::= { switchInfoEntry 17 }

switchOperState OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        other(1),
                        unknown(2),
                        ok(3),
                        noncritical(4),
                        critical(5),
                        nonrecoverable(6)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Global operation state of the switch."
        ::= { switchMgt 4 }

switchProductId     OBJECT IDENTIFIER ::= { switchMgt 5 }

swProdName OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..127))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The product name of this switch."
        ::= { switchProductId 1 }

swProdManufacturer OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..127))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The product manufacturer of this switch."
        ::= { switchProductId 2 }

swProdDescription OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..127))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The product description of this switch."
        ::= { switchProductId 3 }

swProdVersion OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..127))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The runtime code version of this switch."
        ::= { switchProductId 4 }

swProdUrl OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..127))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The URL of this switch, which we can connect through
                     a web browser."
        ::= { switchProductId 5 }

swIdentifier OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "A unique identifier of which switch in the chassis is currently
                     being looked at."
        ::= { switchProductId 6 }

swChassisServiceTag OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..80))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The service tag of the chassis this switch resides in."
        ::= { switchProductId 7 }

switchIndivPowerTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF SwitchIndivPowerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table about the status of individual powers."
        ::= { switchMgt 6 }

switchIndivPowerEntry OBJECT-TYPE
        SYNTAX      SwitchIndivPowerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table about the status of individual power."
        INDEX       { swIndivPowerUnitIndex, swIndivPowerIndex }
        ::= { switchIndivPowerTable 1 }

SwitchIndivPowerEntry ::= SEQUENCE
{
    swIndivPowerUnitIndex   Integer32,
    swIndivPowerIndex       INTEGER,
    swIndivPowerStatus      INTEGER
}

swIndivPowerUnitIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  accessible-for-notify
        STATUS      current
        DESCRIPTION "This is defined as swUnitIndex."
        ::= { switchIndivPowerEntry 1 }

swIndivPowerIndex OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                      internalPower(1),
                      externalPower(2)
                    }
        MAX-ACCESS  accessible-for-notify
        STATUS      current
        DESCRIPTION "1 means internal power, 2 means external power."
        ::= { switchIndivPowerEntry 2 }

swIndivPowerStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        notPresent(1),
                        green(2),
                        red(3)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "notPresent(1) means not present, green(2) means
                     up, red(3) means down."
        ::= { switchIndivPowerEntry 3 }

switchJumboFrameStatus OBJECT-TYPE
         SYNTAX     INTEGER
                    {
                        enabled(1),
                        disabled(2)
                    }
         MAX-ACCESS read-write
         STATUS     current
         DESCRIPTION "enable(1) means the Jumbo Frame has enabled, disabled(2)
                     means the Jumbo Frame has disabled."
         ::= { switchMgt 7 }

-- Address Management

amtrMgt      OBJECT IDENTIFIER   ::= { switchMgt 8 }

amtrMacAddrAgingStatus OBJECT-TYPE
         SYNTAX     EnabledStatus
         MAX-ACCESS read-write
         STATUS     current
         DESCRIPTION "If this is enabled(1), the MAC address table will age out according to
                      its timer. If this is disabled(2), the MAC address table will not
                      age out."
         ::= { amtrMgt 3 }

--switchFanTable

switchFanTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF SwitchFanEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The fan status table."
       ::= { switchMgt 9 }

switchFanEntry OBJECT-TYPE
       SYNTAX      SwitchFanEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "A conceptual row of the switchFanTable."
       INDEX  { switchUnitIndex, switchFanIndex }
       ::= { switchFanTable 1 }

SwitchFanEntry ::= SEQUENCE
{
    switchUnitIndex       Integer32,
    switchFanIndex        Integer32,
    switchFanStatus       INTEGER,
    switchFanFailureCount Integer32
}

switchUnitIndex OBJECT-TYPE
       SYNTAX      Integer32
       MAX-ACCESS  accessible-for-notify
       STATUS      current
       DESCRIPTION "The unit of the switch for the stackable device."
       ::= { switchFanEntry 1 }

switchFanIndex OBJECT-TYPE
       SYNTAX      Integer32
       MAX-ACCESS  accessible-for-notify
       STATUS      current
       DESCRIPTION "The unit number of the fan."
       ::= { switchFanEntry 2 }

switchFanStatus OBJECT-TYPE
       SYNTAX   INTEGER
                {
                    ok(1),
                    failure(2)
                }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "Indicating the status of the fan, 1:ok; 2:failure."
       ::= { switchFanEntry 3 }

switchFanFailureCount OBJECT-TYPE
       SYNTAX      Integer32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "The total failure count of the fan since the switch
                    has reboot."
       ::= { switchFanEntry 5 }

switchRenumberUnitID OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        renumber(1),
                        noRenumber(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The value renumber will automatically assign an ID to
                     units in the stack; all UNIT IDs will be contiguous.
                     The system configurations are not changed but the system
                     will restart after renumbering is completed."
        ::= { switchMgt 14 }

--
-- portMgt
--

-- Management ports. This group also provides information
-- related to trunks because they share the same properties.

portTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information describing
                     the configuration of each switch port. This table also
                     contains information about each trunk."
        ::= { portMgt 1 }

portEntry OBJECT-TYPE
        SYNTAX      PortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, describing the configuration of
                     one switch port or trunk."
        INDEX       { portIndex }
        ::= { portTable 1 }

PortEntry ::= SEQUENCE
{
    portIndex                   Integer32,
    portName                    DisplayString,
    portType                    INTEGER,
    portSpeedDpxCfg             INTEGER,
    portFlowCtrlCfg             INTEGER,
    portCapabilities            BITS,
    portAutonegotiation         EnabledStatus,
    portSpeedDpxStatus          INTEGER,
    portFlowCtrlStatus          INTEGER,
    portTrunkIndex              Integer32,
    portComboForcedMode         INTEGER,
    portMacAddrLearningStatus   EnabledStatus,
    portMacAddrLearningCount    Counter32
}

portIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and the trunk (including trunk members) interface of
                     the portTable. The interface identified by a particular value
                     of this index is the same interface as identified by the same
                     value of ifIndex in the IF-MIB."
        ::= { portEntry 1 }

portName OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..64))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The name of the port or trunk. This is the same as ifAlias
                     in the IF-MIB (RFC2863 or later)."
        ::= { portEntry 2 }

portType OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        other(1),
                        hundredBaseTX(2),
                        hundredBaseFX(3),
                        thousandBaseSX(4),
                        thousandBaseLX(5),
                        thousandBaseT(6),
                        thousandBaseGBIC(7),
                        thousandBaseSfp(8),
                        hundredBaseFxScSingleMode(9),
                        hundredBaseFxScMultiMode(10),
                        thousandBaseCX(11)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the port type of the configuration of the switch."
        ::= { portEntry 3 }

portSpeedDpxCfg OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        reserved(1),
                        halfDuplex10(2),
                        fullDuplex10(3),
                        halfDuplex100(4),
                        fullDuplex100(5),
                        halfDuplex1000(6),
                        fullDuplex1000(7)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Configures the speed and duplex mode for a port or trunk,
                     according to:
                         halfDuplex10(2)    - 10Mbps and half duplex mode
                         fullDuplex10(3)    - 10Mbps and full duplex mode
                         halfDuplex100(4)   - 100Mbps and half duplex mode
                         fullDuplex100(5)   - 100Mbps and full duplex mode
                         halfDuplex1000(6)  - 1000Mbps and half duplex mode
                         fullDuplex1000(7)  - 1000Mbps and full duplex mode

                        hundredBaseTX  port can be set as:
                         halfDuplex10(2)
                         fullDuplex10(3)
                         halfDuplex100(4)
                         fullDuplex100(5)
                        hundredBaseFX  port can be set as:
                            fullDuplex100(5)
                        thousandBaseSX port can be set as:
                            fullDuplex1000(7)
                        thousandBaseLX port can be set as:
                            fullDuplex1000(7)
                        thousandBaseT port can be set as:
                            halfDuplex10(2)
                            fullDuplex10(3)
                            halfDuplex100(4)
                            fullDuplex100(5)
                        thousandBaseGBIC port can be set as:
                            fullDuplex1000(7)
                        thousandBaseSfp port can be set as:
                            fullDuplex1000(7)
                        hundredBaseFxScSingleMode port can be set as:
                            fullDuplex100(5)
                        hundredBaseFxScMultiMode port can be set as:
                            fullDuplex100(5)
                        thousandBaseCX port can be set as:
                            fullDuplex1000(7)

                     The actual operating speed and duplex of the port
                     is given by portSpeedDpxStatus."
        DEFVAL      { halfDuplex10 }
        ::= { portEntry 4 }

portFlowCtrlCfg OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        enabled(1),
                        disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "(1) Flow control mechanism is enabled with tx and rx pause
                         mechansim.
                         If the port type is hundredBaseTX or thousandBaseSX:
                         When the port is operating in halfDuplex mode, the
                         port uses backPressure flow control mechanism. When
                         the port is operating in fullDuplex mode, the port
                         uses IEEE 802.3x flow control mechanism.
                         If the port type is hundredBaseFX:
                         When the port is operating in halfDuplex mode, the
                         port uses backPressure flow control mechanism. When
                         the port is operating in fullDuplex mode, Flow
                         control mechanism will not function.
                     (2) Flow control mechanism is disabled.

                     Fast ethernet and gigabit ethernet ports can be set as:
                         enabled(1),
                         disabled(2).
                     The actual flow control mechanism is used given by
                     portFlowCtrlStatus."
        DEFVAL      { disabled }
        ::= { portEntry 5 }

portCapabilities OBJECT-TYPE
        SYNTAX      BITS
                    {
                        portCap10half(0),
                        portCap10full(1),
                        portCap100half(2),
                        portCap100full(3),
                        portCap1000half(4),
                        portCap1000full(5),
                        portCapSym(14),
                        portCapFlowCtrl(15)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Port or trunk capabilities."
        ::= { portEntry 6 }

portAutonegotiation OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Whether auto-negotiation is enabled."
        ::= { portEntry 7 }

portSpeedDpxStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        error(1),
                        halfDuplex10(2),
                        fullDuplex10(3),
                        halfDuplex100(4),
                        fullDuplex100(5),
                        halfDuplex1000(6),
                        fullDuplex1000(7)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The operating speed and duplex mode of the
                     switched port or trunk. If the entry represents a trunk,
                     the speed is that of its individual members unless
                     the member ports have been inconsistently configured
                     in which case the value is error(1)."
        ::= { portEntry 8 }

portFlowCtrlStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        error(1),
                        backPressure(2),
                        dot3xFlowControl(3),
                        none(4)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "(2) BackPressure flow control mechanism is used.
                     (3) IEEE 802.3 flow control mechanism is used.
                     (4) Flow control mechanism is disabled.
                     If the entry represents a trunk and the member ports
                     have been inconsistently configured then this value
                     is error(1)."
        ::= { portEntry 9 }

portTrunkIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The trunk to which this port belongs. A value of 0
                    means that this port does not belong to any trunk.
                    A value greater than zero means that this port
                    belongs to a trunk in the trunkIndex, defined by the
                    corresponding trunkPorts."
        ::= { portEntry 10 }

portComboForcedMode  OBJECT-TYPE
       SYNTAX     INTEGER
                  {
                    none(1),
                    copperForced(2),
                    sfpForced(4),
                    sfpPreferredAuto(5)
                  }
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION "This determines the running mode of a combo port.
                    For a non-combo port, this variable has a value of none(1),
                    and setting this variable to none(1) has no effect.
                    For a combo port, this has its own valid values not
                    equal to none(1), and setting this variable to none(1) is
                    not allowed. copperForced(2) is set if user want to force
                    this combo port running in copper mode. sfpForced(4)
                    is set if user want to force this combo port running in fiber
                    mode. sfpPreferredAuto(5) is set if user want to change copper or
                    fiber mode automatically by SFP transceiver present state. If SFP
                    transceiver is present, this combo port will run in fiber mode, and
                    if SFP transceiver is not present, this combo port will run in
                    copper mode."
       ::= { portEntry 12 }

portMacAddrLearningStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Set this variable to enabled(1) to start to learn MAC
                     addresses. Set this variable to disabled(2) to stop to
                     learn MAC addresses."
        DEFVAL      { enabled }
        ::= { portEntry 17 }

portMacAddrLearningCount OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The current number of learned MAC addresses."
        ::= { portEntry 18 }

--
-- cable diagnostics
--

cableDiagMgt      OBJECT IDENTIFIER   ::= { portMgt 3 }

cableDiagCtlAction OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "To execute cable diagnostics on a port, assign
                     cableDiagCtlAction to the value of ifIndex defined
                     by the ifIndex in the IF-MIB. When read, this object
                     always returns 0."
        ::= { cableDiagMgt 1 }

cableDiagResultTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CableDiagResultEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for cable diagnostics result."
        ::= { cableDiagMgt 2 }

cableDiagResultEntry OBJECT-TYPE
        SYNTAX      CableDiagResultEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for cable diagnostics result."
        INDEX       { cableDiagResultIfIndex }
        ::= { cableDiagResultTable 1 }

CableDiagResultEntry ::= SEQUENCE
{
    cableDiagResultIfIndex            Integer32,
    cableDiagResultStatusPairA        INTEGER,
    cableDiagResultStatusPairB        INTEGER,
    cableDiagResultDistancePairA      Integer32,
    cableDiagResultDistancePairB      Integer32,
    cableDiagResultTime               DisplayString
}

cableDiagResultIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This is defined as the ifIndex."
        ::= { cableDiagResultEntry 1 }

cableDiagResultStatusPairA OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        notTestedYet(1),
                        ok(2),
                        open(3),
                        short(4),
                        impedanceMismatch(8),
                        failed(9),
                        notSupported(10),
                        noCable(11)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The result of cable diagnostics. If there is no fault
                     on the cable, the value is ok(2). Value notTestedYet(1)
                     means the pair is not tested yet. Value ok(2) means the
                     pair works well. Value open(3) means there is a lack of
                     continuity between pins at each end of the pair. Value
                     short(4) means conductors are short-circuited together on
                     the pair. Value impedanceMismatch(8) means different
                     quality cables connected together. Value failed(9) means
                     test failed. Value notSupported(10) means cable diagnostics
                     is not supported. Value noCable(11) means there is no
                     connected cable."
        ::= { cableDiagResultEntry 2 }

cableDiagResultStatusPairB OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        notTestedYet(1),
                        ok(2),
                        open(3),
                        short(4),
                        impedanceMismatch(8),
                        failed(9),
                        notSupported(10),
                        noCable(11)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The result of cable diagnostics. If there is no fault
                     on the cable, the value is ok(2). Value notTestedYet(1)
                     means the pair is not tested yet. Value ok(2) means the
                     pair works well. Value open(3) means there is a lack of
                     continuity between pins at each end of the pair. Value
                     short(4) means conductors are short-circuited together on
                     the pair. Value impedanceMismatch(8) means different
                     quality cables connected together. Value failed(9) means
                     test failed. Value notSupported(10) means cable diagnostics
                     is not supported. Value noCable(11) means there is no
                     connected cable."
        ::= { cableDiagResultEntry 3 }

cableDiagResultDistancePairA OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Displays the fault distance of pair A of the cable
                     in meters."
        ::= { cableDiagResultEntry 6 }

cableDiagResultDistancePairB OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Displays the fault distance of pair B of the cable
                     in meters."
        ::= { cableDiagResultEntry 7 }

cableDiagResultTime OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..20))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Displays the last time of cable diagnostics.
                     For example, 'Jan  1 02:03:04 2002'."
        ::= { cableDiagResultEntry 11 }

--
-- loopback
--

loopbackTestMgt      OBJECT IDENTIFIER   ::= { portMgt 4 }

loopInternalCtlAction OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "To execute internal loopback test on a port, assign
                     loopInternalCtlAction to the value of ifIndex defined
                     by the ifIndex in the IF-MIB. When read, this object
                     always returns 0."
        ::= { loopbackTestMgt 1 }

loopInternalResultTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF LoopInternalResultEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for internal loopback test result."
        ::= { loopbackTestMgt 2 }

loopInternalResultEntry OBJECT-TYPE
        SYNTAX      LoopInternalResultEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for internal loopback test result."
        INDEX       { loopInternalResultIfIndex }
        ::= { loopInternalResultTable 1 }

LoopInternalResultEntry ::= SEQUENCE
{
    loopInternalResultIfIndex           Integer32,
    loopInternalResultStatus            INTEGER,
    loopInternalResultTime              DisplayString
}

loopInternalResultIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This is defined as the ifIndex."
        ::= { loopInternalResultEntry 1 }

loopInternalResultStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        notTestedYet(1),
                        succeeded(2),
                        failed(3)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The result of internal loopback."
        ::= { loopInternalResultEntry 2 }

loopInternalResultTime OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..20))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Displays the last time of internal loopback.
                     For example, 'Jan  1 02:03:04 2002'."
        ::= { loopInternalResultEntry 3 }

portUtilTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PortUtilEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Dispalys port utilization during recent 300 seconds."
        ::= { portMgt 6 }

portUtilEntry OBJECT-TYPE
        SYNTAX      PortUtilEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Dispalys port utilization during recent 300 seconds."
        INDEX       { portUtilIfIndex }
        ::= { portUtilTable 1 }

PortUtilEntry ::= SEQUENCE
{
    portUtilIfIndex     Integer32,
    portInOctetRate     Counter64,
    portInPacketRate    Counter64,
    portInUtil          Integer32,
    portOutOctetRate    Counter64,
    portOutPacketRate   Counter64,
    portOutUtil         Integer32
}

portUtilIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and trunk interface of the portUtilTable.
                     The interface identified by a particular value of this
                     index is the same interface identified by the same value
                     of ifIndex in the IF-MIB."
        ::= { portUtilEntry 1 }

portInOctetRate OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The input octet rate (kbits/sec) of the port."
        ::= { portUtilEntry 2 }

portInPacketRate OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The input packet rate (pkts/sec) of the port."
        ::= { portUtilEntry 3 }

portInUtil OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The input utilization of the port, in one per
                     hundred."
        ::= { portUtilEntry 4 }

portOutOctetRate OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The output octet rate (kbits/sec) of the port."
        ::= { portUtilEntry 5 }

portOutPacketRate OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The output packet rate (pkts/sec) of the port."
        ::= { portUtilEntry 6 }

portOutUtil OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The output utilization of the port, in one per
                     hundred."
        ::= { portUtilEntry 7 }

portVlanTrunkingTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PortVlanTrunkingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Configures vlan trunking feature."
    ::= { portMgt 7 }

portVlanTrunkingEntry OBJECT-TYPE
    SYNTAX      PortVlanTrunkingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Configures vlan trunking feature."
    INDEX       { portVlanTrunkingIfIndex }
    ::= { portVlanTrunkingTable 1 }

PortVlanTrunkingEntry ::= SEQUENCE
{
    portVlanTrunkingIfIndex     Integer32,
    portVlanTrunkingStatus      EnabledStatus
}

portVlanTrunkingIfIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The port and trunk interface of the portVlanTrunkingTable.
                 The interface identified by a particular value of this
                 index is the same interface identified by the same value
                 of ifIndex in the IF-MIB."
    ::= { portVlanTrunkingEntry 1 }

portVlanTrunkingStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Whether vlan trunking is enabled."
    ::= { portVlanTrunkingEntry 2 }

--
-- trunkMgt
--

-- Trunks: Provides additional information for Trunks


trunkMaxId OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximum number for a trunk identifier."
    ::= { trunkMgt 1 }

trunkValidNumber OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of valid trunks."
    ::= { trunkMgt 2 }

trunkTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF TrunkEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table describing the configuration and status of each
                     trunk."
        ::= { trunkMgt 3 }

trunkEntry OBJECT-TYPE
        SYNTAX      TrunkEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry describing the configuration and status of a
                     particular trunk."
        INDEX       { trunkIndex }
        ::= { trunkTable 1 }

TrunkEntry ::= SEQUENCE
{
    trunkIndex                Integer32,
    trunkPorts                PortList,
    trunkCreation             INTEGER,
    trunkStatus               ValidStatus
}

trunkIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Identifies the trunk within the switch that is
                     described by the table entry."
        ::= { trunkEntry 1 }

trunkPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The complete set of ports currently associated with
        this trunk."
    ::= { trunkEntry 2 }

trunkCreation OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    static(1),
                    lacp(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A value of static(1) means a statically configured trunk.
         A value of lacp(2) means an LACP-configured trunk."
    ::= { trunkEntry 3 }

trunkStatus OBJECT-TYPE
    SYNTAX      ValidStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Writing this to valid(1) creates an entry.
         Writing this to invalid(2) destroys an entry.
         A trunk created by LACP cannot be manually destroyed
         or (re)configured."
    ::= { trunkEntry 4 }

--
-- lacpMgt
--

-- Management for Link Aggregation Control Protocol (LACP, 802.3ad),
-- that is dynamic trunking.

lacpPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF LacpPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for LACP port configuration."
        ::= { lacpMgt 1 }

lacpPortEntry OBJECT-TYPE
        SYNTAX      LacpPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for LACP port configuration. While an entry may
                     exist for a particular port, the port may not support
                     LACP and an attempt to enable LACP may result in
                     failure."
        INDEX       { lacpPortIndex }
        ::= { lacpPortTable 1 }

LacpPortEntry ::= SEQUENCE
{
    lacpPortIndex            Integer32,
    lacpPortStatus           EnabledStatus
}

lacpPortIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port interface of the lacpPortTable. The interface
                     identified by a particular value of this index is the
                     same interface as identified by the same value of
                     ifIndex in the IF-MIB."
        ::= { lacpPortEntry 1 }

lacpPortStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Whether 802.3ad LACP is enabled."
        ::= { lacpPortEntry 2 }

--
-- staMgt
--

-- Management for Spanning Tree Algorithm (STA).
-- This has variables not already defined in the implemented
-- standard MIB(s).

staSystemStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Global spanning tree status.
                     (1) Spanning tree protocol is enabled.
                     (2) Spanning tree protocol is disabled."
        DEFVAL      { enabled }
        ::= { staMgt 1 }

staPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF StaPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The table manages port settings for Spanning Tree
                     Protocol 802.1d, 802.1w or 802.1s depending on the
                     value specified by staProtocolType."
        REFERENCE "IEEE 802.1d, IEEE 802.1w, IEEE 802.1s."
        ::= { staMgt 2 }

staPortEntry OBJECT-TYPE
        SYNTAX      StaPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual entry of staPortTable."
        AUGMENTS       { dot1dStpPortEntry }
        ::= { staPortTable 1 }

StaPortEntry ::= SEQUENCE
{
-- for MST, RSTP
    staPortProtocolMigration        TruthValue,
    staPortOperEdgePort             TruthValue,
    staPortAdminPointToPoint        INTEGER,
    staPortOperPointToPoint         TruthValue,
    staPortSystemStatus             EnabledStatus,
    staPortLongAdminPathCost        Integer32,
    staPortLongOperPathCost         Integer32,
    staPortBpduGuard                EnabledStatus,
    staPortAdminEdgePortWithAuto    INTEGER,
    staPortBpduFilter               EnabledStatus,
    staPortRootGuardStatus          EnabledStatus
}

-- for MSTP RSTP
staPortProtocolMigration OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "When operating in RSTP (version 2) mode, writing true(1)
         to this object forces this port to transmit RSTP BPDUs.
         Any other operation on this object has no effect and
         it always returns false(2) when read."
    REFERENCE
        "IEEE 802.1w clause 14.8.2.4, 17.18.10, 17.26"
    ::= { staPortEntry 3 }

staPortOperEdgePort OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational value of the edge port parameter. The object is
         initialized to the value of staPortAdminEdgePort and is set false
         when a BPDU is received."
    REFERENCE
        "IEEE 802.1t clause 14.8.2, 18.3.4"
    ::= { staPortEntry 5 }

staPortAdminPointToPoint OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    forceTrue(0),
                    forceFalse(1),
                    auto(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
     DESCRIPTION
        "The administrative point-to-point status of the LAN segment
         attached to this port.  A value of forceTrue(0) indicates that
         this port should always be treated as if it is connected to
         a point-to-point link.  A value of forceFalse(1) indicates
         that this port should be treated as having a shared media
         connection.  A value of auto(2) indicates that this port is
         considered to have a point-to-point link if it is an Aggregator
         and all of its members are aggregatable, or if the MAC entity
         is configured for full duplex operation, either through
         auto-negotiation or by management means."
   REFERENCE
       "IEEE 802.1w clause 6.4.3, 6.5, 14.8.2"
   ::= { staPortEntry 6 }

staPortOperPointToPoint OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational point-to-point status of the LAN segment
         attached to this port. This indicates whether a port is
         considered to have a point-to-point connection or not.
         The value is determined by management or by auto-detection,
         as described in the staPortAdminPointToPoint object."
    REFERENCE
        "IEEE 802.1w clause 6.4.3, 6.5, 14.8.2"
    ::= { staPortEntry 7 }

staPortSystemStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Per-port spanning tree status.
                     (1) Spanning tree protocol is enabled.
                     (2) Spanning tree protocol is disabled."
        DEFVAL      { enabled }
        ::= { staPortEntry 9 }

staPortLongAdminPathCost OBJECT-TYPE
    SYNTAX      Integer32(0..200000000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "The admin value of the RSTP path cost or MST external pathcost.
          The contribution of this port to the path cost (in 32
          bits value) of paths towards the spanning tree root which
          include this port.

          This object is used to configure the spanning tree port
          path cost in the 32-bit value range when the
          staPathCostMethod is long(2).

          If the staPathCostMethod is short(1), this mib object is not
          instantiated.

          Setting this to 0 means that the path cost is automatically
          determined. In this case, read staPortLongOperPathCost to get
          the oper value."
    ::= { staPortEntry 10 }

staPortLongOperPathCost OBJECT-TYPE
    SYNTAX      Integer32(1..200000000)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "The oper value of the RSTP path cost or MST external pathcost.
          The contribution of this port to the path cost (in 32
          bits value) of paths towards the spanning tree root which
          include this port.

          This object is used to configure the spanning tree port
          path cost in the 32-bit value range when the
          staPathCostMethod is long(2).

          If the staPathCostMethod is short(1), this mib object is not
          instantiated."
    ::= { staPortEntry 11 }

staPortBpduGuard         OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "A value of enabled(1) indicates that BPDU port guard feature
                 is enabled for each port. A value of disabled(2) indicates
                 that the feature is disabled."
    ::= { staPortEntry 15 }

staPortAdminEdgePortWithAuto OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    true(1),
                    false(2),
                    auto(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The administrative value of the edge port parameter.
    		A value of enable(1) indicates that this port should be
    		assumed as an edge-port, a value of disable(2) indicates
    		that this port should be assumed as a non-edge-port and
    		a value of auot (3) indicates this port in RSPT or MSTP mode
    		should be assumed as an edge-port after migration or max age expire
    		without receiving any BPDU and sending BPDU with proposal flag on."
    ::= { staPortEntry 16 }

staPortBpduFilter  OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The administrative value of the BPDU filter parameter.
                 A value of enabled(1) indicates that this port will avoid
                 transmitting BPDUs on edge-port and the value of disabled(2)
                 indicates that this port will not avoid transmitting BPDUs
                 on edge-port."
    ::= { staPortEntry 17 }

staPortRootGuardStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the desired status of the root guard. This variable
                 configures the root guard feature to enforce the root bridge
                 placement in the network."
    ::= { staPortEntry 18 }

staProtocolType OBJECT-TYPE
    SYNTAX      INTEGER {
                    stp(1),
                    rstp(2),
                    mstp(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The version of Spanning Tree Protocol the bridge is currently
                 running.  The value 'stp(1)' indicates the Spanning Tree
                 Protocol is as specified in IEEE 802.1D,'rstp(2)' indicates that
                 the Rapid Spanning Tree Protocol is as specified in IEEE
                 802.1w, and the value 'mstp(3)' indicates that the Multiple Spanning
                 Tree Protocol is as specified in IEEE 802.1s. New values may
                 be defined in the future as new or updated versions of the
                 protocol become available."
    REFERENCE
        "IEEE 802.1w clause 14.8.1, 17.12, 17.16.1"
    ::= { staMgt 3 }


staTxHoldCount OBJECT-TYPE
    SYNTAX      Integer32 (1..10)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value used by the Port Transmit state machine to limit
         the maximum transmission rate."
    REFERENCE
        "IEEE 802.1w clause 17.16.6"
    DEFVAL      { 3 }
    ::= { staMgt 4 }

staPathCostMethod    OBJECT-TYPE
    SYNTAX       StaPathCostMode
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION "Indicates the type of spanning tree path cost mode configured
                 on the switch. This mode applies to all instances of the
                 spanning tree protocol running on the switch.

                 When the value of this MIB object is changed, the path cost of
                 all ports will be reassigned to the default path cost values
                 based on the new spanning tree path cost mode and the
                 ports' speed.

                 When the value of this MIB object is set to long(2), the
                 staPortLongPathCost MIB object must be used to retrieve/configure
                 the spanning tree port path cost as a 32-bit value.
                 The set operation on dot1dStpPortPathCost in BRIDGE-MIB will be rejected.
                 While retrieving the value of dot1dStpPortPathCost, the maximum
                 value of 65535 will be returned if the value of staPortLongPathCost
                 for the same instance exceeds 65535.

                 When the value of this MIB object is set to short(1), the
                 dot1dStpPortPathCost in BRIDGE-MIB must be used."
   DEFVAL  { short }
   ::= { staMgt 5 }

-- for 1s(MSTP) start
--
-- xstMgt
--

xstMgt OBJECT IDENTIFIER ::= { staMgt 6 }

mstName OBJECT-TYPE
    SYNTAX      DisplayString(SIZE(0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The name of the Multiple Spanning Tree region."
    ::= { xstMgt 1 }

mstRevision OBJECT-TYPE
    SYNTAX      Integer32(0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The Revision number of the Multiple Spanning Tree region."
    ::= { xstMgt 2 }

mstMaxHops OBJECT-TYPE
    SYNTAX      Integer32(1..40)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The max hop number counts of the Multiple Spanning Tree region."
    ::= { xstMgt 3 }

xstInstanceCfgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF XstInstanceCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "This table is used to configure the property of a specific
                 instance in Multiple Spanning Tree or Rapid Spanning Tree.
                 If Rapid Spanning Tree protocol is in use, the
                 mstInstanceEditIndex is always 0."
    ::= { xstMgt 4 }

xstInstanceCfgEntry OBJECT-TYPE
    SYNTAX      XstInstanceCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A conceptual row containing the property of the RST or MST instance."
    INDEX       { xstInstanceCfgIndex }
    ::= { xstInstanceCfgTable 1 }

XstInstanceCfgEntry ::= SEQUENCE
{
      xstInstanceCfgIndex                    Integer32,
      xstInstanceCfgPriority                 Integer32,
      xstInstanceCfgTimeSinceTopologyChange  TimeTicks,
      xstInstanceCfgTopChanges               Integer32,
      xstInstanceCfgDesignatedRoot           BridgeId,
      xstInstanceCfgRootCost                 Integer32,
      xstInstanceCfgRootPort                 Integer32,
      xstInstanceCfgMaxAge                   Timeout,
      xstInstanceCfgHelloTime                Timeout,
      xstInstanceCfgHoldTime                 Timeout,
      xstInstanceCfgForwardDelay             Timeout,
      xstInstanceCfgBridgeMaxAge             Timeout,
      xstInstanceCfgBridgeHelloTime          Timeout,
      xstInstanceCfgBridgeForwardDelay       Timeout,
      xstInstanceCfgTxHoldCount              Integer32,
      xstInstanceCfgPathCostMethod           StaPathCostMode
}

xstInstanceCfgIndex OBJECT-TYPE
      SYNTAX      Integer32 (0..4094)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
          "An arbitrary integer within the range from 1 to the value of
          the maximum instance that uniquely identifies a spanning
          tree instance."
      ::= {xstInstanceCfgEntry 1 }

xstInstanceCfgPriority OBJECT-TYPE
     SYNTAX      Integer32 (0..61440)
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION "The priority of a specific spanning tree instance.
                  The value assigned should be in the range 0-61440
                  in steps of 4096."
     ::= { xstInstanceCfgEntry 2 }


xstInstanceCfgTimeSinceTopologyChange OBJECT-TYPE
     SYNTAX      TimeTicks
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION "The time (in hundredths of a second) since the last topology
                 change detected by the bridge entity in RST or MST."
     ::= { xstInstanceCfgEntry 3 }

xstInstanceCfgTopChanges OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION "The total number of topology changes detected by
                 this bridge in RST or MST since the management entity
                 was last reset or initialized."
     ::= { xstInstanceCfgEntry 4 }


xstInstanceCfgDesignatedRoot OBJECT-TYPE
     SYNTAX      BridgeId
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION "The bridge identifier of the root of the spanning
                 tree as determined by the Multiple Spanning Tree Protocol. (802.1s)
                 or Rapid Spanning Tree Protocol (802.1w) executed by this node.
                 This value is used as the root identifier parameter in
                 all configuration bridge PDUs originated by this node."
     REFERENCE   "IEEE 802.1w."
     ::= { xstInstanceCfgEntry 5 }

xstInstanceCfgRootCost OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION "The cost of the path to the root as seen from
                 this bridge of the RST or MST."
     ::= { xstInstanceCfgEntry 6 }


xstInstanceCfgRootPort OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION "The number of the port which offers the
                 lowest cost path from this bridge to the root
                 bridge of the RST or MST."
     ::= { xstInstanceCfgEntry 7 }

xstInstanceCfgMaxAge OBJECT-TYPE
     SYNTAX      Timeout
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION "The maximum age of Multiple Spanning Tree Protocol (802.1s)
                 or Rapid Spanning Tree Protocol (802.1w) information learned
                 from the network on any port before it is discarded,
                 in units of hundredths of a second. This is the actual
                 value that this bridge is currently using."
     ::= { xstInstanceCfgEntry 8 }


xstInstanceCfgHelloTime OBJECT-TYPE
     SYNTAX      Timeout
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION  "The amount of time between the transmission of
                  configuration bridge PDUs by this node on any port
                  when it is the root of the specific spanning tree or trying
                  to become so, in units of hundredths of a second.
                  This is the actual value that this bridge is
                  currently using in RST or MST."
     ::= { xstInstanceCfgEntry 9 }

xstInstanceCfgHoldTime OBJECT-TYPE
     SYNTAX      Timeout
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION  "This time value determines the interval length
                  during which no more than two configuration bridge
                  PDUs shall be transmitted by this node, in units
                  of hundredths of a second."
     ::= { xstInstanceCfgEntry 10 }

xstInstanceCfgForwardDelay OBJECT-TYPE
     SYNTAX      Timeout
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION  "For RST or MST protocol, this time value, measured in units of
                  hundredths of a second, controls how fast a port changes
                  its spanning state when moving towards the forwarding
                  state.  The value determines how long the port
                  stays in each of the listening and learning
                  states, which precede the forwarding state.  This
                  value is also used, when a topology change has
                  been detected and is underway, to age all dynamic
                  entries in the forwarding database. This value is the
                  current value being used by the bridge.
                  xstInstanceCfgBridgeForwardDelay defines the value that
                  this bridge and all others would start using
                  if/when this bridge were to become the root."
     ::= { xstInstanceCfgEntry 11 }

xstInstanceCfgBridgeMaxAge OBJECT-TYPE
     SYNTAX      Timeout
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION   "For RST or MST protocol, the time (in hundredths of second)
                   that all bridges use for MaxAge when this bridge is acting
                   as the root. Note that 802.1D-1990 specifies that the range
                   for this parameter is related to the value of
                   xstInstanceCfgBridgeHelloTime. The granularity of this
                   timer is specified by 802.1D-1990 to be 1 second."
     REFERENCE   "802.1D-1990."
     ::= { xstInstanceCfgEntry 12 }

xstInstanceCfgBridgeHelloTime OBJECT-TYPE
     SYNTAX      Timeout
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION   "For RST or MST protocol,the time (in hundredths of a second) that
                   all bridges use for HelloTime when this bridge is acting
                   as the root. The granularity of this timer is specified
                   by 802.1D-1990 to be 1 second."
     REFERENCE   "802.1D-1990."
     ::= { xstInstanceCfgEntry 13 }


xstInstanceCfgBridgeForwardDelay OBJECT-TYPE
     SYNTAX      Timeout
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION  "For RST or MST protocol, the time (in hundredths of a second)
                  that all bridges use for ForwardDelay when this bridge
                  is acting as the root.
                  Note that 802.1D-1990 specifies that the range for this
                  parameter is related to the value of
                  xstInstanceCfgBridgeMaxAge. The granularity of this
                  timer is specified by 802.1D-1990 to be 1 second."
     REFERENCE   "802.1D-1990."
     ::= { xstInstanceCfgEntry 14 }

xstInstanceCfgTxHoldCount OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION  "For RST or MST protocol, the value used by the port transmit
                  state machine to limit the maximum transmission rate."
     ::= { xstInstanceCfgEntry 15 }

xstInstanceCfgPathCostMethod OBJECT-TYPE
     SYNTAX      StaPathCostMode
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
       "For RST or MST protocol, this indicates the type of spanning tree path
       cost mode used by the switch. The mode applies to all instances of the
       Spanning Tree protocol running on the switch.

       When the value of this MIB object is changed, the path cost
       of all ports will be reassigned to the default path cost
       values based on the new spanning tree path cost mode and the
       ports' speed.

       When the value of this MIB object is set to long(2),
       the xstInstancePortAdminPathCost and xstInstancePortOperPathCost
       MIB objects must be used in order
       to retrieve/configure the spanning tree port path cost as a
       32-bit value. The set operation on dot1dStpPortPathCost in
       BRIDGE-MIB will be rejected. While retrieving the value of
       dot1dStpPortPathCost, the maximum value of 65535 will be
       returned if the value of xstInstancePortAdminPathCost for the same
       instance exceeds 65535.

       When the value of this MIB object is set to short(1),
       the dot1dStpPortPathCost in BRIDGE-MIB must be used."
     ::= { xstInstanceCfgEntry 16 }

xstInstancePortTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF XstInstancePortEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION "The extension table for dot1dStpPortEntry to provide
                 additional Spanning Tree information and configuration."
     ::= { xstMgt 5 }

xstInstancePortEntry OBJECT-TYPE
     SYNTAX      XstInstancePortEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION "The conceptual row for xstInstancePortTable."
     INDEX       { xstInstancePortInstance, xstInstancePortPort }
     ::= { xstInstancePortTable 1 }

XstInstancePortEntry ::= SEQUENCE
{
  xstInstancePortInstance           Integer32,
  xstInstancePortPort               Integer32,
  xstInstancePortPriority           Integer32,
  xstInstancePortState              INTEGER,
  xstInstancePortEnable             EnabledStatus,
  xstInstancePortDesignatedRoot     BridgeId,
  xstInstancePortDesignatedCost     Integer32,
  xstInstancePortDesignatedBridge   BridgeId,
  xstInstancePortDesignatedPort     OCTET STRING,
  xstInstancePortForwardTransitions Counter32,
  xstInstancePortPortRole           INTEGER,
  xstInstancePortAdminPathCost      Integer32,
  xstInstancePortOperPathCost       Integer32
}

xstInstancePortInstance OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION "The instance of the MSTP."
     ::= { xstInstancePortEntry 1 }

xstInstancePortPort OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION "The port and the trunk (excluding trunk member ports)
                  interface of the mstInstancePortTable. The interface identified
                  by a particular value of this index is the same interface
                  as identified by the same value of dot1dStpPort in the BRIDGE-MIB."
     ::= { xstInstancePortEntry 2 }

xstInstancePortPriority OBJECT-TYPE
     SYNTAX      Integer32(0..240)
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION "Defines the priority used for this port in the Spanning
                 Tree Algorithm. If the path cost for all ports on a
                 switch is the same, the port with the highest priority
                 (i.e., lowest value) will be configured as an active link
                 in the Spanning Tree. This makes a port with higher
                 priority less likely to be blocked if the Spanning Tree
                 Algorithm is detecting network loops. Where more than one
                 port is assigned the highest priority, the port with
                 lowest numeric identifier will be enabled."
     ::= { xstInstancePortEntry 3 }

xstInstancePortState OBJECT-TYPE
     SYNTAX      INTEGER {
                          discarding(1),
                          learning(2),
                          forwarding(3)
                         }
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION  "The port's current state as defined by application of
                  the Spanning Tree Protocol.  This state controls what
                  action a port takes on reception of a frame:
                  discarding(1): Port receives configuration messages,
                                 but does not forward packets.
                  learning(2):   Port has transmitted configuration messages
                                 for an interval set by the Forward Delay
                                 parameter without receiving contradictory
                                 information. Port address table is cleared,
                                 and the port begins learning addresses.
                  forwarding(3): Port forwards packets, and continues learning
                                 addresses.

                  For ports which are disabled (see xstInstancePortEnable),
                  this object will have a value of discarding(1)."
              ::= { xstInstancePortEntry 4 }

xstInstancePortEnable OBJECT-TYPE
     SYNTAX     EnabledStatus
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION    "The enabled/disabled status of the port."
     ::= { xstInstancePortEntry 5 }

xstInstancePortDesignatedRoot OBJECT-TYPE
     SYNTAX      BridgeId
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
                 "The unique bridge identifier of the bridge
                 recorded as the root in the configuration BPDUs
                 transmitted by the designated bridge for the
                 segment to which the port is attached."
     ::= { xstInstancePortEntry 7 }

xstInstancePortDesignatedCost OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
                 "The path cost of the designated port of the
                  segment connected to this port.  This value is
                  compared to the root path cost field in received
                  bridge PDUs."
     ::= { xstInstancePortEntry 8 }

xstInstancePortDesignatedBridge OBJECT-TYPE
     SYNTAX      BridgeId
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
                 "The bridge identifier of the bridge which this
                 port considers to be the designated bridge for
                 this port's segment."
     ::= { xstInstancePortEntry 9 }

xstInstancePortDesignatedPort OBJECT-TYPE
     SYNTAX      OCTET STRING (SIZE (2))
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
            "The port identifier of the port on the designated
            bridge for this port's segment."
     ::= { xstInstancePortEntry 10 }

xstInstancePortForwardTransitions OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of times this port has transitioned
             from the learning state to the forwarding state."
     ::= { xstInstancePortEntry 11 }

xstInstancePortPortRole OBJECT-TYPE
     SYNTAX  INTEGER
             {
               disabled(1),
               root(2),
               designated(3),
               alternate(4),
               backup(5),
               master(6)
             }
     MAX-ACCESS read-only
     STATUS current
     DESCRIPTION "The role of the port in the RST or MST protocol:
                  (1) The port has no role within the spanning tree
                  (2) The port is part of the active topology connecting
                      the bridge to the root bridge (i.e., root port)
                  (3) The port is connecting a LAN through the bridge to the
                      root bridge (i.e., designated port)
                  (4) The port may provide connectivity if other
                      bridges, bridge ports, or LANs fail or are removed.
                  (5) The port provides backup if other
                      bridges, bridge ports, or LANs fail or are removed.
                  (6) For MST protocol only, indicates whether this instance
                      is in a master role."
     ::= { xstInstancePortEntry 12 }

xstInstancePortAdminPathCost OBJECT-TYPE
     SYNTAX      Integer32(1..200000000)
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION "The admin value of the RST pathcost or MST internal pathcost,
                  in the range of 1 to 200000000.
                  This parameter is used to determine the best path between
                  devices. Therefore, lower values should be assigned to
                  ports attached to faster media, and higher values assigned
                  to ports with slower media. (Path cost takes precedence
                  over port priority)."
     ::= { xstInstancePortEntry 13 }

xstInstancePortOperPathCost OBJECT-TYPE
     SYNTAX      Integer32(1..200000000)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION "The oper value of the RST pathcost or MST internal pathcost,
                  in the range of 1 to 200000000.
                  This parameter is used to determine the best path between
                  devices. Therefore, lower values should be assigned to
                  ports attached to faster media, and higher values assigned
                  to ports with slower media. (Path cost takes precedence
                  over port priority)."
     ::= { xstInstancePortEntry 14 }

mstInstanceEditTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF MstInstanceEditEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION "The Multiple Spanning Tree region instance vlan configuration table.
                  Please read the actual instance vlan mapped in the mstInstanceOperTable."
     ::= { xstMgt 6 }

mstInstanceEditEntry OBJECT-TYPE
     SYNTAX      MstInstanceEditEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION  "A conceptual row containing the status of the MSTP instance."
     INDEX       { mstInstanceEditIndex }
     ::= { mstInstanceEditTable 1 }

MstInstanceEditEntry ::= SEQUENCE
{
    mstInstanceEditIndex      Integer32,
    mstInstanceEditVlansMap   OCTET STRING,
    mstInstanceEditVlansMap2k OCTET STRING,
    mstInstanceEditVlansMap3k OCTET STRING,
    mstInstanceEditVlansMap4k OCTET STRING,
    mstInstanceEditRemainingHops Integer32
}

mstInstanceEditIndex OBJECT-TYPE
      SYNTAX      Integer32 (0..4094)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
          "An arbitrary integer within the range from 1 to the value of
          the maximum instance that uniquely identifies a spanning
          tree instance."
      ::= {mstInstanceEditEntry 1 }

mstInstanceEditVlansMap OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN. The
            first octet corresponds to VLANs with vlanIndex values
            of 0 through 7; the second octet to VLANs 8 through
            15; etc., The most significant bit of each octet
            corresponds to the lowest value vlanIndex in that octet.

            For each VLAN, if it is mapped to this MSTP instance,
            then the bit corresponding to that VLAN is set to '1'.

            To create a row, write any of mstInstanceEditVlansMap,
            mstInstanceEditVlansMap2k, mstInstanceEditVlansMap3k or
            mstInstanceEditVlansMap4k, to a non-empty list.
            To destroy a row, write all of these four variables
            to an empty list."
    ::= {mstInstanceEditEntry 2 }

mstInstanceEditVlansMap2k OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN for
            VLANS with vlanIndex values of 1024 through 2047. The
            first octet corresponds to VLANs with vlanIndex values
            of 1024 through 1031; the second octet to VLANs 1032
            through 1039; etc. The most significant bit of each
            octet corresponds to the lowest value vlanIndex in that
            octet.

            For each VLAN, if it is mapped to this MSTP instance,
            then the bit corresponding to that VLAN is set to '1'.

            To create a row, write any of mstInstanceEditVlansMap,
            mstInstanceEditVlansMap2k, mstInstanceEditVlansMap3k or
            mstInstanceEditVlansMap4k, to a non-empty list.
            To destroy a row, write all of these four variables
            to an empty list."
    ::= {mstInstanceEditEntry 3 }

mstInstanceEditVlansMap3k OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN for
            VLANS with vlanIndex values of 2048 through 3071. The
            first octet corresponds to VLANs with vlanIndex values
            of 2048 through 2055; the second octet to VLANs 2056
            through 2063; etc. The most significant bit of each
            octet corresponds to the lowest value vlanIndex in that
            octet.

            For each VLAN, if it is mapped to this MSTP instance,
            then the bit corresponding to that VLAN is set to '1'.

            To create a row, write any of mstInstanceEditVlansMap,
            mstInstanceEditVlansMap2k, mstInstanceEditVlansMap3k or
            mstInstanceEditVlansMap4k, to a non-empty list.
            To destroy a row, write all of these four variables
            to an empty list."
    ::= {mstInstanceEditEntry 4 }

mstInstanceEditVlansMap4k OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN for
            VLANS with vlanIndex values of 3072 through 4095. The
            first octet corresponds to VLANs with vlanIndex values
            of 3072 through 3079; the second octet to VLANs 3080
            through 3087; etc. The most significant bit of each
            octet corresponds to the lowest value vlanIndex in that
            octet.

            For each VLAN, if it is mapped to this MSTP instance,
            then the bit corresponding to that VLAN is set to '1'.

            To create a row, write any of mstInstanceEditVlansMap,
            mstInstanceEditVlansMap2k, mstInstanceEditVlansMap3k or
            mstInstanceEditVlansMap4k, to a non-empty list.
            To destroy a row, write all of these four variables
            to an empty list."
    ::= {mstInstanceEditEntry 5 }

mstInstanceEditRemainingHops OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION "The remaining hop count for this MST instance."
     ::= { mstInstanceEditEntry 6 }

--mstInstanceOperTable
mstInstanceOperTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF MstInstanceOperEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION "The Multiple Spanning Tree region instance vlan mapped table."
     ::= { xstMgt 7 }

mstInstanceOperEntry OBJECT-TYPE
     SYNTAX      MstInstanceOperEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION  "A conceptual row containing the status of the MSTP instance."
     INDEX       { mstInstanceOperIndex }
     ::= { mstInstanceOperTable 1 }

MstInstanceOperEntry ::= SEQUENCE
{
    mstInstanceOperIndex      Integer32,
    mstInstanceOperVlansMap   OCTET STRING,
    mstInstanceOperVlansMap2k OCTET STRING,
    mstInstanceOperVlansMap3k OCTET STRING,
    mstInstanceOperVlansMap4k OCTET STRING
}

mstInstanceOperIndex OBJECT-TYPE
      SYNTAX      Integer32 (0..4094)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
          "An arbitrary integer within the range from 1 to the value of
          the maximum instance that uniquely identifies a spanning
          tree instance."
      ::= {mstInstanceOperEntry 1 }

mstInstanceOperVlansMap OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN. The
            first octet corresponds to VLANs with vlanIndex values
            of 0 through 7; the second octet to VLANs 8 through
            15; etc., The most significant bit of each octet
            corresponds to the lowest value vlanIndex in that octet.

            For each VLAN, if it is mapped to this MSTP instance,
            then the bit corresponding to that VLAN is set to '1'."
    ::= {mstInstanceOperEntry 2 }

mstInstanceOperVlansMap2k OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN for
            VLANS with vlanIndex values of 1024 through 2047. The
            first octet corresponds to VLANs with vlanIndex values
            of 1024 through 1031; the second octet to VLANs 1032
            through 1039; etc. The most significant bit of each
            octet corresponds to the lowest value vlanIndex in that
            octet.

            For each VLAN, if it is mapped to this MSTP instance,
            then the bit corresponding to that VLAN is set to '1'."
    ::= {mstInstanceOperEntry 3 }

mstInstanceOperVlansMap3k OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN for
            VLANS with vlanIndex values of 2048 through 3071. The
            first octet corresponds to VLANs with vlanIndex values
            of 2048 through 2055; the second octet to VLANs 2056
            through 2063; etc. The most significant bit of each
            octet corresponds to the lowest value vlanIndex in that
            octet.

            For each VLAN, if it is mapped to this MSTP instance,
            then the bit corresponding to that VLAN is set to '1'."
    ::= {mstInstanceOperEntry 4 }

mstInstanceOperVlansMap4k OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN for
            VLANS with vlanIndex values of 3072 through 4095. The
            first octet corresponds to VLANs with vlanIndex values
            of 3072 through 3079; the second octet to VLANs 3080
            through 3087; etc. The most significant bit of each
            octet corresponds to the lowest value vlanIndex in that
            octet.

            For each VLAN, if it is mapped to this MSTP instance,
            then the bit corresponding to that VLAN is set to '1'."
    ::= {mstInstanceOperEntry 5 }

-- for 1s(MSTP) end

staLoopbackDetectionPortTable    OBJECT-TYPE
        SYNTAX      SEQUENCE OF StaLoopbackDetectionPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table provides the mechanism to configure the
                     spanning tree loopback detection of each port or trunk"
        ::= { staMgt 8 }

staLoopbackDetectionPortEntry    OBJECT-TYPE
        SYNTAX      StaLoopbackDetectionPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A conceptual row of staLoopbackDetectionPortTable."
        INDEX       { staLoopbackDetectionPortIfIndex}
        ::= { staLoopbackDetectionPortTable  1 }

StaLoopbackDetectionPortEntry    ::= SEQUENCE
{
        staLoopbackDetectionPortIfIndex            InterfaceIndex,
        staLoopbackDetectionPortStatus             EnabledStatus,
        staLoopbackDetectionPortTrapStatus         EnabledStatus,
        staLoopbackDetectionPortReleaseMode        INTEGER,
        staLoopbackDetectionPortRelease            INTEGER
}

staLoopbackDetectionPortIfIndex        OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and the trunk interfaces of the portTable. The interface
                     identified by a particular value of this index is the same interface
                     as identified by the same value of ifIndex in the IF-MIB."
        ::= { staLoopbackDetectionPortEntry  1 }

staLoopbackDetectionPortStatus    OBJECT-TYPE
        SYNTAX     EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Status of the port on whether spanning tree loopback detection is enabled."
        ::= { staLoopbackDetectionPortEntry  2 }

staLoopbackDetectionPortTrapStatus    OBJECT-TYPE
        SYNTAX     EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The parameter indicates whether the trap has
                     to be sent when the loopback BPDUs have been detected."
        ::= { staLoopbackDetectionPortEntry  3 }

 staLoopbackDetectionPortReleaseMode   OBJECT-TYPE
        SYNTAX     INTEGER
        {
            auto(1),
            manual(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting it to auto(1) indicates that this port can be released
                     from discarding state automatically after loopback has occurred.
                     Setting it to manual(2) indicates that this port can be released
                     from discarding state manually after loopback has occurred."
        ::= { staLoopbackDetectionPortEntry  4 }

staLoopbackDetectionPortRelease    OBJECT-TYPE
        SYNTAX     INTEGER
        {
            noRelease(1),
            release(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Set this to release(2) to release the port from discarding state.
                     noRelease(1) will always be obtained when reading this variable."
        ::= { staLoopbackDetectionPortEntry  5 }

--
-- restartMgt
--

-- Management for restarting the switch.


restartOpCodeFile OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..127))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Name of op-code file for start-up."
        ::= { restartMgt 1 }

restartConfigFile OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..127))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Name of configuration file for start-up."
        ::= { restartMgt 2 }

restartControl  OBJECT-TYPE
    SYNTAX     INTEGER {
                    running(1),
                    warmBoot(2),
                    coldBoot(3)
              }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "Setting this object to warmBoot(2) causes the device to
         reinitialize itself such that neither the agent configuration
         nor the protocol entity implementation is altered. Setting this
         object to coldBoot(3) causes the device to reinitialize itself such
         that the agent's configuration or the protocol entity implementation
         may be altered. When the device is running normally, this
         variable has a value of running(1)."
    ::= { restartMgt 3 }

--
-- mirrorMgt
--

-- Management for port mirroring.

mirrorTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF MirrorEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for port mirroring, enabling a port to be mirrored
                     to/from another port. Not all ports can be mirrored and
                     limitations may apply as to which ports can be used as either
                     source or destination ports."
        ::= { mirrorMgt 1 }

mirrorEntry OBJECT-TYPE
        SYNTAX      MirrorEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual row of mirrorTable."
        INDEX       { mirrorDestinationPort, mirrorSourcePort }
        ::= { mirrorTable 1 }

MirrorEntry ::= SEQUENCE
{
    mirrorDestinationPort  Integer32,
    mirrorSourcePort       Integer32,
    mirrorType             INTEGER,
    mirrorStatus           ValidStatus
}

mirrorDestinationPort OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The destination port interface for mirrored packets.
                     The interface identified by a particular value of
                     this index is the same interface as identified by
                     the same value of ifIndex in the IF-MIB."
        ::= { mirrorEntry 1 }

mirrorSourcePort OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The source port interface for mirrored packets.
                     The interface identified by a particular value of
                     this index is the same interface as identified by
                     the same value of ifIndex in the IF-MIB."
        ::= { mirrorEntry 2 }

mirrorType OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        rx(1),
                        tx(2),
                        both(3)
                    }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "If this value is rx(1), receive packets will
                    be mirrored. If this value is tx(2), transmit
                    packets will be mirrored. If this value is both(3),
                    both receive and transmit packets will be mirrored."
        ::= { mirrorEntry 3 }

mirrorStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Setting this to valid(1) creates an entry.
                     Setting this to invalid(2) destroys an entry."
        ::= { mirrorEntry 4 }

vlanMirrorTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF VlanMirrorEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for VLAN mirroring, enabling a VLAN to be mirrored
                     to a port."
        ::= { mirrorMgt 2 }

vlanMirrorEntry OBJECT-TYPE
        SYNTAX      VlanMirrorEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual row of vlanMirrorTable."
        INDEX       { vlanMirrorDestinationPort, vlanMirrorSourceVlan }
        ::= { vlanMirrorTable 1 }

VlanMirrorEntry ::= SEQUENCE
{
    vlanMirrorDestinationPort  Integer32,
    vlanMirrorSourceVlan       Integer32,
    vlanMirrorStatus           ValidStatus
}

vlanMirrorDestinationPort OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The destination port interface for mirrored packets.
                     The interface identified by a particular value of
                     this index is the same interface as identified by
                     the same value of ifIndex in the IF-MIB."
        ::= { vlanMirrorEntry 1 }

vlanMirrorSourceVlan OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The source VLAN for mirrored packets. The interface
                     identified by a particular value of this index is the same
                     interface as identified by the same value of dot1qVlanIndex
                     in the Q-BRIDGE-MIB."
        ::= { vlanMirrorEntry 2 }

vlanMirrorStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Set this to valid(1) to create an entry. Set this to
                     invalid(2) to destroy an entry."
        ::= { vlanMirrorEntry 4 }

macMirrorTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF MacMirrorEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for MAC mirroring, enabling a MAC address to be
                     mirrored to a port."
        ::= { mirrorMgt 4 }

macMirrorEntry OBJECT-TYPE
        SYNTAX      MacMirrorEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual row of mirrorMacTable."
        INDEX       { macMirrorDestinationPort, macMirrorSourceMacAddr }
        ::= { macMirrorTable 1 }

MacMirrorEntry ::= SEQUENCE
{
    macMirrorDestinationPort  Integer32,
    macMirrorSourceMacAddr    MacAddress,
    macMirrorStatus           ValidStatus
}

macMirrorDestinationPort OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The destination port interface for mirrored packets.
                     The interface identified by a particular value of
                     this index is the same interface as identified by
                     the same value of ifIndex in the IF-MIB."
        ::= { macMirrorEntry 1 }

macMirrorSourceMacAddr OBJECT-TYPE
        SYNTAX      MacAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Packets with matching source MAC address will be
                     monitored."
        ::= { macMirrorEntry 2 }

macMirrorStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Setting this to valid(1) creates an entry.
                     Setting this to invalid(2) destroys an entry."
        ::= { macMirrorEntry 3 }

--
-- igmpSnoopMgt
--

-- Management for Internet Group Management Protocol (IGMP)
-- Snooping.


igmpSnoopStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Parameter to enable or disable IGMP snooping on the device.
                     When enabled, the device will examine IGMP packets and set
                     up filters for IGMP ports. "
        DEFVAL      { enabled }
        ::= { igmpSnoopMgt 1 }

igmpSnoopQuerier OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Enables (disables) whether the switch acts as an IGMP
                     querier."
        DEFVAL      { enabled }
        ::= { igmpSnoopMgt 2 }

igmpSnoopRouterPortExpireTime OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Sets the time (in seconds) the switch waits after
                     the previous querier has stopped querying before
                     the router port (which received query packets from
                     previous querier) expires."
        DEFVAL      { 300 }
        ::= { igmpSnoopMgt 6 }

igmpSnoopVersion OBJECT-TYPE
        SYNTAX      Integer32 (1..3)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "IGMP version snooped"
        DEFVAL      { 2 }
        ::= { igmpSnoopMgt 7 }

igmpSnoopRouterCurrentTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF IgmpSnoopRouterCurrentEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for current router ports."
    ::= { igmpSnoopMgt 8 }

igmpSnoopRouterCurrentEntry OBJECT-TYPE
    SYNTAX      IgmpSnoopRouterCurrentEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for current router ports."
    INDEX   { igmpSnoopRouterCurrentVlanIndex }
    ::= {
igmpSnoopRouterCurrentTable 1 }

IgmpSnoopRouterCurrentEntry ::=
    SEQUENCE {
        igmpSnoopRouterCurrentVlanIndex
            Unsigned32,
        igmpSnoopRouterCurrentPorts
            PortList,
        igmpSnoopRouterCurrentStatus
            PortList
    }

igmpSnoopRouterCurrentVlanIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The interface identified by a particular value of
         this index is the same interface as identified by
         the same value of dot1qVlanIndex in the Q-BRIDGE-MIB.
         The entry will only appear here after a configure to
         igmpSnoopRouterStaticTable."
    ::= { igmpSnoopRouterCurrentEntry 1 }

igmpSnoopRouterCurrentPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The set of ports which are current router ports, including static
                 router ports. Please refer to igmpSnoopRouterStaticTable."
    ::= { igmpSnoopRouterCurrentEntry 2 }

igmpSnoopRouterCurrentStatus OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The set of ports which are static router ports."
    ::= { igmpSnoopRouterCurrentEntry 3 }

igmpSnoopRouterStaticTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF IgmpSnoopRouterStaticEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for static router ports."
    ::= { igmpSnoopMgt 9 }

igmpSnoopRouterStaticEntry OBJECT-TYPE
    SYNTAX      IgmpSnoopRouterStaticEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for static router ports."
    INDEX   { igmpSnoopRouterStaticVlanIndex }
    ::= {
igmpSnoopRouterStaticTable 1 }

IgmpSnoopRouterStaticEntry ::=
    SEQUENCE {
        igmpSnoopRouterStaticVlanIndex
            Unsigned32,
        igmpSnoopRouterStaticPorts
            PortList,
        igmpSnoopRouterStaticStatus
            ValidStatus
    }

igmpSnoopRouterStaticVlanIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The interface identified by a particular value of
         this index is the same interface as identified by
         the same value of dot1qVlanIndex in the Q-BRIDGE-MIB.
         The entry will only appear here after a configure to
         igmpSnoopRouterStaticTable."
    ::= { igmpSnoopRouterStaticEntry 1 }

igmpSnoopRouterStaticPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The set of ports which are static router ports."
    ::= { igmpSnoopRouterStaticEntry 2 }

igmpSnoopRouterStaticStatus OBJECT-TYPE
    SYNTAX      ValidStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Setting this to valid(1) creates an entry.
         Setting this to invalid(2) destroys an entry."
    ::= { igmpSnoopRouterStaticEntry 3 }

igmpSnoopMulticastCurrentTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF IgmpSnoopMulticastCurrentEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for current multicast addresses."
    ::= { igmpSnoopMgt 10 }

igmpSnoopMulticastCurrentEntry OBJECT-TYPE
    SYNTAX      IgmpSnoopMulticastCurrentEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for current multicast addresses."
    INDEX   { igmpSnoopMulticastCurrentVlanIndex,
              igmpSnoopMulticastCurrentIpAddress }
    ::= {
igmpSnoopMulticastCurrentTable 1 }

IgmpSnoopMulticastCurrentEntry ::=
    SEQUENCE {
        igmpSnoopMulticastCurrentVlanIndex
            Unsigned32,
        igmpSnoopMulticastCurrentIpAddress
            IpAddress,
        igmpSnoopMulticastCurrentPorts
            PortList,
        igmpSnoopMulticastCurrentStatus
            PortList
    }

igmpSnoopMulticastCurrentVlanIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The interface identified by a particular value of
         this index is the same interface as identified by
         the same value of dot1qVlanIndex in the Q-BRIDGE-MIB.
         The entry will only appear here after a configure to
         igmpSnoopMulticastStaticTable."
    ::= { igmpSnoopMulticastCurrentEntry 1 }

igmpSnoopMulticastCurrentIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IP address of multicast group."
    ::= { igmpSnoopMulticastCurrentEntry 2 }

igmpSnoopMulticastCurrentPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The set of ports which are members of a multicast group, including
         static members. Please refer to igmpSnoopMulticastStaticTable."
    ::= { igmpSnoopMulticastCurrentEntry 3 }

igmpSnoopMulticastCurrentStatus OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The set of ports which are static members."
    ::= { igmpSnoopMulticastCurrentEntry 4 }

igmpSnoopMulticastStaticTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF IgmpSnoopMulticastStaticEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for static multicast addresses."
    ::= { igmpSnoopMgt 11 }

igmpSnoopMulticastStaticEntry OBJECT-TYPE
    SYNTAX      IgmpSnoopMulticastStaticEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for static multicast addresses."
    INDEX   { igmpSnoopMulticastStaticVlanIndex,
              igmpSnoopMulticastStaticIpAddress }
    ::= {
igmpSnoopMulticastStaticTable 1 }

IgmpSnoopMulticastStaticEntry ::=
    SEQUENCE {
        igmpSnoopMulticastStaticVlanIndex
            Unsigned32,
        igmpSnoopMulticastStaticIpAddress
            IpAddress,
        igmpSnoopMulticastStaticPorts
            PortList,
        igmpSnoopMulticastStaticStatus
            ValidStatus
    }

igmpSnoopMulticastStaticVlanIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The interface identified by a particular value of
         this index is the same interface as identified by
         the same value of dot1qVlanIndex in the Q-BRIDGE-MIB.
         The entry will only appear here after a configure to
         igmpSnoopMulticastStaticTable."
    ::= { igmpSnoopMulticastStaticEntry 1 }

igmpSnoopMulticastStaticIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IP address of multicast group."
    ::= { igmpSnoopMulticastStaticEntry 2 }

igmpSnoopMulticastStaticPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The set of ports which are members."
    ::= { igmpSnoopMulticastStaticEntry 3 }

igmpSnoopMulticastStaticStatus OBJECT-TYPE
    SYNTAX      ValidStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Setting this to valid(1) creates an entry.
         Setting this to invalid(2) destroys an entry."
    ::= { igmpSnoopMulticastStaticEntry 4 }

igmpSnoopCurrentVlanTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IgmpSnoopCurrentVlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for enabling or disabling IGMP snooping per VLAN."
        ::= { igmpSnoopMgt 14 }

igmpSnoopCurrentVlanEntry OBJECT-TYPE
        SYNTAX      IgmpSnoopCurrentVlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for enabling or disabling IGMP snooping."
        INDEX       { igmpSnoopCurrentVlanIndex }
        ::= { igmpSnoopCurrentVlanTable 1 }

IgmpSnoopCurrentVlanEntry ::= SEQUENCE
{
    igmpSnoopCurrentVlanIndex                   Unsigned32,
    igmpSnoopCurrentVlanStatus                  EnabledStatus,
    igmpSnoopCurrentVlanImmediateLeave          EnabledStatus,
    igmpSnoopCurrentVlanGeneralQuerySuppression EnabledStatus,
    igmpSnoopCurrentVlanLastMemQueryCount       Unsigned32,
    igmpSnoopCurrentVlanLastMemQueryIntvl       Unsigned32,
    igmpSnoopCurrentVlanProxyAddress            IpAddress,
    igmpSnoopCurrentVlanQueryIntvl              Unsigned32,
    igmpSnoopCurrentVlanQueryRespIntvl          Unsigned32,
    igmpSnoopCurrentVlanProxyReporting          INTEGER,
    igmpSnoopCurrentVlanVersion                 Unsigned32,
    igmpSnoopCurrentVlanVersionExclusive        EnabledStatus
}

igmpSnoopCurrentVlanIndex OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Same is dot1qVlanIndex in the Q-BRIDGE-MIB.
            This table has only one entry - the entry for
            the VLAN of the management interface."
        ::= { igmpSnoopCurrentVlanEntry 1 }

igmpSnoopCurrentVlanStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Parameter to enable or disable IGMP snooping on this VLAN.
                     When enabled, the device will examine IGMP packets and set
                     up filters for IGMP ports."
        ::= { igmpSnoopCurrentVlanEntry 2 }

igmpSnoopCurrentVlanImmediateLeave OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The parameter to enable or disable the Immediate-Leave feature on this VLAN."
        ::= { igmpSnoopCurrentVlanEntry 3 }

igmpSnoopCurrentVlanGeneralQuerySuppression OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The parameter to enable or disable the general query suppresion
                     on this VLAN."
        ::= { igmpSnoopCurrentVlanEntry 4 }

igmpSnoopCurrentVlanLastMemQueryCount OBJECT-TYPE
        SYNTAX      Unsigned32(1..255)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Represents the number of queries sent by the switch before
                     it assumes there are no local members."
        ::= { igmpSnoopCurrentVlanEntry 5 }

igmpSnoopCurrentVlanLastMemQueryIntvl OBJECT-TYPE
        SYNTAX      Unsigned32(1..31744)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The last member query interval is the max response time
                     inserted into group-specific queries sent in response to
                     leave group messages,and is also the the max response time
                     inserted into group-and-source-specific query messages."
        ::= { igmpSnoopCurrentVlanEntry 6 }

igmpSnoopCurrentVlanProxyAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Represents the address of queries sent by the switch."
        ::= { igmpSnoopCurrentVlanEntry 7 }

igmpSnoopCurrentVlanQueryIntvl OBJECT-TYPE
        SYNTAX      Unsigned32(2..31744)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Represents the query interval of queries sent by the switch."
        ::= { igmpSnoopCurrentVlanEntry 8 }

igmpSnoopCurrentVlanQueryRespIntvl OBJECT-TYPE
        SYNTAX      Unsigned32(10..31740)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Represents the query response interval of queries
                     sent by the switch."
        ::= { igmpSnoopCurrentVlanEntry 9 }

igmpSnoopCurrentVlanProxyReporting OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        enabled(1),
                        disabled(2),
                        default(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Set this variable to enabled(1) to enable the feature.
                     Set this variable to disabled(2) to disable the feature.
                     Set this variable to default(3), the status of the feature
                     is decided by the global configuration."
        ::= { igmpSnoopCurrentVlanEntry 10 }

igmpSnoopCurrentVlanVersion OBJECT-TYPE
        SYNTAX      Unsigned32(1..3)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "the version of igmp packets is supported by this vlan."
        ::= { igmpSnoopCurrentVlanEntry 11 }

igmpSnoopCurrentVlanVersionExclusive OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Enable/disable control of the IGMP Snooping exclusive
                     supported version."
        ::= { igmpSnoopCurrentVlanEntry 12 }

igmpSnoopMulticastGroupTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF IgmpSnoopMulticastGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for current multicast addresses."
    ::= { igmpSnoopMgt 15 }

igmpSnoopMulticastGroupEntry OBJECT-TYPE
    SYNTAX      IgmpSnoopMulticastGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for Group multicast addresses."
    INDEX   { igmpSnoopMulticastGroupVlanIndex,
              igmpSnoopMulticastGroupIpAddress,
              igmpSnoopMulticastGroupSourceIPAddress }
    ::= { igmpSnoopMulticastGroupTable 1 }

IgmpSnoopMulticastGroupEntry ::=
    SEQUENCE {
        igmpSnoopMulticastGroupVlanIndex
            Unsigned32,
        igmpSnoopMulticastGroupIpAddress
            IpAddress,
        igmpSnoopMulticastGroupSourceIPAddress
            IpAddress,
        igmpSnoopMulticastGroupPorts
            PortList,
        igmpSnoopMulticastGroupStatus
            PortList
    }

igmpSnoopMulticastGroupVlanIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The interface identified by a particular value of
         this index is the same interface as identified by
         the same value of dot1qVlanIndex in the Q-BRIDGE-MIB.
         The entry will only appear here after a configure to
         igmpSnoopMulticastStaticTable."
    ::= { igmpSnoopMulticastGroupEntry 1 }

igmpSnoopMulticastGroupIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IP address of multicast group."
    ::= { igmpSnoopMulticastGroupEntry 2 }

igmpSnoopMulticastGroupSourceIPAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Source IP address of source."
    ::= { igmpSnoopMulticastGroupEntry 3 }

igmpSnoopMulticastGroupPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The set of ports which are members of a multicast group, including
         static members. Please refer to igmpSnoopMulticastStaticTable."
    ::= { igmpSnoopMulticastGroupEntry 4 }

igmpSnoopMulticastGroupStatus OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The set of ports which are static IGMP member ports."
    ::= { igmpSnoopMulticastGroupEntry 5 }

igmpSnoopFilterStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Parameter to enable or disable IGMP filtering on the device."
    ::= { igmpSnoopMgt 17 }

igmpSnoopProfileTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IgmpSnoopProfileEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The table for configuring the IGMP snooping profile."
        ::= { igmpSnoopMgt 18 }

igmpSnoopProfileEntry OBJECT-TYPE
        SYNTAX      IgmpSnoopProfileEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The entry for configuring the IGMP snooping profile."
        INDEX       { igmpSnoopProfileId }
        ::= { igmpSnoopProfileTable 1 }

IgmpSnoopProfileEntry ::= SEQUENCE
{
    igmpSnoopProfileId               Unsigned32,
    igmpSnoopProfileAction           INTEGER,
    igmpSnoopProfileStatus           ValidStatus
}

igmpSnoopProfileId OBJECT-TYPE
        SYNTAX      Unsigned32 (1..4294967295)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The ID of the IGMP snooping profile."
        ::= { igmpSnoopProfileEntry 1 }

igmpSnoopProfileAction OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    permit(1),
                    deny(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The access mode of the IGMP snooping profile."
    DEFVAL      { deny }
    ::= { igmpSnoopProfileEntry 2 }

igmpSnoopProfileStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting this to valid(1) creates an entry.
                     Setting this to invalid(2) destroys an entry."
        ::= { igmpSnoopProfileEntry 3 }

igmpSnoopProfileCtl      OBJECT IDENTIFIER   ::= { igmpSnoopMgt 19 }

igmpSnoopProfileCtlId   OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The ID of the IGMP snooping profile. The default value
                     is zero, meaning that no ID is specified. In order to
                     create a profile, the range of values which may
                     correspond to an entry in the igmpSnoopProfileTable is
                     determined by the igmpSnoopProfileId object."
        ::= { igmpSnoopProfileCtl 1 }

igmpSnoopProfileCtlInetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The address type is associated with this agent.
                 Only ipv4(1) type is supported."
    ::= { igmpSnoopProfileCtl 2 }

igmpSnoopProfileCtlStartInetAddress OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The specified addresses in the start of the controlled
                     IP multicast addresses."
        ::= { igmpSnoopProfileCtl 3 }

igmpSnoopProfileCtlEndInetAddress OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The specified addresses in the end of the controlled
                     IP multicast addresses."
        ::= { igmpSnoopProfileCtl 4 }

igmpSnoopProfileCtlAction OBJECT-TYPE
        SYNTAX      INTEGER
        {
            noAction(1),
            create(2),
            destroy(3)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting it to create(2) creates the range of the
                     controlled IP multicast addresses.
                     Setting it to destroy(3) destroys the range of the
                     controlled IP multicast addresses.
                     When the action is completed, this object becomes
                     noAction(1)."
        ::= { igmpSnoopProfileCtl 5 }

igmpSnoopProfileRangeTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IgmpSnoopProfileRangeEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The table for configuring the range of the IGMP snooping
                     profile."
        ::= { igmpSnoopMgt 20 }

igmpSnoopProfileRangeEntry OBJECT-TYPE
        SYNTAX      IgmpSnoopProfileRangeEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The entry for configuring the range of the IGMP snooping
                     profile."
        INDEX       { igmpSnoopProfileRangeProfileId,
                      igmpSnoopProfileRangeInetAddressType,
                      igmpSnoopProfileRangeStartInetAddress }
        ::= { igmpSnoopProfileRangeTable 1 }

IgmpSnoopProfileRangeEntry ::= SEQUENCE
{
    igmpSnoopProfileRangeProfileId           Unsigned32,
    igmpSnoopProfileRangeInetAddressType     InetAddressType,
    igmpSnoopProfileRangeStartInetAddress    InetAddress,
    igmpSnoopProfileRangeEndInetAddress      InetAddress,
    igmpSnoopProfileRangeAction              INTEGER
}

igmpSnoopProfileRangeProfileId OBJECT-TYPE
        SYNTAX      Unsigned32 (1..4294967295)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This is defined as igmpSnoopProfileId."
        ::= { igmpSnoopProfileRangeEntry 1 }

igmpSnoopProfileRangeInetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "The address type is associated with this agent.
        Only ipv4(1) type is supported."
    ::= { igmpSnoopProfileRangeEntry 2 }

igmpSnoopProfileRangeStartInetAddress OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The specified addresses in the start of the controlled
                     IP multicast addresses."
        ::= { igmpSnoopProfileRangeEntry 3 }

igmpSnoopProfileRangeEndInetAddress OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The specified addresses in the end of the controlled
                     IP multicast addresses."
        ::= { igmpSnoopProfileRangeEntry 4 }

igmpSnoopProfileRangeAction OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    permit(1),
                    deny(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The access mode of the IGMP snooping profile."
    DEFVAL      { deny }
    ::= { igmpSnoopProfileRangeEntry 5 }

igmpSnoopFilterPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IgmpSnoopFilterPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for port configuration in IGMP filtering."
        ::= { igmpSnoopMgt 21 }

igmpSnoopFilterPortEntry OBJECT-TYPE
        SYNTAX      IgmpSnoopFilterPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for port configuration in IGMP filtering."
        INDEX       { igmpSnoopFilterPortIndex }
        ::= { igmpSnoopFilterPortTable 1 }

IgmpSnoopFilterPortEntry ::= SEQUENCE
{
    igmpSnoopFilterPortIndex              Unsigned32,
    igmpSnoopFilterPortProfileId          Integer32
}

igmpSnoopFilterPortIndex OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and trunk (including trunk members) interface of
                     the portTable. The interface identified by a particular
                     value of this index is the same interface identified by
                     the same value of ifIndex in the IF-MIB."
        ::= { igmpSnoopFilterPortEntry 1 }

igmpSnoopFilterPortProfileId OBJECT-TYPE
        SYNTAX     Integer32
        MAX-ACCESS read-write
        STATUS     current
        DESCRIPTION
            "The igmpSnoopProfileEntry identified by a particular value of
             this index is the same profile identified by the same value of
             the igmpSnoopProfileId object. If there is no corresponding entry
             in the igmpSnoopProfileTable, then no association exists.
             In particular, if this value is zero, no associated profile
             will be generated, as zero is not a valid profile index."
        ::= { igmpSnoopFilterPortEntry 2 }

igmpSnoopThrottlePortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF IgmpSnoopThrottlePortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for port configuration in IGMP throttling."
        ::= { igmpSnoopMgt 22 }

igmpSnoopThrottlePortEntry OBJECT-TYPE
        SYNTAX      IgmpSnoopThrottlePortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for port configuration in IGMP throttling."
        INDEX       { igmpSnoopThrottlePortIndex }
        ::= { igmpSnoopThrottlePortTable 1 }

IgmpSnoopThrottlePortEntry ::= SEQUENCE
{
    igmpSnoopThrottlePortIndex            Unsigned32,
    igmpSnoopThrottlePortRunningStatus    INTEGER,
    igmpSnoopThrottlePortAction           INTEGER,
    igmpSnoopThrottlePortMaxGroups        Integer32,
    igmpSnoopThrottlePortCurrentGroups    Integer32
}

igmpSnoopThrottlePortIndex OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and trunk (including trunk members) interface of
                     the portTable. The interface identified by a particular
                     value of this index is the same interface identified by
                     the same value of ifIndex in the IF-MIB."
        ::= { igmpSnoopThrottlePortEntry 1 }

igmpSnoopThrottlePortRunningStatus OBJECT-TYPE
        SYNTAX  TruthValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Describes the running status of the IGMP throttling to
                     the switch. A value of true(1) indicates the IGMP
                     throttling mechanism is active. A value of false(2)
                     indicates the IGMP throttling mechanism is inactive."
        ::= { igmpSnoopThrottlePortEntry 2 }

igmpSnoopThrottlePortAction OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    replace(1),
                    deny(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The action mode of the IGMP throttling. A value of replace(1)
                 means to replace a joined multicast group randomly when
                 an interface receives an IGMP report and the number of
                 current joined multicast groups is equal to the maximum number
                 of IGMP groups that the interface can join.
                 A value of deny(2) means to deny the IGMP report request when
                 an interface receives an IGMP report and the number of current
                 joined multicast groups is equal to the maximum number of
                 IGMP groups that the interface can join."
    DEFVAL      { deny }
    ::= { igmpSnoopThrottlePortEntry 3 }

igmpSnoopThrottlePortMaxGroups OBJECT-TYPE
        SYNTAX      Integer32(0..256)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The maximum number of IGMP groups that the interface can
                     join."
        ::= { igmpSnoopThrottlePortEntry 4 }

igmpSnoopThrottlePortCurrentGroups OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The current number of IGMP groups that the interface has
                     joined."
        ::= { igmpSnoopThrottlePortEntry 5 }

--
-- igmpSnoopGlobalMgt
--

-- Global Management for Internet Group Management Protocol (IGMP)
-- Snooping.

igmpSnoopGlobalMgt        OBJECT IDENTIFIER ::= { igmpSnoopMgt 28 }

igmpSnoopProxyReporting OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Parameter to enable or disable IGMP snooping proxy
                     reporting on the device."
        DEFVAL      { enabled }
        ::= { igmpSnoopGlobalMgt 1 }

igmpSnoopRouterAlertOptionCheck OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Parameter to enable or disable IGMP snooping router alert
                    option check on the device."
        DEFVAL      { disabled }
        ::= { igmpSnoopGlobalMgt 2 }

igmpSnoopTcnFlood OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Parameter to enable or disable IGMP snooping tcn flood
                    on the device."
        DEFVAL      { disabled }
        ::= { igmpSnoopGlobalMgt 3 }

igmpSnoopTcnQuerySolicit OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Parameter to enable or disable IGMP snooping tcn query
                    solicit on the device."
        DEFVAL      { disabled }
        ::= { igmpSnoopGlobalMgt 4 }

igmpSnoopUnregisteredDataFlood OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Parameter to enable or disable IGMP snooping Unregistered
                    data flood solicit on the device."
        DEFVAL      { disabled }
        ::= { igmpSnoopGlobalMgt 5 }

igmpSnoopUnsolicitedReportInterval OBJECT-TYPE
        SYNTAX      Unsigned32(1..65535)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting this value to specify how long (in seconds) the
                     uplink ports should transmit unsolicited reports."
        DEFVAL      { 400 }
        ::= { igmpSnoopGlobalMgt 6 }

igmpSnoopVersionExclusive OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Parameter to enable or disable IGMP snooping version
                     exclusive on the device."
        DEFVAL      { disabled }
        ::= { igmpSnoopGlobalMgt 7 }

--
-- The IpMgt Group
--

-- Management for Internet Protocol (IP).

netConfigTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF NetConfigEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of netConfigEntry."
    ::= { ipMgt 1 }

netConfigEntry  OBJECT-TYPE
    SYNTAX     NetConfigEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A set of configuration parameters for a particular
        network interface on this device. If the device has no network
        interface, this table is empty.

        The index is composed of the ifIndex assigned to the
        corresponding interface."
    INDEX  { netConfigIfIndex, netConfigIPAddress, netConfigSubnetMask }
    ::= { netConfigTable 1 }

NetConfigEntry ::= SEQUENCE {
    netConfigIfIndex           Integer32,
    netConfigIPAddress         IpAddress,
    netConfigSubnetMask        IpAddress,
    netConfigPrimaryInterface  INTEGER,
    netConfigUnnumbered        INTEGER,
    netConfigStatus            RowStatus
}

netConfigIfIndex  OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION "The VLAN interface being used by this table entry. Only the
                 VLAN interfaces which have an IP configured will appear in
                 the table."
    ::= { netConfigEntry 1 }

netConfigIPAddress  OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The IP address of this Net interface.  The default value
        for this object is 0.0.0.0.  If either the netConfigIPAddress
        or netConfigSubnetMask is 0.0.0.0, then when the device
        boots, it may use BOOTP to try to figure out what these
        values should be. If BOOTP fails, before the device
        can talk on the network, this value must be configured
        (e.g., through a terminal attached to the device)."
    ::= { netConfigEntry 2 }

netConfigSubnetMask  OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The subnet mask of this Net interface.  The default value
        for this object is 0.0.0.0.  If either the netConfigIPAddress
        or netConfigSubnetMask are 0.0.0.0, then when the device
        boots, it may use BOOTP to try to figure out what these
        values should be. If BOOTP fails, before the device
        can talk on the network, this value must be configured
        (e.g., through a terminal attached to the device)."
    ::= { netConfigEntry 3 }

netConfigPrimaryInterface OBJECT-TYPE
    SYNTAX     INTEGER
               {
                   primary(1),
                   secondary(2)
               }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "Whether this is a primary interface."
    ::= { netConfigEntry 4 }

netConfigUnnumbered OBJECT-TYPE
    SYNTAX     INTEGER
               {
                   unnumbered(1),
                   notUnnumbered(2)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Whether this is an unnumbered interface."
    ::= { netConfigEntry 5 }

netConfigStatus  OBJECT-TYPE
    SYNTAX     RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
			"The status of this conceptual row entry.
            This object is used to manage the
			creation and deletion of conceptual rows.

			The status column has six defined values:

			     - 'active', which indicates that the conceptual row is
			     available for use by the managed device;

			     - 'notInService', which indicates that the conceptual
			     row exists in the agent, but is unavailable for use by
			     the managed device (see NOTE below);

			     - 'notReady', which indicates that the conceptual row
			     exists in the agent, but is missing information
			     necessary in order to be available for use by the
			     managed device;

			     - 'createAndGo', which is supplied by a management
			     station wishing to create a new instance of a
			     conceptual row and to have its status automatically set
			     to active, making it available for use by the managed
			     device;

			     - 'createAndWait', which is supplied by a management
			     station wishing to create a new instance of a
			     conceptual row (but not make it available for use by
			     the managed device); and,

			     - 'destroy', which is supplied by a management station
			     wishing to delete all of the instances associated with
			     an existing conceptual row.

			Whereas five of the six values (all except 'notReady') may
			be specified in a management protocol set operation, only
			three values will be returned in response to a management
			protocol retrieval operation: 'notReady', 'notInService' or
			'active'. That is, when queried, an existing conceptual row
			has only three states:  it is either available for use by
			the managed device (the status column has value 'active');
			it is not available for use by the managed device, though
			the agent has sufficient information to make it so (the
			status column has value 'notInService'); or, it is not
			available for use by the managed device, and an attempt to
			make it so would fail because the agent has insufficient
			information (the state column has value 'notReady').

            For a detailed description of this object, please refer to
            SNMPv2-TC MIB."
    ::= { netConfigEntry 6 }

netDefaultGateway  OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The IP Address of the default gateway.  If this value is
        undefined or unknown, it shall have the value 0.0.0.0."
    ::= { ipMgt 2 }

ipHttpState OBJECT-TYPE
    SYNTAX     EnabledStatus
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Whether HTTP is enabled."
    ::= { ipMgt 3 }

ipHttpPort OBJECT-TYPE
   SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The port number for HTTP."
    ::= { ipMgt 4 }

ipDhcpRestart OBJECT-TYPE
    SYNTAX     INTEGER
               {
                   restart(1),
                   noRestart(2)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "When set to restart(1) the DHCP server will restart. When read,
                 this value always returns noRestart(2)."
    ::= { ipMgt 5 }

-- optional
ipHttpsState OBJECT-TYPE
    SYNTAX     EnabledStatus
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Whether HTTPS is enabled."
    ::= { ipMgt 6 }

ipHttpsPort OBJECT-TYPE
    SYNTAX     Integer32 (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The port number for HTTPS."
    ::= { ipMgt 7 }

dhcpMgt              OBJECT IDENTIFIER ::= { ipMgt 11 }
dhcpClient           OBJECT IDENTIFIER ::= { dhcpMgt 1 }
dhcpcOptions         OBJECT IDENTIFIER ::= { dhcpClient 1 }

dhcpcInterfaceTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DhcpcInterfaceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for DHCP client information listed by interface.
                     Depending on the nature of the product, this table may
                     have only one entry (e.g. for the management VLAN), or
                     may have many entries (e.g. for all ports, or for all
                     static VLANs)."
        ::= { dhcpcOptions 1 }

dhcpcInterfaceEntry OBJECT-TYPE
        SYNTAX      DhcpcInterfaceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for DHCP client information listed by interface."
        INDEX       { dhcpcIfIndex }
        ::= { dhcpcInterfaceTable 1 }

DhcpcInterfaceEntry ::= SEQUENCE
{
   dhcpcIfIndex             Integer32,
   dhcpcIfVendorClassIdMode INTEGER,
   dhcpcIfVendorClassId     OCTET STRING
}

dhcpcIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This is defined by ifIndex in the IF-MIB
                     (static vlan if index)."
        ::= { dhcpcInterfaceEntry 1 }

dhcpcIfVendorClassIdMode OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                      notSpecified(1),
                      text(2),
                      hex(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Whether the vendor class ID is in text mode or in
                     hex mode."
        ::= { dhcpcInterfaceEntry 4 }

dhcpcIfVendorClassId OBJECT-TYPE
         SYNTAX      OCTET STRING (SIZE(1..32))
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION "The value that the DHCP client sets in the
                      vendor-class-identifier option of
                      DHCPDISCOVER and DHCPREQUEST messages.
                      This value may be used by DHCP servers to identify
                      the vendor class of the client."
         ::= { dhcpcInterfaceEntry 5 }

--
--pingMgt
--

pingMgt              OBJECT IDENTIFIER ::= { ipMgt 15 }

pingIpAddress OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "Specifies the IP address of the device that is planned
                 to ping."
    ::= { pingMgt 1 }

pingPacketSize OBJECT-TYPE
    SYNTAX     Integer32 (32..512)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "Specifies the size of each data potion of ping packets
                 in bytes."
    DEFVAL { 32 }
    ::= { pingMgt 2 }

pingCompleted OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION "A value of true(1) will be read when this ping operation has
                 been either responded to or changed to the time-out status.
                 A value of false(2) will be read when there is a ping
                 operation running and all associated objects in the pingMgt
                 operation cannot be modified during this period."
    ::= { pingMgt 4 }

pingAction OBJECT-TYPE
    SYNTAX      INTEGER
                {
                   noAction(1),
                   pingStart(2)
                }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The action of the pingMgt operation. Sets these objects to
                 pingStart(2) to begin the ping operation. Once the action
                 is set to pingStart(2), the associated pingMgt objects cannot
                 be modified until this ping operation is completed
                 (pingCompleted is true). When the ping has ended or there is
                 no ping operation performing, this object will get a value of
                 noAction(1)."
    ::= { pingMgt 5 }

-- ASV3518KO-FLF-02, 2007-01, for CHT
--
pingProbeCount OBJECT-TYPE
    SYNTAX      INTEGER (1..15)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the number of times to perform a ping operation at a
                 remote host."
    ::= { pingMgt 6 }

-- For CHT

pingSentPackets OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The value of this object reflects the number of probes sent.
                 The value of this object must be reported as 0 when no probes
                 have been sent."
    ::= { pingMgt 7 }

pingReceivedPackets OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Number of responses received. The value of this object must
                 be reported as 0 when no probe responses have been received."
    ::= { pingMgt 8 }

-- For CHT

pingPacketLossRate OBJECT-TYPE
    SYNTAX      INTEGER(0..100)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Packet loss rate of this ping operation. This variable is
                 calculated by pingReceivedPackets and pingSentPackets. The
                 rate is expressed as a percentage."
    ::= { pingMgt 9 }


-- For CHT

pingHistoryTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PingHistoryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Contains the executive result information for the ping
                 operation."
    ::= { pingMgt 10 }

pingHistoryEntry OBJECT-TYPE
    SYNTAX      PingHistoryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A conceptual row in the pingHistory table."
    INDEX { pingHistoryIndex  }
    ::= { pingHistoryTable 1 }

PingHistoryEntry::= SEQUENCE
{
    pingHistoryIndex          Integer32,
    pingHistoryResponse       Integer32
}

pingHistoryIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A new entry in this table is created when the result of
                 a ping probe is determined. The old entries will be cleared
                 when a new ping action is started."
    ::= { pingHistoryEntry  1 }

pingHistoryResponse OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This variable represents the round trip time and is
                 measured in milliseconds. The variable is the difference
                 between received time and sent time for a ping probe. If
                 the difference value is more than the time-out value or no
                 response is received, then the variable will be 5000
                 milliseconds."
    ::= { pingHistoryEntry 2 }

--
-- vlanMgt
--

-- Management for Virtual Local Area Network (VLAN).
-- This has variables not already defined in the implemented
-- standard MIB(s).

vlanTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF VlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for VLAN configuration."
        ::= { vlanMgt 1 }

vlanEntry OBJECT-TYPE
        SYNTAX      VlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for VLAN configuration."
        INDEX       { vlanIndex }
        ::= { vlanTable 1 }

VlanEntry ::= SEQUENCE
{
    vlanIndex               Unsigned32,
    vlanAddressMethod       INTEGER
}

vlanIndex OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Based on dot1qVlanIndex in the Q-BRIDGE-MIB.
            This table has only one entry - the entry for
            the VLAN of the management interface."
        ::= { vlanEntry 1 }

vlanAddressMethod OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        user(1),
                        bootp(2),
                        dhcp(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Method to get the IP address."
        ::= { vlanEntry 2 }

vlanPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF VlanPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for port configuration in VLAN."
        ::= { vlanMgt 2 }

vlanPortEntry OBJECT-TYPE
        SYNTAX      VlanPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for port configuration in VLAN."
        INDEX       { vlanPortIndex }
        ::= { vlanPortTable 1 }

VlanPortEntry ::= SEQUENCE
{
    vlanPortIndex            Integer32,
    vlanPortMode             INTEGER
}

vlanPortIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and the trunk (excluding trunk members) interface of
                     the portTable. The interface identified by a particular value
                     of this index is the same interface as identified by the same
                     value of dot1qPvid in the Q-BRIDGE-MIB."
        ::= { vlanPortEntry 1 }

vlanPortMode OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        hybrid(1),
                        dot1qTrunk(2),
                        access(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This variable sets the 802.1Q VLAN mode.
                    Setting it to hybrid(1) sets a hybrid link.
                    Setting it to dot1qTrunk(2) sets a trunk link.
                    Setting it to access(3) sets an access link."
        ::= { vlanPortEntry 2 }

vlanDot1qTunnelGlobalConfig OBJECT IDENTIFIER ::= { vlanMgt 8 }

vlanDot1qTunnelStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This parameter is used to globally enable/disable
                     802.1Q Tunneling on the device."
        ::= { vlanDot1qTunnelGlobalConfig 1 }

vlanDot1qTunnelPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF VlanDot1qTunnelPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for port configuration in 802.1Q Tunneling."
        ::= { vlanMgt 9 }

vlanDot1qTunnelPortEntry OBJECT-TYPE
        SYNTAX      VlanDot1qTunnelPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for port configuration in 802.1Q Tunneling."
        INDEX       { vlanDot1qTunnelPortIndex }
        ::= { vlanDot1qTunnelPortTable 1 }

VlanDot1qTunnelPortEntry ::= SEQUENCE
{
    vlanDot1qTunnelPortIndex                Integer32,
    vlanDot1qTunnelPortMode                 INTEGER,
    vlanDot1qTunnelPortEtherType            Unsigned32
}

vlanDot1qTunnelPortIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and the trunk (excluding trunk members) interface of
                     the portTable. The interface identified by a particular value
                     of this index is the same interface as identified by the same
                     value of ifIndex in the IF-MIB."
        ::= { vlanDot1qTunnelPortEntry 1 }

vlanDot1qTunnelPortMode OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        none(1),
                        access(2),
                        uplink(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This variable sets the 802.1Q Tunneling mode.
                     Setting it to none(1) indicates no mode in this port.
                     Setting it to access(2) sets as dot1q-tunnel mode port which link to customer.
                     Setting it to uplink(3) sets as dot1q-tunnel mode port which link to service-provider.
                     If vlanDot1qTunnelStatus is disabled, it means vlanDot1qTunnelPortMode is inactive."
        ::= { vlanDot1qTunnelPortEntry 2 }

vlanDot1qTunnelPortEtherType OBJECT-TYPE
       SYNTAX     Unsigned32 ('0800'h..'ffff'h)
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION "TPID for 802.1Q encapsulation. It's used to select a nonstandard
                    (nondefault) 2-byte ethertype to identify 802.1Q tagged frames."
       ::= { vlanDot1qTunnelPortEntry 3 }

--
-- voiceVlanMgt
--

voiceVlanMgt        OBJECT IDENTIFIER ::= { vlanMgt 6 }

voiceVlanOuiTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF VoiceVlanOuiEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A table containing the mac address which can be identified
                 by Voice VLAN."
    ::= { voiceVlanMgt 1 }

voiceVlanOuiEntry OBJECT-TYPE
        SYNTAX  VoiceVlanOuiEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION "A table containing the mac address which can be identified
                     by Voice VLAN."
        INDEX   { voiceVlanOuiAddress }
        ::= { voiceVlanOuiTable 1 }

VoiceVlanOuiEntry	::=
        SEQUENCE
        {
            voiceVlanOuiAddress	    MacAddress,
            voiceVlanOuiMask        MacAddress,
            voiceVlanOuiDescription DisplayString,
            voiceVlanOuiStatus      ValidStatus
        }

voiceVlanOuiAddress OBJECT-TYPE
        SYNTAX      MacAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "MAC address can be identified by voice vlan."
        ::= { voiceVlanOuiEntry 1 }

voiceVlanOuiMask OBJECT-TYPE
        SYNTAX      MacAddress
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The mask of MAC address."
        ::= { voiceVlanOuiEntry 2 }

voiceVlanOuiDescription OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..30))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The description of OUI."
        ::= { voiceVlanOuiEntry 3 }

voiceVlanOuiStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Current operation status of the row."
        ::= { voiceVlanOuiEntry 4 }

voiceVlanEnabledId OBJECT-TYPE
        SYNTAX      INTEGER (-1|1..4093)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Voice VLAN enabled status and VLAN ID:
                     enabled (1..4093), disabled (-1)."
        ::= { voiceVlanMgt 2 }

voiceVlanAgingTime OBJECT-TYPE
        SYNTAX  INTEGER (5..43200)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "Voice VLAN aging time, the unit of which is minute."
        DEFVAL      { 1440 }
        ::= { voiceVlanMgt 3 }

voiceVlanPortTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF VoiceVlanPortEntry
        MAX-ACCESS not-accessible
        STATUS   current
        DESCRIPTION "A list of voice VLAN port entries."
        ::= { voiceVlanMgt 7 }

voiceVlanPortEntry OBJECT-TYPE
        SYNTAX      VoiceVlanPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry containing Voice VLAN port information,
                    which is applicable to a Voice VLAN enabled interface."
        INDEX   { voiceVlanPortIfIndex }
        ::= { voiceVlanPortTable 1 }

VoiceVlanPortEntry ::=
        SEQUENCE
        {
            voiceVlanPortIfIndex   Integer32,
            voiceVlanPortMode      INTEGER,
            voiceVlanPortSecurity  EnabledStatus,
            voiceVlanPortPriority  INTEGER,
            voiceVlanPortRuleOui   EnabledStatus,
            voiceVlanPortRuleLldp  EnabledStatus,
            voiceVlanPortRemainAge Integer32
        }

voiceVlanPortIfIndex OBJECT-TYPE
        SYNTAX      Integer32(1..2147483647)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The index of interface on which Voice VLAN function
                    is enabled."
        REFERENCE "IfIndex in RFC1213."
    ::= { voiceVlanPortEntry 1 }

voiceVlanPortMode OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        auto(1),
                        manual(2),
                        none(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Voice VLAN configuration mode status."
        ::= { voiceVlanPortEntry 2 }

voiceVlanPortSecurity OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "If the security is enabled, the port only allows voice
                     traffic for the Voice VLAN."
        ::= { voiceVlanPortEntry 3 }

voiceVlanPortPriority OBJECT-TYPE
        SYNTAX      INTEGER(0..6)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The priority of the voice vlan traffic in the port."
        ::= { voiceVlanPortEntry 4 }

voiceVlanPortRuleOui OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The address of voice device is learned from
                     OUI table."
        ::=  { voiceVlanPortEntry 5 }

voiceVlanPortRuleLldp OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The address of voice device is learned from
                     LLDP discovery."
        ::= { voiceVlanPortEntry 6 }

voiceVlanPortRemainAge OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION  "Remaining age, the units of which is minutes.
                      - 1 means NA (not applicable); - 2 means not started;
                      - 3 means less than 1 minute."
        ::= { voiceVlanPortEntry 7 }

--
-- macVlanMgt
--

macVlanTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF MacVlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table that contains the settings for MAC-based VLAN."
        ::= { vlanMgt 11 }

macVlanEntry OBJECT-TYPE
        SYNTAX      MacVlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A conceptual row in the macVlanTable."
        INDEX       { macVlanMacAddress }
        ::= { macVlanTable 1 }

MacVlanEntry ::= SEQUENCE
{
        macVlanMacAddress       MacAddress,
        macVlanId               Integer32,
        macVlanPriority         Integer32,
        macVlanStatus           ValidStatus
}

macVlanMacAddress OBJECT-TYPE
        SYNTAX      MacAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The MAC address that may specify an entry in the table
                     which contains MAC-based VLAN information."
        ::= { macVlanEntry 1 }

macVlanId OBJECT-TYPE
        SYNTAX      Integer32 (1..4092)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Specifies the VLAN ID which the MAC address associates
                     with."
        ::= { macVlanEntry 2 }

macVlanPriority OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Specifies the priority whcich the MAC address associates
                     with."
        ::= { macVlanEntry 3 }

macVlanStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Set this to valid(1) to create an entry. Set this to
                     invalid(2) to destroy an entry."
        ::= { macVlanEntry 4 }

macVlanClearAction OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        noClear(1),
                        clear(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Action for clearing macVlanTable. When this object is set
                     to clear(2), all entries in macVlanTable will be cleared.
                     When this object is read, the value of this object is
                     always noClear(1)."
        ::= { vlanMgt 12 }

--
-- subnetVlanMgt
--

subnetVlanTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF SubnetVlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table that contains the settings for IP subnet-based
                     VLAN."
        ::= { vlanMgt 13 }

subnetVlanEntry OBJECT-TYPE
        SYNTAX      SubnetVlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A conceptual row in the subnetVlanTable."
        INDEX       { subnetVlanMask, subnetVlanIpAddress }
        ::= { subnetVlanTable 1 }

SubnetVlanEntry ::= SEQUENCE
{
        subnetVlanIpAddress IpAddress,
        subnetVlanMask      IpAddress,
        subnetVlanId        Integer32,
        subnetVlanPriority  Integer32,
        subnetVlanStatus    ValidStatus
}

subnetVlanIpAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The IPv4 address of a subnet. Any assignment (implicit or
                     otherwise) of an instance of this object to a value x must
                     be rejected if the bitwise logical-AND of x with the value
                     of the corresponding instance of the subnetVlanMask object
                     is not equal to x."
        ::= { subnetVlanEntry 1 }

subnetVlanMask OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The netmask of a subnet. Any assignment (implicit or
                     otherwise) of an instance of this object to a value x must
                     be rejected if the bitwise logical-AND of x with the value
                     of the corresponding instance of the subnetVlanIpAddress
                     object is not equal to subnetVlanIpAddress."
        ::= { subnetVlanEntry 2 }

subnetVlanId OBJECT-TYPE
        SYNTAX      Integer32 (1..4094)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Specifies the VLAN ID which the subnet associates with."
        ::= { subnetVlanEntry 3 }

subnetVlanPriority OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Specifies the priority whcich the subnet associates with."
        ::= { subnetVlanEntry 4 }

subnetVlanStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Set this to valid(1) to create an entry. Set this to
                     invalid(2) to destroy an entry."
        ::= { subnetVlanEntry 5 }

subnetVlanClearAction OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        noClear(1),
                        clear(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Action for clearing subnetVlanTable. When this object is
                     set to clear(2), all entries in subnetVlanTable will be
                     cleared. When this object is read, the value of this object
                     is always noClear(1)."
        ::= { vlanMgt 14 }

--
-- L2/L3 VLAN Mgt
--

vlanStaticTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF VlanStaticEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for static VLAN configuration including VLAN aggregation support."
    ::= { vlanMgt 17 }

vlanStaticEntry OBJECT-TYPE
    SYNTAX      VlanStaticEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Static information for a VLAN configured on the device by (local or
         network) management."
    INDEX
    {
        vlanStaticIndex
    }
    ::= { vlanStaticTable 1 }

VlanStaticEntry ::= SEQUENCE
{
    vlanStaticIndex                 VlanIndex,
    vlanStaticInterfaceType         INTEGER
}

vlanStaticIndex OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The VLAN ID of the VLAN."
    ::= { vlanStaticEntry 1 }

vlanStaticInterfaceType OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    l2vlan(135),
                    l3ipvlan(136)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The interface type of the VLAN (there is a subtype of IANAifType).
         l2vlan(135) refers to L2 interface and can't accept any L3 related
         configuration. l3ipvlan(136) refers to L3 interface and can accept
         L3 related configuration."
    DEFVAL      { l2vlan }
    ::= { vlanStaticEntry 2 }

--
-- priorityMgt
--

-- Management for traffic priority. This allows a user
-- to specify which data packets have greater precedence
-- when traffic is buffered in the switch due to congestion.

prioIpPrecDscpStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        disabled(1),
                        precedence(2),
                        dscp(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Selects whether no frame priority mapping, IP ToS
                     precedence mapping or DSCP mapping is performed."
        ::= { priorityMgt 1 }

prioIpDscpTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PrioIpDscpEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for IP DSCP priority mapping."
        ::= { priorityMgt 4 }

prioIpDscpEntry OBJECT-TYPE
        SYNTAX      PrioIpDscpEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for IP DSCP priority mapping."
        INDEX       { prioIpDscpPort, prioIpDscpValue }
        ::= { prioIpDscpTable 1 }

PrioIpDscpEntry ::= SEQUENCE
{
    prioIpDscpPort           Integer32,
    prioIpDscpValue          Integer32,
    prioIpDscpCos            Integer32
}

prioIpDscpPort OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and the trunk (excluding trunk members) interface of
                     the portTable. The interface identified by a particular value
                     of this index is the same interface as identified by the same
                     value of ifIndex in the IF-MIB."
        ::= { prioIpDscpEntry 1 }

prioIpDscpValue OBJECT-TYPE
        SYNTAX      Integer32 (0..63)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Value of IP DSCP as specified in the packet header."
        ::= { prioIpDscpEntry 2 }

prioIpDscpCos OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Class of Service as defined by dot1dTrafficClassPriority
                     in the P-BRIDGE-MIB. The prioIpDscpValue value in the same
                     table row will be mapped to this Class of Service (CoS).
                     This CoS is then further mapped to the hardware
                     queue according to dot1dTrafficClassTable."
        REFERENCE   "P-BRIDGE-MIB.dot1dPriority.dot1dTrafficClassTable."
        ::= { prioIpDscpEntry 3 }

prioIpDscpRestoreDefault OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Enables the IP DSCP settings of a port to be reset to their
                     defaults. To reset the IP DSCP settings of a port, assign
                     the value of the relevant ifIndex defined by the ifIndex in
                     the IF-MIB. For example, assigning the value 1 will result in
                     the IP DSCP settings of port 1 being restored to their default.
                     0 will always be obtained when reading this variable"
        ::= { priorityMgt 5 }

-- optional

prioCopy            OBJECT IDENTIFIER ::= { priorityMgt 8 }

prioCopyIpDscp OBJECT-TYPE
        SYNTAX      OCTET STRING
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Action to copy IP DSCP settings from
                    a source port to many destination ports.
                    The first four octets represent an integer for
                    the source port in high-to-low (big-endian) order.
                    Starting from the 5th octet is the destination port list
                    in a form described by PortList in the Q-BRIDGE-MIB.
                    Writing this object will perform copy.
                    Reading this object will always get a zero-length
                    octet string."
        ::= { prioCopy 2 }

prioWrrTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PrioWrrEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for weighted round robin (WRR)."
        ::= { priorityMgt 9 }

prioWrrEntry OBJECT-TYPE
        SYNTAX      PrioWrrEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for weighted round robin (WRR)."
        INDEX       { prioWrrTrafficClass }
        ::= { prioWrrTable 1 }

PrioWrrEntry ::= SEQUENCE
{
    prioWrrTrafficClass    Integer32,
    prioWrrWeight          Integer32
}

prioWrrTrafficClass OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Traffic class for this entry, as defined in
                    dot1dTrafficClass in the P-BRIDGE-MIB. The actual
                    maximum depends on the hardware, and is
                    equal to dot1dPortNumTrafficClasses-1."
        REFERENCE "MIB.IETF|P-BRIDGE-MIB.dot1dTrafficClass."
        ::= { prioWrrEntry 1 }

prioWrrWeight OBJECT-TYPE
        SYNTAX      Integer32 (0..255)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Weight for this entry.  0 means strict queue."
        ::= { prioWrrEntry 2 }

prioQueueMode OBJECT-TYPE
        SYNTAX 	INTEGER {
	                wrr(1),
	                strict(2),
	                strict-wrr(4)
            	}
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The global status for the prioQueue. Set to wrr(1) for
                     Weighted Round Robin mode. Set to strict(2) for strict
                     mode. Set to
                     strict-wrr(4) for WRR and strict mode. 
                     Mode wrr(1) and strict-wrr(4)
                     refer to prioPortTable."
        ::= { priorityMgt 10 }

-- prioAclToCosTable

prioAclToCosTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PrioAclToCosEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for ACL to CoS Mapping."
        ::= { priorityMgt 13 }

prioAclToCosEntry OBJECT-TYPE
        SYNTAX      PrioAclToCosEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for ACL to CoS Mapping."
        INDEX       { prioAclToCosIfIndex }
        ::= { prioAclToCosTable 1 }

PrioAclToCosEntry ::= SEQUENCE
{
    prioAclToCosIfIndex    Integer32,
    prioAclToCosIpAclName  DisplayString,
    prioAclToCosMacAclName DisplayString,
    prioAclToIpCosValue      Integer32,
    prioAclToMacCosValue      Integer32
}

prioAclToCosIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port interface of the prioAclToCosEntry. The interface
                     identified by a particular value of this index is the
                     same interface as identified by the same value of
                     ifIndex in the IF-MIB."
        ::= { prioAclToCosEntry 1 }

prioAclToCosIpAclName OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..16))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The name of an IP ACL. Within a feature, a unique
                    name is used to identify the list to
                    which the entry belongs in the device."
        ::= { prioAclToCosEntry 2 }

prioAclToCosMacAclName OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..16))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The name of an MAC ACL. Within a feature a unique
                    name is used to identify the list to
                    which the entry belongs in the device."
        ::= { prioAclToCosEntry 3 }

prioAclToIpCosValue OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "IP CoS for this entry."
        ::= { prioAclToCosEntry 4 }

prioAclToMacCosValue OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "MAC CoS for this entry."
        ::= { prioAclToCosEntry 5 }

--
-- trapDestMgt
--

-- Management for SNMP traps and trap destinations.

trapDestTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF TrapDestEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A list of trap destination entries."
    REFERENCE "RMON2-MIB, mib2(1).rmon(16).probeConfig(19).trapDestTable(13)."
    ::= { trapDestMgt 1 }

trapDestEntry  OBJECT-TYPE
    SYNTAX     TrapDestEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION  "A destination entry describes the destination IP address,
                  the community string, and SNMP version to use when sending
                  a trap."
    INDEX { trapDestAddress }
    ::= { trapDestTable 1 }

TrapDestEntry ::= SEQUENCE {
    trapDestAddress             IpAddress,
    trapDestCommunity           OCTET STRING,
    trapDestStatus              ValidStatus,
    trapDestVersion             INTEGER,
    trapDestUdpPort             Integer32
}

trapDestAddress  OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The address to send traps."
    ::= { trapDestEntry 1 }

trapDestCommunity  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(0..32))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "A community to which this destination address belongs."
    ::= { trapDestEntry 2 }

trapDestStatus  OBJECT-TYPE
    SYNTAX     ValidStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "Setting this to valid(1) creates an entry.
         Setting this to invalid(2) destroys an entry."
    ::= { trapDestEntry 3 }

trapDestVersion OBJECT-TYPE
    SYNTAX      INTEGER
                {
                   version1(1),
                   version2(2)
                }
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION "Determines the version of the trap that is to be sent to the
                 trap receiver. If the value is 1, then an SNMP version 1 trap
                 is sent and if the value is 2, an SNMP version 2 trap is
                 sent."
    ::= { trapDestEntry 4 }

trapDestUdpPort OBJECT-TYPE
    SYNTAX      Integer32 ( 1..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Determines the UDP port number that the trap will be sent to."
    DEFVAL      { 162 }
    ::= { trapDestEntry 5 }

-- trapVar is for binding variables for traps, there is no value when
-- no trap is sent.

trapVar OBJECT IDENTIFIER ::= { trapDestMgt 2 }

-- For IP Filter Reject

trapIpFilterRejectMode OBJECT-TYPE
     SYNTAX      INTEGER
                 {
                     web(1),
                     snmp(2),
                     telnet(3)
                 }
     MAX-ACCESS  accessible-for-notify
     STATUS      current
     DESCRIPTION "This variable is for trap var binding,
                  indicated the ipfilter reject mode.
                  web(1),
                  snmp(2),
                  telnet(3)."
     ::= { trapVar 6 }

trapIpFilterRejectInetAddressType OBJECT-TYPE
     SYNTAX      InetAddressType
     MAX-ACCESS  accessible-for-notify
     STATUS      current
     DESCRIPTION "This variable is for trap var binding, indicating
                  the IP address that was rejected by the IP filter."
     ::= { trapVar 17 }

trapIpFilterRejectInetAddress OBJECT-TYPE
     SYNTAX      InetAddress
     MAX-ACCESS  accessible-for-notify
     STATUS      current
     DESCRIPTION "This variable is for trap var binding, indicating
                  the IP address that was rejected by the IP filter."
     ::= { trapVar 18 }

trapLoginMode OBJECT-TYPE
     SYNTAX      INTEGER
                 {
                     console(1),
                     telnet(2),
                     web(3)
                 }
     MAX-ACCESS  accessible-for-notify
     STATUS      current
     DESCRIPTION "This variable is for trap var binding,
                  indicated the login mode.
                  console(1),
                  telnet(2),
                  web(3)."
     ::= { trapVar 19 }

trapLoginUsername OBJECT-TYPE
     SYNTAX      DisplayString
     MAX-ACCESS  accessible-for-notify
     STATUS      current
     DESCRIPTION "This variable is for trap var binding,
                 indicating the login username."
     ::= { trapVar 20 }

trapLoginIp OBJECT-TYPE
     SYNTAX      Integer32
     MAX-ACCESS  accessible-for-notify
     STATUS      current
     DESCRIPTION "This variable is for trap var binding,
                 indicating the login IP address."
     ::= { trapVar 21 }

--For Auto Upgrade

trapAutoUpgradeResult OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    succeeded(1),
                    failed(2)
                }
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION "The parameter indicates which result triggers the trap."
    ::= { trapVar 22 }

trapAutoUpgradeNewVer OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..20))
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION "The parameter indicates new version which was upgraded to.
                 When trapAutoUpgradeResult was failed(2), it would be
                 null string."
    ::= { trapVar 23 }

trapPortSecurityIntrusionMac OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION "This variable indicates the intrusion MAC address."
    ::= { trapVar 29 }

--
-- qosMgt
--

-- Management for Quality of Service (QoS) for network traffic.

--
-- rateLimitMgt
--

-- optional

rateLimitMgt        OBJECT IDENTIFIER ::= { qosMgt 1 }

rateLimitPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RateLimitPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for rate limit of each port."
        ::= { rateLimitMgt 2 }

rateLimitPortEntry OBJECT-TYPE
        SYNTAX      RateLimitPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for rate limit of each port."
        INDEX       { rlPortIndex }
        ::= { rateLimitPortTable 1 }


RateLimitPortEntry ::= SEQUENCE
{
    rlPortIndex              Integer32,
    rlPortInputStatus        EnabledStatus,
    rlPortOutputStatus       EnabledStatus,
    rlPortInputLimitInKilo   Integer32,
    rlPortOutputLimitInKilo  Integer32
}

rlPortIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and the trunk (including trunk member) interface of
                     the portTable. The interface identified by a particular value
                     of this index is the same interface as identified by the same
                     value of ifIndex in the IF-MIB."
        ::= { rateLimitPortEntry 1 }

-- all need (both acd and non-acd)
rlPortInputStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Whether input rate limit is enabled for this port."
        ::= { rateLimitPortEntry 6 }

-- all need (both acd and non-acd)
rlPortOutputStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Whether output rate limit is enabled for this port."
        ::= { rateLimitPortEntry 7 }

rlPortInputLimitInKilo OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Value of the input rate limit. Its unit is kilobits per
                     second. For a 100 Mbps port, the range is 64 to 100000.
                     For a 1000 Mbps port, the range is 64 to 1000000."
        ::= { rateLimitPortEntry 10 }

rlPortOutputLimitInKilo OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Value of the output rate limit. Its unit is kilobits per
                     second. For a 100 Mbps port, the range is 64 to 100000.
                     For a 1000 Mbps port, the range is 64 to 1000000."
        ::= { rateLimitPortEntry 11 }

cosMgt        OBJECT IDENTIFIER ::= { qosMgt 3 }

--prioAclToCosMappingTable
prioAclToCosMappingTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PrioAclToCosMappingEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for ACL to CoS Mapping."
        ::= { cosMgt 1 }

prioAclToCosMappingEntry OBJECT-TYPE
        SYNTAX      PrioAclToCosMappingEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for ACL to CoS Mapping."
        INDEX       { prioAclToCosMappingIfIndex, prioAclToCosMappingAclName }
        ::= { prioAclToCosMappingTable 1 }

PrioAclToCosMappingEntry ::= SEQUENCE
{
    prioAclToCosMappingIfIndex  Integer32,
    prioAclToCosMappingAclName  DisplayString,
    prioAclToCosMappingCosValue Integer32,
    prioAclToCosMappingStatus   RowStatus
}

prioAclToCosMappingIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port interface of the prioAclToCosMappingEntry. The interface
                     identified by a particular value of this index is the
                     same interface as identified by the same value of
                     ifIndex in the IF-MIB."
        ::= { prioAclToCosMappingEntry 1 }

prioAclToCosMappingAclName OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(1..16))
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The name of an IP ACL. Within a feature a unique name is
                     used to identify the list to which the entry belongs
                     in the device."
        ::= { prioAclToCosMappingEntry 2 }

prioAclToCosMappingCosValue OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "CoS value of the prioAclToCosMappingTable."
        ::= { prioAclToCosMappingEntry 3 }

prioAclToCosMappingStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The status of this conceptual row entry. This object isused to manage the
            creation and deletion of conceptual rows.

            The status column has six defined values:

                 - 'active', which indicates that the conceptual row is
                 available for use by the managed device;

                 - 'notInService', which indicates that the conceptual
                 row exists in the agent, but is unavailable for use by
                 the managed device (see NOTE below);

                 - 'notReady', which indicates that the conceptual row
                 exists in the agent, but is missing information
                 necessary in order to be available for use by the
                 managed device;

                 - 'createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device;

                 - 'createAndWait', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row (but not make it available for use by
                 the managed device); and,

                 - 'destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Whereas five of the six values (all except 'notReady') may
            be specified in a management protocol set operation, only
            three values will be returned in response to a management
            protocol retrieval operation:  'notReady', 'notInService' or
            'active'.  That is, when queried, an existing conceptual row
            has only three states:  it is either available for use by
            the managed device (the status column has value 'active');
            it is not available for use by the managed device, though
            the agent has sufficient information to make it so (the
            status column has value 'notInService'); or, it is not
            available for use by the managed device, and an attempt to
            make it so would fail because the agent has insufficient
            information (the state column has value 'notReady').

            For a detailed description of this object, please refer to
            SNMPv2-TC MIB."
        ::= { prioAclToCosMappingEntry 4 }

prioIfClassificationModeTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PrioIfClassificationModeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for setting the interface Qos mapping classification mode."
    ::= { cosMgt 2 }

prioIfClassificationModeEntry OBJECT-TYPE
    SYNTAX      PrioIfClassificationModeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for setting the interface Qos mapping classification mode."
    INDEX
    {
        prioIfClassificationModeIf
    }
    ::= { prioIfClassificationModeTable 1 }

PrioIfClassificationModeEntry ::= SEQUENCE
{
    prioIfClassificationModeIf     Integer32,
    prioIfClassificationModeStatus INTEGER
}

prioIfClassificationModeIf OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The port or trunk interface of the device. The interface identified by
         a particular value of this index is the same interface as identified
         by the same value of ifIndex in the IF-MIB."
    ::= { prioIfClassificationModeEntry 1 }

prioIfClassificationModeStatus OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    cos(0),
                    dscp(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The QoS mapping classification mode of the interface. CoS mode means
         that the internal priority is mapped from priority field of packet's
         VLAN tag if a VLAN tag exists;
         DSCP mode means that the internal priority is mapped from the
         DSCP value of IP packets."
    ::= { prioIfClassificationModeEntry 2 }


--
-- The mapping table from CoS/CFI to internal QoS label
--

prioCosToDscpTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PrioCosToDscpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for CoS/CFI to internal QoS label mapping."
    ::= { cosMgt 3 }

prioCosToDscpEntry OBJECT-TYPE
    SYNTAX      PrioCosToDscpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for CoS/CFI to internal QoS label mapping."
    INDEX
    {
          prioCosToDscpIfValue,
          prioCosToDscpCosValue,
          prioCosToDscpCFIValue
    }
    ::= { prioCosToDscpTable 1 }

PrioCosToDscpEntry ::= SEQUENCE
{
    prioCosToDscpIfValue    Integer32,
    prioCosToDscpCosValue   Integer32,
    prioCosToDscpCFIValue   Integer32,
    prioCosToDscpDscpValue  Integer32
}

prioCosToDscpIfValue OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The port or the trunk interface of the device. The interface
         identified by a particular value of this index is the same interface
         as identified by the same value of ifIndex in the IF-MIB."
    ::= { prioCosToDscpEntry 1 }

prioCosToDscpCosValue OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The CoS value (0 to 7) mapped to an internal QoS label value which is
         composed of PHB (3 bits) and drop precedence (2 bits)."
    ::= { prioCosToDscpEntry 2 }

prioCosToDscpCFIValue OBJECT-TYPE
    SYNTAX      Integer32 (0..1)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The CFI value (0 or 1) mapped to an internal QoS label value which is
         composed of PHB (3 bits) and drop precedence (2 bits)."
    ::= { prioCosToDscpEntry 3 }

prioCosToDscpDscpValue OBJECT-TYPE
    SYNTAX      Integer32 (0..31)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The DSCP value used to represent internal QoS label (3 bits PHB + 2
         bits Drop precedence). The high 3 bits of DSCP are used to represent
         PHB value of QoS label; The low 2 bits of DSCP are used to represent
         the drop precedence value of QoS label: Green(0), Yellow(3), Red(1).
         In a word, PHB = DSCP right-shift 2, Drop precedence = DSCP
         bitwise-and '3'h.

         Note: The setting range of PHB value must be from 0 to 7 and the 
         setting drop precedence value must be one of the values (0, 1, 3)."
    ::= { prioCosToDscpEntry 4 }

--
-- The mapping table from IP precedence to internal Qos label
--

prioPrecToDscpTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PrioPrecToDscpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for IP precedence to internal QoS label mapping. This table
         setting will take effect only when the interface QoS mapping
         classification mode is set to IP precedence mode."
    ::= { cosMgt 4 }

prioPrecToDscpEntry OBJECT-TYPE
    SYNTAX      PrioPrecToDscpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for IP precedence to internal QoS label mapping."
    INDEX
    {
        prioPrecToDscpIfValue,
        prioPrecToDscpPrecValue
    }
    ::= { prioPrecToDscpTable 1 }

PrioPrecToDscpEntry ::= SEQUENCE
{
    prioPrecToDscpIfValue   Integer32,
    prioPrecToDscpPrecValue Integer32,
    prioPrecToDscpDscpValue Integer32
}

prioPrecToDscpIfValue OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The port or trunk interface of the device. The interface identified by
         a particular value of this index is the same interface as identified
         by the same value of ifIndex in the IF-MIB."
    ::= { prioPrecToDscpEntry 1 }

prioPrecToDscpPrecValue OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP precedence value mapped to internal QoS label value which is
         composed of PHB (3 bits) and drop precedence (2 bits)."
    ::= { prioPrecToDscpEntry 2 }

prioPrecToDscpDscpValue OBJECT-TYPE
    SYNTAX      Integer32 (0..31)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The DSCP value used to represent internal QoS label (3 bits PHB + 2
         bits Drop precedence). The high 3 bits of DSCP are used to represent
         PHB value of QoS label; The low 2 bits of DSCP are used to represent
         the drop precedence value of QoS label: Green(0), Yellow(3), Red(1).
         In a word, PHB = DSCP right-shift 2, Drop precedence = DSCP
         bitwise-and '3'h.

         Note: The setting range of PHB value must be from 0 to 7 and the 
         setting drop precedence value must be one of the values (0, 1, 3)."
    ::= { prioPrecToDscpEntry 3 }

--
-- The mapping table from DSCP to internal Qos label
--

prioDscpToDscpTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PrioDscpToDscpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for DSCP to internal QoS label mapping. This table setting will
         take effect only when the interface Qos mapping classification mode is
         set to DSCP mode."
    ::= { cosMgt 5 }

prioDscpToDscpEntry OBJECT-TYPE
    SYNTAX      PrioDscpToDscpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for ingress DSCP to internal QoS label mapping."
    INDEX
    {
        prioDscpToDscpIfValue,
        prioDscpToDscpIngressDscpValue
    }
    ::= { prioDscpToDscpTable 1 }

PrioDscpToDscpEntry ::= SEQUENCE
{
    prioDscpToDscpIfValue           Integer32,
    prioDscpToDscpIngressDscpValue  Integer32,
    prioDscpToDscpDscpValue         Integer32
}

prioDscpToDscpIfValue OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The port or trunk interface of the device. The interface identified by
         a particular value of this index is the same interface as identified
         by the same value of ifIndex in the IF-MIB."
    ::= { prioDscpToDscpEntry 1 }

prioDscpToDscpIngressDscpValue OBJECT-TYPE
    SYNTAX      Integer32 (0..63)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ingress DSCP value which will be mapped to internal QoS label
         value."
    ::= { prioDscpToDscpEntry 2 }

prioDscpToDscpDscpValue OBJECT-TYPE
    SYNTAX      Integer32 (0..31)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The DSCP value used to represent internal QoS label (3 bits PHB + 2
         bits Drop precedence). The high 3 bits of DSCP are used to represent
         PHB value of QoS label; The low 2 bits of DSCP are used to represent
         the drop precedence value of QoS label: Green(0), Yellow(3), Red(1).
         In a word, PHB = DSCP right-shift 2, Drop precedence = DSCP
         bitwise-and '3'h.

         Note: The setting range of PHB value must be from 0 to 7 and the 
         setting drop precedence value must be one of the values (0, 1, 3)."
    ::= { prioDscpToDscpEntry 3 }

--
-- The mapping table from TCP/UDP destination port number to internal Qos label
--

prioDstPortToDscpTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PrioDstPortToDscpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for TCP/UDP destination port number to internal Qos label
         mapping. This table setting will always take effect for TCP/UDP
         packets no matter of what interface QoS mapping classification mode is
         set."
    ::= { cosMgt 6 }

prioDstPortToDscpEntry OBJECT-TYPE
    SYNTAX      PrioDstPortToDscpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for TCP/UDP destination port to internal QoS label mapping."
    INDEX
    {
        prioDstPortToDscpIfValue,
        prioDstPortToDscpProtocolValue,
        prioDstPortToDscpDstPortValue
    }
    ::= { prioDstPortToDscpTable 1 }

PrioDstPortToDscpEntry ::= SEQUENCE
{
    prioDstPortToDscpIfValue        Integer32,
    prioDstPortToDscpProtocolValue  INTEGER,
    prioDstPortToDscpDstPortValue   Integer32,
    prioDstPortToDscpDscpValue      Integer32
}

prioDstPortToDscpIfValue OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The port or the trunk interface of the device. The interface
         identified by a particular value of this index is the same interface
         as identified by the same value of ifIndex in the IF-MIB."
    ::= { prioDstPortToDscpEntry 1 }

prioDstPortToDscpProtocolValue OBJECT-TYPE
    SYNTAX      INTEGER
                {
                      tcp(6),
                      udp(17)
                }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The protocol value (TCP:6, UDP:17) which will be mapped to internal
         QoS label value."
::= { prioDstPortToDscpEntry 2 }

prioDstPortToDscpDstPortValue OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The destination port number value which will be mapped to internal
         QoS label value."
    ::= { prioDstPortToDscpEntry 3 }

prioDstPortToDscpDscpValue OBJECT-TYPE
    SYNTAX      Integer32 (0..31)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The DSCP value used to represent internal QoS label (3 bits PHB + 2
         bits Drop precedence). The high 3 bits of DSCP are used to represent
         PHB value of QoS label; The low 2 bits of DSCP are used to represent
         the drop precedence value of QoS label: Green(0), Yellow(3), Red(1).
         In a word, PHB = DSCP right-shift 2, Drop precedence = DSCP
         bitwise-and '3'h.

         Note: The setting range of PHB value must be from 0 to 7 and the 
         setting drop precedence value must be one of the values (0, 1, 3)."
    ::= { prioDstPortToDscpEntry 4 }


--
-- The mapping table from internal Qos label to CoS and CFI
--

prioDscpToCosTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PrioDscpToCosEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for internal QoS label to CoS and CFI mapping."
    ::= { cosMgt 7 }

prioDscpToCosEntry OBJECT-TYPE
    SYNTAX      PrioDscpToCosEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for internal QoS label to CoS and CFI mapping."
    INDEX
    {
        prioDscpToCosIfValue,
        prioDscpToCosPHBValue,
        prioDscpToCosDropPrecedenceValue
    }
    ::= { prioDscpToCosTable 1 }

PrioDscpToCosEntry ::= SEQUENCE
{
    prioDscpToCosIfValue                Integer32,
    prioDscpToCosPHBValue               Integer32,
    prioDscpToCosDropPrecedenceValue    INTEGER,
    prioDscpToCosCFICosValue            Integer32
}

prioDscpToCosIfValue OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The port or trunk interface of the device. The interface identified by
         a particular value of this index is the same interface as identified
         by the same value of ifIndex in the IF-MIB."
    ::= { prioDscpToCosEntry 1 }

prioDscpToCosPHBValue OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The PHB value of internal QoS label."
    ::= { prioDscpToCosEntry 2 }

prioDscpToCosDropPrecedenceValue OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    green(0),
                    red(1),
                    yellow(3)
                }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The drop precedence value of internal QoS label. Green(0), Yellow(3),
         Red(1)."
    ::= { prioDscpToCosEntry 3 }

prioDscpToCosCFICosValue OBJECT-TYPE
    SYNTAX      Integer32 (0..15)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The remarked CFI and CoS value mapped from the internal Qos label
         value when the packet leaves the device. The egress remarked CFI value
         equals (prioDscpToCosCFICosValue right-shift 3) and the egress
         remarked CoS value equals (prioDscpToCosCFICosValue bitwise-and '7'h)."
    ::= { prioDscpToCosEntry 4 }

-- The mapping table for packet priority to drop precedence mapping.

prioPrioToDropPrecTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PrioPrioToDropPrecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for packet priority to drop precedence mapping."
    ::= { cosMgt 8 }

prioPrioToDropPrecEntry OBJECT-TYPE
    SYNTAX      PrioPrioToDropPrecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for packet priority to drop precedence mapping."
    INDEX
    {
        prioPrioToDropPrecIfValue,
        prioPrioToDropPrecPriorityValue
    }
    ::= { prioPrioToDropPrecTable 1 }

PrioPrioToDropPrecEntry ::= SEQUENCE
{
    prioPrioToDropPrecIfValue       Integer32,
    prioPrioToDropPrecPriorityValue Integer32,
    prioPrioToDropPrecPrecValue     INTEGER
}

prioPrioToDropPrecIfValue OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The port or the trunk interface of the device. The interface
         identified by a particular value of this index is the same interface
         as identified by the same value of ifIndex in the IF-MIB."
    ::= { prioPrioToDropPrecEntry 1 }


prioPrioToDropPrecPriorityValue OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of packet default priority."
    ::= { prioPrioToDropPrecEntry 2 }

prioPrioToDropPrecPrecValue OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    green(0),
                    red(1),
                    yellow(3)
                }

    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "The drop precedence value of internal QoS label. Green(0), Yellow(3),
         Red(1)."
    ::= { prioPrioToDropPrecEntry 3 }

-- The mapping table from PHB to queue
--

prioDscpToQueueTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PrioDscpToQueueEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for PHB to queue mapping."
    ::= { cosMgt 9 }

prioDscpToQueueEntry OBJECT-TYPE
    SYNTAX      PrioDscpToQueueEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry for PHB to queue mapping."
    INDEX
    {
        prioDscpToQueueIfValue,
        prioDscpToQueuePHBValue
    }
    ::= { prioDscpToQueueTable 1 }

PrioDscpToQueueEntry ::= SEQUENCE
{
    prioDscpToQueueIfValue      Integer32,
    prioDscpToQueuePHBValue     Integer32,
    prioDscpToQueueQueueValue   Integer32
}

prioDscpToQueueIfValue OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The port or trunk interface of the device. The interface identified by
         a particular value of this index is the same interface as identified
         by the same value of ifIndex in the IF-MIB."
    ::= { prioDscpToQueueEntry 1 }

prioDscpToQueuePHBValue OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The PHB value of internal QoS label."
    ::= { prioDscpToQueueEntry 2 }

prioDscpToQueueQueueValue OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The queue value which is mapped from the PHB value of QoS label."
    ::= { prioDscpToQueueEntry 3 }

--
--diffServMgt
--

diffServMgt    OBJECT IDENTIFIER ::= { qosMgt 4 }

diffServPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DiffServPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for differentiated services on each port."
        ::= { diffServMgt 9 }

diffServPortEntry OBJECT-TYPE
        SYNTAX      DiffServPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for differentiated services on each port."
        INDEX       { diffServPortIfIndex }
        ::= { diffServPortTable 1 }

DiffServPortEntry ::= SEQUENCE
{
    diffServPortIfIndex             Integer32,
    diffServPortPolicyMapIndex      Integer32,
    diffServPortIngressIpAclIndex   Integer32,
    diffServPortIngressMacAclIndex  Integer32,
    diffServPortIngressIpv6AclIndex Integer32
}

diffServPortIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This object is the interface index of diffServPortEntry.
                     The interface identified by a particular value of this
                     index is the same interface as identified by the same
                     value of ifIndex in the IF-MIB."
        ::= { diffServPortEntry 1 }

diffServPortPolicyMapIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the policy map binding to the interface. The policy
                 map identified by a particular value of this index is
                 associated with the same DiffServPolicyMapEntry as identified
                 by the same value of diffServPolicyMapIndex."
    ::= { diffServPortEntry 2 }

diffServPortIngressIpAclIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the ingress IP ACL binding to the interface. The
                 ingress IP ACL identified by a particular value of this index
                 is associated with the same diffServAclEntry as identified by
                 the same value of diffServAclIndex."
    ::= { diffServPortEntry 3 }

diffServPortIngressMacAclIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the ingress MAC ACL binding to the interface. The
                 ingress MAC ACL identified by a particular value of this
                 index is associated with the same diffServAclEntry as
                 identified by the same value of diffServAclIndex."
    ::= { diffServPortEntry 4 }

diffServPortIngressIpv6AclIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the ingress IPv6 ACL binding to the interface. The
                 ingress IPv6 ACL identified by a particular value of this
                 index is associated with the same diffServAclEntry as
                 identified by the same value of diffServAclIndex."
    ::= { diffServPortEntry 5 }

diffServPolicyMapTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DiffServPolicyMapEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for policy map."
        ::= { diffServMgt 10 }

diffServPolicyMapEntry OBJECT-TYPE
        SYNTAX      DiffServPolicyMapEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for policy map."
        INDEX       { diffServPolicyMapIndex }
        ::= { diffServPolicyMapTable 1 }

DiffServPolicyMapEntry ::= SEQUENCE
{
    diffServPolicyMapIndex              Integer32,
    diffServPolicyMapName               DisplayString,
    diffServPolicyMapDescription        DisplayString,
    diffServPolicyMapElementIndexList   OCTET STRING,
    diffServPolicyMapStatus             RowStatus
}

diffServPolicyMapIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An index that uniquely identifies an entry in this table."
        ::= { diffServPolicyMapEntry 1 }

diffServPolicyMapName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (1..16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The name of this entry."
    ::= { diffServPolicyMapEntry 2 }

diffServPolicyMapDescription OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The description of this entry."
    ::= { diffServPolicyMapEntry 3 }

diffServPolicyMapElementIndexList OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The octet string containes the diffServPolicyMapElementEntry
                 indexes. Two octets express one index and it is represented
                 in network order. This index list indicates the
                 diffServPolicyMapEntrys which belong to this entry."
    ::= { diffServPolicyMapEntry 4 }

diffServPolicyMapStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "This object is used to create a new row, or modify or delete
                 an existing row, in this table. The status column has six
                 defined values:
                 The status column has six defined values:

                      - 'active', which indicates that the conceptual row is
                      available for use by the managed device;

                      - 'notInService', which indicates that the conceptual
                      row exists in the agent, but is unavailable for use by
                      the managed device (see NOTE below);

                      - 'notReady', which indicates that the conceptual row
                      exists in the agent, but is missing information
                      necessary in order to be available for use by the
                      managed device;

                      - 'createAndGo', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row and to have its status automatically set
                      to active, making it available for use by the managed
                      device;

                      - 'createAndWait', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row (but not make it available for use by
                      the managed device); and,

                      - 'destroy', which is supplied by a management station
                      wishing to delete all of the instances associated with
                      an existing conceptual row.

                 Whereas five of the six values (all except 'notReady') may
                 be specified in a management protocol set operation, only
                 three values will be returned in response to a management
                 protocol retrieval operation:  'notReady', 'notInService' or
                 'active'.  That is, when queried, an existing conceptual row
                 has only three states:  it is either available for use by
                 the managed device (the status column has the value
                 'active');it is not available for use by the managed device,
                 though the agent has sufficient information to make it so
                 (the status column has the value 'notInService'); or, it is
                 not available for use by the managed device, and an attempt
                 to make it so would fail because the agent has insufficient
                 information (the state column has the value 'notReady').

                 For a detailed description of this object, please refer to
                 SNMPv2-TC MIB."
    ::= { diffServPolicyMapEntry 5 }

diffServPolicyMapAttachCtl  OBJECT IDENTIFIER   ::= { diffServMgt 11 }

diffServPolicyMapAttachCtlIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Index for attachment control.
                     Specifies the policy map as the target to relate with
                     the policy map element. The policy map identified by
                     a particular value of this index is associated with
                     the same diffServPolicyMapEntry as identified by the
                     same value of diffServPolicyMapIndex."
        ::= { diffServPolicyMapAttachCtl 1 }

diffServPolicyMapAttachCtlElementIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Element Index for attachment control. Specifies the policy map
                 element to relate with the policy map. The policy map element
                 identified by a particular value of this index is associated
                 with the same diffServPolicyMapElementEntry as identified by
                 the same value of diffServPolicyMapElementIndex."
    ::= { diffServPolicyMapAttachCtl 2 }

diffServPolicyMapAttachCtlAction OBJECT-TYPE
    SYNTAX      INTEGER
                    {
                        noAction(1),
                        attach(2),
                        detach(3)
                    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Action for attachment control. When setting this object to
                 attach(2) to begin the attaching operation, a particular
                 policy map element is attached to a particular policy map.
                 When setting this object to detach(3) to begin the not
                 attached operation, a particular policy map element is not
                 attached to a particular policy map. When the action is
                 finshed or no action is taken, the value of this object is
                 noAction(1). A particular policy map is specified in the
                 diffServPolicyMapAttachCtlIndex. A particularpolicy map
                 element is specified in the
                 diffServPolicyMapAttachCtlElementIndex."
    ::= { diffServPolicyMapAttachCtl 3 }

diffServPolicyMapElementTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DiffServPolicyMapElementEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for policy map element."
        ::= { diffServMgt 12 }

diffServPolicyMapElementEntry OBJECT-TYPE
        SYNTAX      DiffServPolicyMapElementEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for policy map element."
        INDEX       { diffServPolicyMapElementIndex }
        ::= { diffServPolicyMapElementTable 1 }

DiffServPolicyMapElementEntry ::= SEQUENCE
{
    diffServPolicyMapElementIndex           Integer32,
    diffServPolicyMapElementClassMapIndex   Integer32,
    diffServPolicyMapElementMeterIndex      Integer32,
    diffServPolicyMapElementActionIndex     Integer32,
    diffServPolicyMapElementStatus          RowStatus
}

diffServPolicyMapElementIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An index that uniquely identifies an entry in this table."
        ::= { diffServPolicyMapElementEntry 1 }

diffServPolicyMapElementClassMapIndex OBJECT-TYPE
    SYNTAX      Integer32(1..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Specifies the class map binding to this entry. The class map
                 identified by a particular value of this index is associated
                 with the same diffServClassMapEntry as identified by the same
                 value of diffServClassMapIndex."
    ::= { diffServPolicyMapElementEntry 2 }

diffServPolicyMapElementMeterIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Specifies the meter binding to this entry. The meter
                 identified by a particular value of this index is associated
                 with the same diffServMeterEntry as identified by the same
                 value of diffServMeterIndex. If this value is
                 zero, no associated meter will be associated, as zero is not a
                 valid meter index."
    ::= { diffServPolicyMapElementEntry 3 }

diffServPolicyMapElementActionIndex OBJECT-TYPE
    SYNTAX      Integer32(1..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Specifies the action binding to this entry. The action
                 identified by a particular value of this index is associated
                 with the same diffServActionEntry as identified by the same
                 value of diffServActionIndex."
    ::= { diffServPolicyMapElementEntry 4 }

diffServPolicyMapElementStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "This object is used to create a new row, or modify or delete
                 an existing row, in this table. The status column has six
                 defined values:

                 The status column has six defined values:

                      - 'active', which indicates that the conceptual row is
                      available for use by the managed device;

                      - 'notInService', which indicates that the conceptual
                      row exists in the agent, but is unavailable for use by
                      the managed device (see NOTE below);

                      - 'notReady', which indicates that the conceptual row
                      exists in the agent, but is missing information
                      necessary in order to be available for use by the
                      managed device;

                      - 'createAndGo', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row and to have its status automatically set
                      to active, making it available for use by the managed
                      device;

                      - 'createAndWait', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row (but not make it available for use by
                      the managed device); and,

                      - 'destroy', which is supplied by a management station
                      wishing to delete all of the instances associated with
                      an existing conceptual row.

                 Whereas five of the six values (all except 'notReady') may
                 be specified in a management protocol set operation, only
                 three values will be returned in response to a management
                 protocol retrieval operation:  'notReady', 'notInService' or
                 'active'.  That is, when queried, an existing conceptual row
                 has only three states:  it is either available for use by
                 the managed device (the status column has the value
                 'active'); it is not available for use by the managed device,
                 though the agent has sufficient information to make it so
                 (the status column has the value 'notInService'); or, it is
                 not available for use by the managed device, and an attempt
                 to make it so would fail because the agent has insufficient
                 information (the state column has the value 'notReady').

                 For a detailed description of this object, please refer to
                 SNMPv2-TC MIB."
    ::= { diffServPolicyMapElementEntry 5 }

diffServClassMapTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DiffServClassMapEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for class map."
        ::= { diffServMgt 13 }

diffServClassMapEntry OBJECT-TYPE
        SYNTAX      DiffServClassMapEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for class map."
        INDEX       { diffServClassMapIndex }
        ::= { diffServClassMapTable 1 }

DiffServClassMapEntry ::= SEQUENCE
{
    diffServClassMapIndex                Integer32,
    diffServClassMapName                 DisplayString,
    diffServClassMapDescription          DisplayString,
    diffServClassMapMatchType            INTEGER,
    diffServClassMapElementIndexTypeList OCTET STRING,
    diffServClassMapElementIndexList     OCTET STRING,
    diffServClassMapStatus               RowStatus
}

diffServClassMapIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An index that uniquely identifies an entry in this table."
        ::= { diffServClassMapEntry 1 }

diffServClassMapName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The name of this entry."
    ::= { diffServClassMapEntry 2 }

diffServClassMapDescription OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The description of this entry."
    ::= { diffServClassMapEntry 3 }

diffServClassMapMatchType OBJECT-TYPE
    SYNTAX       INTEGER {
                     matchAny(1),
                     matchAll(2)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The map match type of this entry."
    ::= { diffServClassMapEntry 4 }

diffServClassMapElementIndexTypeList OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The octet string containes the type of class map element
                 indexes. Two octets which are represented in network order
                 express one type of the class map element index in network
                 order and it maps the index of
                 differServClasssMapElementIndexList in order. When the type is
                 macAce(1), the maping index of
                 differServClasssMapElementIndexList is the
                 diffServMacAceEntry. When the type is ipAce(2), the maping
                 index of differServClasssMapElementIndexList is the
                 diffServIpAceEntry. When the type is acl(3), the maping index
                 of differServClasssMapElementIndexList is the diffServAclEntry."
    ::= { diffServClassMapEntry 5 }

diffServClassMapElementIndexList OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The octet string containes the class map element indexes. Two
                 octets express one index and it is represented in
                 network order. This index list indicates the particular
                 class map elements which belong to this table. The class map
                 element uses type to indicate diffServAclEntry, the
                 diffServIpAceEntry or diffServMacAceEntry. The type is two
                 octet specified in differServClasssMapElementIndexTypeList
                 in order. When the type is macAce(1), the maping index of
                 differServClasssMapElementIndexList is the
                 diffServMacAceEntry. When the type is ipAce(2), the maping
                 index of differServClasssMapElementIndexList is the
                 diffServIpAceEntry. When the type is acl(3), the maping index
                 of differServClasssMapElementIndexList is the diffServAclEntry."
    ::= { diffServClassMapEntry 6 }

diffServClassMapStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "This object is used to create a new row or modify or delete
                 an existing row in this table.The status column has six
                 defined values:

                 The status column has six defined values:

                      - 'active', which indicates that the conceptual row is
                      available for use by the managed device;

                      - 'notInService', which indicates that the conceptual
                      row exists in the agent, but is unavailable for use by
                      the managed device (see NOTE below);

                      - 'notReady', which indicates that the conceptual row
                      exists in the agent, but is missing information
                      necessary in order to be available for use by the
                      managed device;

                      - 'createAndGo', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row and to have its status automatically set
                      to active, making it available for use by the managed
                      device;

                      - 'createAndWait', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row (but not make it available for use by
                      the managed device); and,

                      - 'destroy', which is supplied by a management station
                      wishing to delete all of the instances associated with
                      an existing conceptual row.

                 Whereas five of the six values (all except 'notReady') may
                 be specified in a management protocol set operation, only
                 three values will be returned in response to a management
                 protocol retrieval operation:  'notReady', 'notInService' or
                 'active'.  That is, when queried, an existing conceptual row
                 has only three states:  it is either available for use by
                 the managed device (the status column has the value
                 'active'); it is not available for use by the managed device,
                 though the agent has sufficient information to make it so
                 (the status column has the value 'notInService'); or, it is
                 not available for use by the managed device, and an attempt
                 to make it so would fail because the agent has insufficient
                 information (the state column has the value 'notReady').

                 For a detailed description of this object, please refer to
                 SNMPv2-TC MIB."
    ::= { diffServClassMapEntry 7 }

diffServClassMapAttachCtl  OBJECT IDENTIFIER   ::= { diffServMgt 14 }

diffServClassMapAttachCtlIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Index for attachment control. Specifies the class map as
                     the target to relate with class map elements. The class
                     map identified by a particular value of this index is
                     associated with the same diffServClassMapEntry as
                     identified by the same value of diffServClassMapIndex."
        ::= { diffServClassMapAttachCtl 1 }

diffServClassMapAttachCtlElementIndexType OBJECT-TYPE
    SYNTAX    INTEGER {
                     macAce(1),
                     ipAce(2),
                     acl(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Element Index for attachment control. Specifies the type of
                 class map element to relate with the class map. When type is
                 macAce(1), the index of diffServClassMapAttachCtlElementIndex
                 is the index of diffServMacAceEntry. When the type is
                 ipAce(2), the index of diffServClassMapAttachCtlElementIndex
                 is the index of diffServIpAceEntry. When the type is acl(3),
                 the index of diffServClassMapAttachCtlElementIndex is the
                 index of diffServAclEntry."
    ::= { diffServClassMapAttachCtl 2 }

diffServClassMapAttachCtlElementIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Element Index for attachment control. Specifies the class map
                 element related with the class map. The class map element uses
                 type to indicate diffServAclEntry, the diffServIpAceEntry or
                 diffServMacAceEntry. The type is specified in
                 diffServClassMapAttachCtlElementIndexType. When
                 the type is macAce(1), the maping index of
                 differServClasssMapElementIndexList is the
                 diffServMacAceEntry. When the type is ipAce(2), the maping
                 index of differServClasssMapElementIndexList is the
                 diffServIpAceEntry. When the type is acl(3), the maping index
                 of differServClasssMapElementIndexList is the
                 diffServAclEntry."
    ::= { diffServClassMapAttachCtl 3 }

diffServClassMapAttachCtlAction OBJECT-TYPE
    SYNTAX      INTEGER
                    {
                        noAction(1),
                        attach(2),
                        detach(3)
                    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Action for attachment control. When setting this object to
                 attach(2) to begin the attaching operation, a particular class
                 map element is attached to a particular class map. When
                 setting this object to detach(3) to begin the not attached
                 operation, then a particular class map element is not attached
                 to a particular class map. When the action is finshed whether
                 successfully or not, or no action is taken, the value of this
                 object always is noAction(1). The value of a particular class
                 map is specified in the AclAttachCtlTargetIndex. The class map
                 element is specified by diffServClassMapAttachCtlElementIndexType
                 and diffServClassMapAttachCtlElementIndex."
    ::= { diffServClassMapAttachCtl 4 }

diffServAclTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DiffServAclEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for ACL."
        ::= { diffServMgt 15 }

diffServAclEntry OBJECT-TYPE
        SYNTAX      DiffServAclEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for ACL."
        INDEX       { diffServAclIndex }
        ::= { diffServAclTable 1 }

DiffServAclEntry ::= SEQUENCE
{
    diffServAclIndex        Integer32,
    diffServAclName         DisplayString,
    diffServAclType         INTEGER,
    diffServAclAceIndexList OCTET STRING,
    diffServAclStatus       RowStatus
}

diffServAclIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An index that uniquely identifies an entry in the ACL
                     table."
        ::= { diffServAclEntry 1 }

diffServAclName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (1..16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The name of this entry."
    ::= { diffServAclEntry 2 }

diffServAclType OBJECT-TYPE
    SYNTAX      INTEGER {
                    mac(1),
                    ipstandard(2),
                    ipextended(3),
                    ipv6standard(4),
                    ipv6extended(5),
                    arp(6)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The type of this entry. When the value of ACL type is
                 modified, then the ACEs in the diffServAclAceIndexList of
                 this entry will be auto-removed, and this entry will be auto-
                 unbound from the diffServPortTable and the
                 diffServClassMapTable."
    ::= { diffServAclEntry 3 }

diffServAclAceIndexList OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The octet string containes the ACE indexes. Two octets
                 express one index and it is represented in network
                 order. This index list indicates the particular ACEs which
                 belong to this table. The ACE uses type to indicate the
                 diffServMacAceEntry, the diffServIpAceEntry, the
                 diffServIpv6AceEntry or the diffServArpAceEntry. The type is
                 specified in diffServAclType. When the type is mac(1), the
                 index of diffServAclAceIndexList is the diffServMacAceEntry.
                 When the type is ipstandard(2) or ipextended(3), the index of
                 diffServAclAceIndexList is the diffServIpAceEntry. When the
                 type is ipv6standard(4) or ipv6extended(5), the index of
                 diffServAclAceIndexList is the diffServIpv6AceEntry. When the
                 type is arp(6), the index of diffServAclAceIndexList is the
                 diffServArpAceEntry."
    ::= { diffServAclEntry 4 }

diffServAclStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "This object is used to create a new row or modify or delete
                 an existing row in this table. The status column has six
                 defined values:

                      - 'active', which indicates that the conceptual row is
                      available for use by the managed device;

                      - 'notInService', which indicates that the conceptual
                      row exists in the agent, but is unavailable for use by
                      the managed device (see NOTE below);

                      - 'notReady', which indicates that the conceptual row
                      exists in the agent, but is missing information
                      necessary in order to be available for use by the
                      managed device;

                      - 'createAndGo', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row and to have its status automatically set
                      to active, making it available for use by the managed
                      device;

                      - 'createAndWait', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row (but not make it available for use by
                      the managed device); and,

                      - 'destroy', which is supplied by a management station
                      wishing to delete all of the instances associated with
                      an existing conceptual row.

                 Whereas five of the six values (all except 'notReady') may
                 be specified in a management protocol set operation, only
                 three values will be returned in response to a management
                 protocol retrieval operation:  'notReady', 'notInService' or
                 'active'.  That is, when queried, an existing conceptual row
                 has only three states:  it is either available for use by
                 the managed device (the status column has the value
                 'active'); it is not available for use by the managed device,
                 though the agent has sufficient information to make it so
                 (the status column has the value 'notInService'); or, it is
                 not available for use by the managed device, and an attempt
                 to make it so would fail because the agent has insufficient
                 information (the state column has the value 'notReady').

                 For a detailed description of this object, please refer to
                 SNMPv2-TC MIB."
    ::= { diffServAclEntry 5 }

diffServAclAttachCtl  OBJECT IDENTIFIER   ::= { diffServMgt 16 }

diffServAclAttachCtlIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Index for attachment control. Specifies the ACL as the
                     target to relate with the IP ACE, the MAC ACE or IPv6 ACE.
                     The ACL identified by a particular value of this index  is
                     associated with the same diffServAclEntry as identified by
                     the same value of diffServAclIndex."
        ::= { diffServAclAttachCtl 1 }

diffServAclAttachCtlAceType OBJECT-TYPE
        SYNTAX  INTEGER
                {
                    macAce(1),
                    ipAce(2),
                    ipv6Ace(3),
                    arpAce(4)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Type for attachment control. Specifies the type of
                 diffServAclAttachCtlAceIndex to relate with the
                 diffServAclAttachCtlIndex. When the type is macAce(1), the
                 index of diffServAclAceIndexList is the diffServMacAceEntry.
                 When the type is ipAce(2), the index of
                 diffServAclAceIndexList is the diffServIpAceEntry. When the
                 type is ipv6Ace(3), the index of diffServAclAceIndexList
                 is the diffServIpv6AceEntry. When the type is arpAce(4), the
                 index of diffServAclAceIndexList is the diffServArpAceEntry."
    ::= { diffServAclAttachCtl 2 }

diffServAclAttachCtlAceIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Index for attachment control. Specifies the ACE to relate with
                 the diffServAclAttachCtlIndex. When
                 diffServAclAttachCtlAceType is macAce(1), the value of
                 diffServAclAttachCtlIndex is the diffServMacAceEntry. When
                 diffServAclAttachCtlAceType is ipAce(2), the value of
                 diffServAclAttachCtlIndex is the diffServIpAceEntry. When
                 diffServAclAttachCtlAceType is ipv6Ace(3), the value of
                 diffServAclAttachCtlIndex is the diffServIpv6AceEntry. When
                 diffServAclAttachCtlAceType is arpAce(4), the value of
                 diffServAclAttachCtlIndex is the diffServArpAceEntry."
    ::= { diffServAclAttachCtl 3 }

diffServAclAttachCtlAction OBJECT-TYPE
    SYNTAX      INTEGER
                    {
                        noAction(1),
                        attach(2),
                        detach(3)
                    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Action for attachment control. When setting this object to
                 attach(2) to begin the attaching operation, a particular ACE
                 is attached to a particular ACL. When setting this object to
                 detach(3) to begin the not attached operation, then a
                 particular ACE is not attached to a particular ACL. When the
                 action is finshed whether successfully or not, or no action
                 is taken, the value of this object always is noAction(1), The
                 value of a particular ACL is specified in the
                 diffServAclAttachCtlAceType and diffServAclAttachCtlAceIndex."
    ::= { diffServAclAttachCtl 4 }

diffServIpAceTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DiffServIpAceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for IP ACE."
        ::= { diffServMgt 17 }

diffServIpAceEntry OBJECT-TYPE
        SYNTAX      DiffServIpAceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for IP ACE."
        INDEX       { diffServIpAceIndex }
        ::= { diffServIpAceTable 1 }

DiffServIpAceEntry ::= SEQUENCE
{
    diffServIpAceIndex                  Integer32,
    diffServIpAceType                   INTEGER,
    diffServIpAceAccess                 INTEGER,
    diffServIpAceSourceIpAddr           IpAddress,
    diffServIpAceSourceIpAddrBitmask    IpAddress,
    diffServIpAceDestIpAddr             IpAddress,
    diffServIpAceDestIpAddrBitmask      IpAddress,
    diffServIpAceProtocol               Integer32,
    diffServIpAcePrec                   Integer32,
    diffServIpAceTos                    Integer32,
    diffServIpAceDscp                   Integer32,
    diffServIpAceSourcePortOp           INTEGER,
    diffServIpAceMinSourcePort          Integer32,
    diffServIpAceSourcePortBitmask      Integer32,
    diffServIpAceDestPortOp             INTEGER,
    diffServIpAceMinDestPort            Integer32,
    diffServIpAceDestPortBitmask        Integer32,
    diffServIpAceControlCode            Integer32,
    diffServIpAceControlCodeBitmask     Integer32,
    diffServIpAceStatus                 RowStatus,
    diffServIpAceIfIndex                Integer32,
    diffServIpAceTimeRange              DisplayString
}

diffServIpAceIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An index that uniquely identifies an entry in the IP ACE
                     table."
        ::= { diffServIpAceEntry 1 }

diffServIpAceType OBJECT-TYPE
    SYNTAX  INTEGER {
      standard(1),
      extended(2)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The specified IP ACE type. When the type of this entry is
                 modified, then this entry will be auto-unbound from the
                 diffServAclEntry and the not supporting field of this entry
                 will be set 0."
    ::= { diffServIpAceEntry 2 }

diffServIpAceAccess OBJECT-TYPE
    SYNTAX  INTEGER {
        permit(1),
        deny(2),
        redirect(3)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates the action to be taken if a packet matches this
                 ACE."
    ::= { diffServIpAceEntry 3 }

diffServIpAceSourceIpAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The specified source IP address. The packet's source address
                 is AND-ed with the value of IpAceSourceIpAddrBitmask and then
                 compared against the value of this object."
    ::= { diffServIpAceEntry 4 }

diffServIpAceSourceIpAddrBitmask OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The specified source IP address mask. The packet's source
                 address is AND-ed with the value of IpAceSourceIpAddr and
                 then compared against the value of this object."
    ::= { diffServIpAceEntry 5 }

diffServIpAceDestIpAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The specified destination IP address. The packet's
                 destination address is AND-ed with the value of
                 diffServIpAceDestIpAddrBitmask and then compared against the
                 value of this object. This object may not be modified if the
                 associated diffServIpAceType object is equal to standard(1)."
    ::= { diffServIpAceEntry 6 }

diffServIpAceDestIpAddrBitmask OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The specified destination IP address mask. This object may
                     not be modified if the associated diffServIpAceType object
                     is equal to standard(1)."
        ::= { diffServIpAceEntry 7 }

diffServIpAceProtocol OBJECT-TYPE
    SYNTAX      Integer32 (0..256)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The protocol number field in the IP header used to indicate
                 the higher layer protocol as specified in RFC 1700. A value
                 of 0 matches every IP packet. The object=256 means 'any'. For
                 example: 0 is IP, 1 is ICMP, 2 is IGMP, 4 is IP in IP
                 encapsulation, 6 is TCP, 9 is IGRP, 17 is UDP, 47 is GRE, 50
                 is ESP, 51 is AH, 88 is IGRP, 89 is OSPF, 94 is KA9Q/NOS
                 compatible IP over IP, 103 is PIMv2, 108 is PCP. This object
                 may not be modified if the associated diffServIpAceType object
                 is equal to standard(1)."
    ::= { diffServIpAceEntry 8 }

diffServIpAcePrec OBJECT-TYPE
    SYNTAX      Integer32 (0..8)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Specifies the IP precedence value to match against. The value
                 of this object is ignored whenever the value of
                 diffServIpAcePrec object is 8. This object may not be modified
                 if the associated diffServIpAceType object is equal to
                 standard(1)."
    ::= { diffServIpAceEntry 9 }

diffServIpAceTos OBJECT-TYPE
    SYNTAX      Integer32 (0..16)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Specifies the IP ToS facility value to match against. The
                 value of this object is ignored whenever the value of
                 diffServIpAcePrec object is 9. This object may not be modified
                 if the associated diffServIpAceType object is equal to
                 standard(1)."
    ::= { diffServIpAceEntry 10 }

diffServIpAceDscp OBJECT-TYPE
    SYNTAX      Integer32 (0..64)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Specifies the DSCP value to match against. The value of this
                 object is ignored whenever the value of diffServIpAcePrec
                 object is 64. This object may not be modified if the
                 associated diffServIpAceType object is equal to standard(1)."
    ::= { diffServIpAceEntry 11 }

diffServIpAceSourcePortOp OBJECT-TYPE
    SYNTAX  INTEGER {
                noOperator(1),
                equal(2),
                range(3)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates how a packet's source TCP/UDP port number is to be
                 compared. noOperator(1), which is the default value, means no
                 comparison is to be made with the source TCP/UDP port
                 number. equal(2), which is used the
                 diffServIpAceSourcePortBitmask and the
                 diffServIpAceMinSourcePort to match against. range(3),which is
                 used the diffServIpAceMinSourcePort and the
                 diffServIpAceMaxSourcePort to match against. This object may
                 not be modified if the associated diffServIpAceType object is
                 equal to standard(1)."
    ::= { diffServIpAceEntry 12 }

diffServIpAceMinSourcePort OBJECT-TYPE
        SYNTAX      Integer32 (0..'FFFF'h)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "If the diffServIpAceSourcePortOp is range(3), this
                     indicates the lower bound of the TCP/UDP port number
                     value range. This object may not be modified if the
                     associated diffServIpAceType object is equal to
                     standard(1)."
        ::= { diffServIpAceEntry 13 }

diffServIpAceSourcePortBitmask OBJECT-TYPE
    SYNTAX      Integer32 (0..'FFFF'h)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "If the diffServIpAceSourcePortOp is equal(2), this indicates
                 the bitmask of the diffServIpAceMinSourcePort. This object may
                 not be modified if the associated diffServIpAceType object is
                 equal to standard(1)."
    ::= { diffServIpAceEntry 15 }

diffServIpAceDestPortOp OBJECT-TYPE
    SYNTAX      INTEGER{
                noOperator(1),
                equal(2),
                range(3)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates how a packet's destination TCP/UDP port number is
                 to be compared. noOperator(1), which is the default value,
                 means that no comparison is to be made with the destination
                 TCP/UDP port number. equal(2), which is used the
                 diffServIpAceSourcePortBitmask and the
                 diffServIpAceMinDestPort to match against. range(3),which is
                 used the diffServIpAceMinDestPort and the
                 diffServIpAceMaxDestPort to match against. This object may not
                 be modified if the associated diffServIpAceType object is
                 equal to standard(1)."
    ::= { diffServIpAceEntry 16 }

diffServIpAceMinDestPort OBJECT-TYPE
    SYNTAX      Integer32 (0..'FFFF'h)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "If the diffServIpAceDestPortOp is range(3), this indicates
                 the lower bound of the TCP/UDP port number value range. This
                 object may not be modified if the associated
                 diffServIpAceType object is equal to standard(1)."
    ::= { diffServIpAceEntry 17 }

diffServIpAceDestPortBitmask OBJECT-TYPE
    SYNTAX      Integer32 (0..'FFFF'h)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "If the diffServIpAceDestPortOp is equal(2), this indicates
                 the bitmask of the diffServIpAceMinDestPort. This object may
                 not be modified if the associated diffServIpAceType object
                 is equal to standard(1)."
    ::= { diffServIpAceEntry 19 }

diffServIpAceControlCode OBJECT-TYPE
    SYNTAX      Integer32 (0..63)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates how the control flags of TCP packets are to be
                 compared. diffServIpAceControlCode is AND-ed with
                 diffServIpAceControlCodeBitmask. This object may not be
                 modified if the associated diffServIpAceType object is
                 equal to standard(1)."
    ::= { diffServIpAceEntry 20 }

diffServIpAceControlCodeBitmask OBJECT-TYPE
    SYNTAX      Integer32 (0..63)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates how the control flags of TCP packets are to be
                 compared. It can be used to check multiple flags of the FIN,
                 SYN, RST, PSH, ACK, URG by the sum of FIN=1, SYN=2, RST=4,
                 PSH=8, ACK=16, URG=32. This object may not be modified if the
                 associated diffServIpAceType object is equal to standard(1)."
    ::= { diffServIpAceEntry 21 }

diffServIpAceStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "This object is used to create a new row or modify or delete
                 an existing row in this table. The status column has six
                 defined values:

                 The status column has six defined values:

                      - 'active', which indicates that the conceptual row is
                      available for use by the managed device;

                      - 'notInService', which indicates that the conceptual
                      row exists in the agent, but is unavailable for use by
                      the managed device (see NOTE below);

                      - 'notReady', which indicates that the conceptual row
                      exists in the agent, but is missing information
                      necessary in order to be available for use by the
                      managed device;

                      - 'createAndGo', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row and to have its status automatically set
                      to active, making it available for use by the managed
                      device;

                      - 'createAndWait', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row (but not make it available for use by
                      the managed device); and,

                      - 'destroy', which is supplied by a management station
                      wishing to delete all of the instances associated with
                      an existing conceptual row.

                 Whereas five of the six values (all except 'notReady') may
                 be specified in a management protocol set operation, only
                 three values will be returned in response to a management
                 protocol retrieval operation:  'notReady', 'notInService' or
                 'active'.  That is, when queried, an existing conceptual row
                 has only three states:  it is either available for use by
                 the managed device (the status column has the value
                 'active'); it is not available for use by the managed device,
                 though the agent has sufficient information to make it so
                 (the status column has the value 'notInService'); or, it is
                 not available for use by the managed device, and an attempt
                 to make it so would fail because the agent has insufficient
                 information (the state column has the value 'notReady').

                 For a detailed description of this object, please refer to
                 SNMPv2-TC MIB."
    ::= { diffServIpAceEntry 22 }

diffServIpAceIfIndex OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION  "Indicates this ace will redirect packet to which ifindex.
                      It only work when the value of diffServIpAceAccess is redirect(3)."
        ::= { diffServIpAceEntry 23 }

diffServIpAceTimeRange OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..16))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The name of the time range entry bound to the ACE.
                     This object should be equal to one of the timeRangeName
                     objects in timeRangeTable."
        ::= { diffServIpAceEntry 24 }

diffServMacAceTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DiffServMacAceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for MAC ACE."
        ::= { diffServMgt 18 }

diffServMacAceEntry OBJECT-TYPE
        SYNTAX      DiffServMacAceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for MAC ACE."
        INDEX       { diffServMacAceIndex }
        ::= { diffServMacAceTable 1 }

DiffServMacAceEntry ::= SEQUENCE
{
    diffServMacAceIndex                 Integer32,
    diffServMacAceAccess                INTEGER,
    diffServMacAcePktformat             INTEGER,
    diffServMacAceSourceMacAddr         MacAddress,
    diffServMacAceSourceMacAddrBitmask  MacAddress,
    diffServMacAceDestMacAddr           MacAddress,
    diffServMacAceDestMacAddrBitmask    MacAddress,
    diffServMacAceVidOp                 INTEGER,
    diffServMacAceMinVid                Integer32,
    diffServMacAceVidBitmask            Integer32,
    diffServMacAceEtherTypeOp           INTEGER,
    diffServMacAceEtherTypeBitmask      Integer32,
    diffServMacAceMinEtherType          Integer32,
    diffServMacAceCosOp                 INTEGER,
    diffServMacAceCosBitmask            INTEGER,
    diffServMacAceMinCos                INTEGER,
    diffServMacAceStatus                RowStatus,
    diffServMacAceIfIndex               Integer32,
    diffServMacAceTimeRange             DisplayString
}

diffServMacAceIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An index that uniquely identifies an entry in the MAC ACE
                     table."
        ::= { diffServMacAceEntry 1 }

diffServMacAceAccess OBJECT-TYPE
    SYNTAX      INTEGER 
    {
        permit(1),
        deny(2),
        redirect(3)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates the action to be taken if a packet matches this
                 ACE."
    ::= { diffServMacAceEntry 2 }

diffServMacAcePktformat OBJECT-TYPE
    SYNTAX      INTEGER 
    {
        any(1),
        untagged-Eth2(2),
        untagged802Dot3(3),
        tagggedEth2(4),
        tagged802Dot3(5)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Used to check the packet format of the packets. This object
                 cannot be configured when the status of the entry,
                 diffServMacAceStatus, is active(1)."
    ::= { diffServMacAceEntry 3 }

diffServMacAceSourceMacAddr OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates the 48-bit source MAC address. The specified source
                 MAC of the packet. The packet's source MAC address is AND-ed
                 with the value of diffServMacAceSourceMacAddrBitmask
                 and then compared against the value of this object."
    ::= { diffServMacAceEntry 4 }

diffServMacAceSourceMacAddrBitmask OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The specified source MAC address mask."
    ::= { diffServMacAceEntry 5 }

diffServMacAceDestMacAddr OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates the 48-bit destination MAC address. The specified
                 destination MAC of the packet. The packet's destination MAC
                 address is AND-ed with the value of
                 diffServMacAceDestMacAddrBitmask and then compared against
                 the value of this object."
    ::= { diffServMacAceEntry 6 }

diffServMacAceDestMacAddrBitmask OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The specified destination MAC address mask."
    ::= { diffServMacAceEntry 7 }

diffServMacAceVidOp OBJECT-TYPE
    SYNTAX      INTEGER 
    {
        noOperator(1),
        equal(2),
        range(3)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates how a packet's VID is to be compared. This
                 object cannot be configured when the status of the entry,
                 diffServMacAceStatus, is active(1)."
    ::= { diffServMacAceEntry 8 }

diffServMacAceMinVid OBJECT-TYPE
    SYNTAX      Integer32 (1..4094)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates the lower bound of the VID value range if the
                 diffServMacAceVidOp is range(3)."
    ::= { diffServMacAceEntry 9 }

diffServMacAceVidBitmask OBJECT-TYPE
    SYNTAX      Integer32 (0..'0FFF'h)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The bit mask of the VID. The default value is 0."
    DEFVAL     { 0 }
    ::= { diffServMacAceEntry 10 }

diffServMacAceEtherTypeOp OBJECT-TYPE
    SYNTAX    INTEGER {
        noOperator(1),
        equal(2),
        range(3)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates how a packet's ether type is to be compared."
    ::= { diffServMacAceEntry 12 }

diffServMacAceEtherTypeBitmask OBJECT-TYPE
    SYNTAX      Integer32 (0..'FFFF'h)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The bit mask of Ether type. The default value is 0."
    DEFVAL     { 0 }
    ::= { diffServMacAceEntry 13 }

diffServMacAceMinEtherType OBJECT-TYPE
        SYNTAX      Integer32 ('0000'h..'FFFF'h)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Indicates the lower bound of the ether type value range
                     if the diffServMacAceEtherTypeOp is range(3)."
        ::= { diffServMacAceEntry 14 }

diffServMacAceStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "This object is used to create a new row or modify or delete
                 an existing row in this table. The status column has six
                 defined values:

                 The status column has six defined values:

                      - 'active', which indicates that the conceptual row is
                      available for use by the managed device;

                      - 'notInService', which indicates that the conceptual
                      row exists in the agent, but is unavailable for use by
                      the managed device (see NOTE below);

                      - 'notReady', which indicates that the conceptual row
                      exists in the agent, but is missing information
                      necessary in order to be available for use by the
                      managed device;

                      - 'createAndGo', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row and to have its status automatically set
                      to active, making it available for use by the managed
                      device;

                      - 'createAndWait', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row (but not make it available for use by
                      the managed device); and,

                      - 'destroy', which is supplied by a management station
                      wishing to delete all of the instances associated with
                      an existing conceptual row.

                 Whereas five of the six values (all except 'notReady') may
                 be specified in a management protocol set operation, only
                 three values will be returned in response to a management
                 protocol retrieval operation:  'notReady', 'notInService' or
                 'active'.  That is, when queried, an existing conceptual row
                 has only three states:  it is either available for use by
                 the managed device (the status column has the value
                 'active'); it is not available for use by the managed device,
                 though the agent has sufficient information to make it so
                 (the status column has the value 'notInService'); or, it is
                 not available for use by the managed device, and an attempt
                 to make it so would fail because the agent has insufficient
                 information (the state column has the value 'notReady').

                 For a detailed description of this object, please refer to
                 SNMPv2-TC MIB."
    ::= { diffServMacAceEntry 16 }

diffServMacAceCosOp OBJECT-TYPE
    SYNTAX    INTEGER {
        noOperator(1),
        equal(2),
        range(3)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates how a packet's CoS is compared.
                 If the object type of diffServMacAceCosOp is equal(2),
                 diffServMacAceMinCos indicates the CoS value for comparing, and
                 diffServMacAceCosBitmask is used as the bitmask of the CoS value.
                 If the object type of diffServMacAceCosOp is range(3),
                 diffServMacAceMinCos should be used as the lower bound of the CoS value."

    ::= { diffServMacAceEntry 17 }

diffServMacAceCosBitmask OBJECT-TYPE
    SYNTAX      INTEGER ('0'h..'7'h)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates the bitmask of the CoS value if the object type of
                 diffServMacAceCosOp is equal(2). The default value is 0."
    ::= { diffServMacAceEntry 18 }

diffServMacAceMinCos OBJECT-TYPE
        SYNTAX      INTEGER ('0'h..'7'h)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "If the object type of diffServMacAceCosOp is equal(2),
                     diffServMacAceMinCos indicates the CoS value for comparing.
                     If the object type of diffServMacAceCosOp is range(3),
                     diffServMacAceMinCos indicates the lower bound of the CoS value."
    ::= { diffServMacAceEntry 19 }

diffServMacAceIfIndex OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION  "Indicates this ace will redirect packet to which ifindex.
                      It only work when the value of diffServMacAceAccess is redirect(3)."
        ::= { diffServMacAceEntry 27 }

diffServMacAceTimeRange OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..16))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The name of the time range entry bound to the ACE.
                     This object should be equal to one of the timeRangeName
                     objects in timeRangeTable."
        ::= { diffServMacAceEntry 28 }

diffServActionTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DiffServActionEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for action."
        ::= { diffServMgt 19 }

diffServActionEntry OBJECT-TYPE
        SYNTAX      DiffServActionEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for action."
        INDEX       { diffServActionIndex }
        ::= { diffServActionTable 1 }

DiffServActionEntry ::= SEQUENCE
{
    diffServActionIndex                 Integer32,
    diffServActionList                  BITS,
    diffServActionPktNewPri             Integer32,
    diffServActionPktPhb                Integer32,
    diffServActionGreenPktTransmit      EnabledStatus,
    diffServActionGreenPktNewDscp       Integer32,
    diffServActionYellowPktNewDscp      Integer32,  
    diffServActionYellowDrop            EnabledStatus,
    diffServActionRedPktNewDscp         Integer32,
    diffServActionRedDrop               EnabledStatus,
    diffServActionStatus                RowStatus
}

diffServActionIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An index that uniquely identifies an entry in the
                     action table."
        ::= { diffServActionEntry 1 }

diffServActionList OBJECT-TYPE
        SYNTAX      BITS
                    {
                        actionPktNewPri(0), 
                        reserved1(1),
                        actionGreenPktNewDscp(2),
                        actionRedPktNewDscp(3),
                        actionRedDrop(4),
                        actionYellowPktNewDscp(5), 
                        reserved6(6),   
                        actionYellowDrop(7),               
                        actionPktPhb(8), 
                        actionGreenPktTransmit(9)
                    }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The bitmap value used to identify which action
                     capabilities are enabled on the entry. The
                     actionPktNewPri and actionPktNewDscp can not be
                     enabled at the same time on the entry. The
                     actionRedPktNewDscp and actionRedDrop can not be
                     enabled at the same time on the entry."
        ::= { diffServActionEntry 2 }

diffServActionPktNewPri OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Specifies the new priority value for the packet when
                     the action is satisfied. If the actionPktNewPri bit of
                     the diffServActionList is not enabled, this object can
                     not be set."
        ::= { diffServActionEntry 3 }
        
diffServActionPktPhb OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Specifies the inner priority value for the packet when
                     the action is satisfied. If the actionPktPhb bit of
                     the diffServActionList is not enabled, this object can
                     not be set."
        ::= { diffServActionEntry 4 }    
        
diffServActionGreenPktTransmit OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The actionGreenPktTransmit bit of the
                     diffServActionList is for configuring this
                     object. If the value of this object is enabled, the
                     green marking packet will be Transmitted."
        ::= { diffServActionEntry 5 }

diffServActionGreenPktNewDscp OBJECT-TYPE
        SYNTAX      Integer32 (0..63)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Specifies the new DSCP value for the packet when
                     the action is satisfied. If the actionPktNewDscp bit of
                     the diffServActionList is not enabled, this object
                     can not be set."
        ::= { diffServActionEntry 6 }
        
diffServActionYellowPktNewDscp OBJECT-TYPE
        SYNTAX      Integer32 (0..63)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Specifies the new DSCP value for the packet when
                     the action is satisfied. The value of this object is ignored 
                     whenever the value of diffServActionYellowPktNewDscp object is 64. 
                     If the actionYellowPktNewDscp bit of the diffServActionList is 
                     not enabled, this object can not be set."
        ::= { diffServActionEntry 7 }        
        
diffServActionYellowDrop OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The actionYellowDrop bit of the
                     diffServActionList is for configuring this
                     object. If the value of this object is enabled, the
                     red marking packet will be dropped."
        ::= { diffServActionEntry 8 }

diffServActionRedPktNewDscp OBJECT-TYPE
        SYNTAX      Integer32 (0..63)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Specifies the new DSCP value for the red
                     marking packet when the action is satisfied. If the
                     actionRedPktNewDscp bit of the diffServActionList is
                     not enabled, this object can not be set."
        ::= { diffServActionEntry 9 }

diffServActionRedDrop OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The actionRedDrop bit of the
                     diffServActionList is for configuring this
                     object. If the value of this object is enabled, the
                     red marking packet will be dropped."
        ::= { diffServActionEntry 10 }

diffServActionStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "This object is used to create a new row, modify or
                     delete an existing row in this table.
                 The status column has six defined values:

                 The status column has six defined values:

                      - 'active', which indicates that the conceptual row
                         is available for use by the managed device;

                      - 'notInService', which indicates that the conceptual
                      row exists in the agent, but is unavailable for use
                      by the managed device (see NOTE below);

                      - 'notReady', which indicates that the conceptual row
                      exists in the agent, but is missing information
                      necessary in order to be available for use by the
                      managed device;

                      - 'createAndGo', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row and to have its status automatically
                      set to active, making it available for use by the
                      managed device;

                      - 'createAndWait', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row (but not make it available for use by
                      the managed device); and,

                      - 'destroy', which is supplied by a management
                      station wishing to delete all of the instances
                      associated with an existing conceptual row.

                 Whereas five of the six values (all except 'notReady') may
                 be specified in a management protocol set operation, only
                 three values will be returned in response to a management
                 protocol retrieval operation:  'notReady', 'notInService'
                 or 'active'.  That is, when queried, an existing
                 conceptual row has only three states:  it is either
                 available for use by the managed device (the status column
                 has the value 'active'); it is not available for use by
                 the managed device, though the agent has sufficient
                 information to make it so (the status column has the value
                 'notInService'); or, it is not available for use by the
                 managed device, and an attempt to make it so would fail
                 because the agent has insufficient information (the state
                 column has the value 'notReady').

                 For a detailed description of this object, please refer to
                 SNMPv2-TC MIB."
        ::= { diffServActionEntry 11 }

diffServMeterTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DiffServMeterEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for meter."
        ::= { diffServMgt 20 }

diffServMeterEntry OBJECT-TYPE
        SYNTAX      DiffServMeterEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for meter."
        INDEX       { diffServActionIndex }
        ::= { diffServMeterTable 1 }

DiffServMeterEntry ::= SEQUENCE
{
    diffServMeterIndex          Integer32,
    diffServMeterModel          INTEGER,
    diffServMeterRate           Integer32,
    diffServMeterBurstSize      Integer32,
    diffServMeterStatus         RowStatus,
    diffServMeterPeakRate       Integer32,
    diffServMeterPeakBurstSize  Integer32
}

diffServMeterIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry that describes a single set of token bucket
                     parameters."
        ::= { diffServMeterEntry 1 }

diffServMeterModel OBJECT-TYPE
    SYNTAX    INTEGER
        {
            default(1),
            flow(2),
            trTcmColorBlind(3),
            trTcmColorAware(4),
            srTcmColorBlind(5),
            srTcmColorAware(6)
        }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The Metering algorithm associated with the Token Bucket
                 parameters. The zeroDotZero indicates this is unknown."
    ::= { diffServMeterEntry 2 }

diffServMeterRate OBJECT-TYPE
    SYNTAX      Integer32 (1..1000000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The token-bucket rate, in kilobits per second (kbps)."
    ::= { diffServMeterEntry 3 }

diffServMeterBurstSize OBJECT-TYPE
    SYNTAX      Integer32 (64..524288)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The maximum number of bytes in a single transmission burst."
    ::= { diffServMeterEntry 4 }

diffServMeterStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "This object is used to create a new row or modify or delete
                 an existing row in this table. The status column has six
                 defined values:

                 The status column has six defined values:

                      - 'active', which indicates that the conceptual row is
                      available for use by the managed device;

                      - 'notInService', which indicates that the conceptual
                      row exists in the agent, but is unavailable for use by
                      the managed device (see NOTE below);

                      - 'notReady', which indicates that the conceptual row
                      exists in the agent, but is missing information
                      necessary in order to be available for use by the
                      managed device;

                      - 'createAndGo', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row and to have its status automatically set
                      to active, making it available for use by the managed
                      device;

                      - 'createAndWait', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row (but not make it available for use by
                      the managed device); and,

                      - 'destroy', which is supplied by a management station
                      wishing to delete all of the instances associated with
                      an existing conceptual row.

                 Whereas five of the six values (all except 'notReady') may
                 be specified in a management protocol set operation, only
                 three values will be returned in response to a management
                 protocol retrieval operation:  'notReady', 'notInService' or
                 'active'.  That is, when queried, an existing conceptual row
                 has only three states:  it is either available for use by
                 the managed device (the status column has the value
                 'active'); it is not available for use by the managed device,
                 though the agent has sufficient information to make it so
                 (the status column has the value 'notInService'); or, it is
                 not available for use by the managed device, and an attempt
                 to make it so would fail because the agent has insufficient
                 information (the state column has the value 'notReady').

                 For a detailed description of this object, please refer to
                 SNMPv2-TC MIB."
    ::= { diffServMeterEntry 6 }

diffServMeterPeakRate OBJECT-TYPE
    SYNTAX      Integer32 (0|64..10000000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The token-bucket rate, in kilobits per second (kbps)."
    ::= { diffServMeterEntry 7 }

diffServMeterPeakBurstSize OBJECT-TYPE
    SYNTAX      Integer32 (0|4000..16000000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The maximum number of bytes in a double transmission burst."
    ::= { diffServMeterEntry 8 }

diffServIpv6AceTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF DiffServIpv6AceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Table for IPv6 ACE."
    ::= { diffServMgt 21 }

diffServIpv6AceEntry OBJECT-TYPE
    SYNTAX      DiffServIpv6AceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Entry fo IPv6 ACE."
    INDEX       { diffServIpv6AceIndex }
        ::= { diffServIpv6AceTable 1 }

DiffServIpv6AceEntry ::= SEQUENCE
{
    diffServIpv6AceIndex                 Integer32,
    diffServIpv6AceType                  INTEGER,
    diffServIpv6AceAccess                INTEGER,
    diffServIpv6AceSourceIpAddr          OCTET STRING,
    diffServIpv6AceSourceIpAddrPrefixLen Integer32,
    diffServIpv6AceDestIpAddr            OCTET STRING,
    diffServIpv6AceDestIpAddrPrefixLen   Integer32,
    diffServIpv6AceDscp                  Integer32,
    diffServIpv6AceStatus                RowStatus
}

diffServIpv6AceIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An index that uniquely identifies an entry in the IPv6 table."
    ::= { diffServIpv6AceEntry 1 }

diffServIpv6AceType OBJECT-TYPE
    SYNTAX  INTEGER {
      standard(1),
      extended(2)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The specified IP v6 ACE type. When the type of this entry is
                 modified, then this entry will be auto-unbound from the
                 diffServAclEntry and the not supporting field of this entry
                 will be set 0."
    ::= { diffServIpv6AceEntry 2 }

diffServIpv6AceAccess OBJECT-TYPE
    SYNTAX  INTEGER {
        permit(1),
        deny(2)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Indicates the action to be taken if a packet matches this
                 ACE."
    ::= { diffServIpv6AceEntry 3 }

diffServIpv6AceSourceIpAddr OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Specifies the source IPv6 address."
    ::= { diffServIpv6AceEntry 4 }

diffServIpv6AceSourceIpAddrPrefixLen OBJECT-TYPE
    SYNTAX      Integer32 (0..128)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The length (in bits) associated with the source IPv6 address
                 prefix of this entry."
    ::= { diffServIpv6AceEntry 5 }

diffServIpv6AceDestIpAddr OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Specifies the destination IPv6 address. This object may not be
                 modified if the associated diffServIpv6AceType object is equal
                 to standard(1)."
    ::= { diffServIpv6AceEntry 6 }

diffServIpv6AceDestIpAddrPrefixLen OBJECT-TYPE
    SYNTAX      Integer32 (0..8)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The length (in bits) associated with the destination IPv6
                 address prefix of this entry. This object may not be modified
                 if the associated diffServIpv6AceType object is equal to
                 standard(1)."
    ::= { diffServIpv6AceEntry 7 }

diffServIpv6AceDscp OBJECT-TYPE
    SYNTAX      Integer32 (0..64)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Specifies the DSCP value to match against. This object may not
                 be modified if the associated diffServIpv6AceType object is
                 equal to standard(1)."
    ::= { diffServIpv6AceEntry 9 }

diffServIpv6AceStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "This object is used to create a new row or modify or delete
                 an existing row in this table. The status column has six
                 defined values:

                 The status column has six defined values:

                      - 'active', which indicates that the conceptual row is
                      available for use by the managed device;

                      - 'notInService', which indicates that the conceptual
                      row exists in the agent, but is unavailable for use by
                      the managed device (see NOTE below);

                      - 'notReady', which indicates that the conceptual row
                      exists in the agent, but is missing information
                      necessary in order to be available for use by the
                      managed device;

                      - 'createAndGo', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row and to have its status automatically set
                      to active, making it available for use by the managed
                      device;

                      - 'createAndWait', which is supplied by a management
                      station wishing to create a new instance of a
                      conceptual row (but not make it available for use by
                      the managed device); and,

                      - 'destroy', which is supplied by a management station
                      wishing to delete all of the instances associated with
                      an existing conceptual row.

                 Whereas five of the six values (all except 'notReady') may
                 be specified in a management protocol set operation, only
                 three values will be returned in response to a management
                 protocol retrieval operation:  'notReady', 'notInService' or
                 'active'.  That is, when queried, an existing conceptual row
                 has only three states:  it is either available for use by
                 the managed device (the status column has the value
                 'active'); it is not available for use by the managed device,
                 though the agent has sufficient information to make it so
                 (the status column has the value 'notInService'); or, it is
                 not available for use by the managed device, and an attempt
                 to make it so would fail because the agent has insufficient
                 information (the state column has the value 'notReady').

                 For a detailed description of this object, please refer to
                 SNMPv2-TC MIB."
    ::= { diffServIpv6AceEntry 11 }

diffServArpAceTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DiffServArpAceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual table of all of diffServArpAceEntry."
        ::= { diffServMgt 23 }

diffServArpAceEntry OBJECT-TYPE
        SYNTAX      DiffServArpAceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual row for diffServArpAceTable."
        INDEX       { diffServArpAceIndex }
        ::= { diffServArpAceTable 1 }

DiffServArpAceEntry ::= SEQUENCE
{
    diffServArpAceIndex                     Integer32,
    diffServArpAceAction                    INTEGER,
    diffServArpAcePktType                   INTEGER,
    diffServArpAceSourceIpAddr              IpAddress,
    diffServArpAceSourceIpAddrBitmask       IpAddress,
    diffServArpAceDestIpAddr                IpAddress,
    diffServArpAceDestIpAddrBitmask         IpAddress,
    diffServArpAceSourceMacAddr             OCTET STRING,
    diffServArpAceSourceMacAddrBitmask      OCTET STRING,
    diffServArpAceDestMacAddr               OCTET STRING,
    diffServArpAceDestMacAddrBitmask        OCTET STRING,
    diffServArpAceLogStatus                 EnabledStatus,
    diffServArpAceStatus                    RowStatus
}

diffServArpAceIndex OBJECT-TYPE
        SYNTAX      Integer32 (1..32)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The unique index of an ACE within an ACL."
        ::= { diffServArpAceEntry 1 }

diffServArpAceAction OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        permit(1),
                        deny(2)
                    }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Indicates the action to be taken if a packet matches
                     this ACE. This object cannot not be configured when
                     the status of the entry, diffServArpAceStatus, is
                     active(1)."
        ::= { diffServArpAceEntry 2 }

diffServArpAcePktType OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        request(1),
                        response(2),
                        both(3)
                    }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Indicates the packet type to be taken if a packet matches
                     this ACE. This object can not be configured when the
                     status of the entry, diffServArpAceStatus, is active(1)."
        ::= { diffServArpAceEntry 3 }

diffServArpAceSourceIpAddr OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The specified source ARP address. The packet's source
                     address is AND'ed with the value of
                     diffServArpAceSourceIpAddrBitmask and then compared
                     against the value of this object.
                     This object cannot be configured when the status of the
                     entry, diffServArpAceStatus, is active(1)."
        ::= { diffServArpAceEntry 4 }

diffServArpAceSourceIpAddrBitmask OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The specified source ARP address mask. The packet's
                     destination address is AND'ed with the value of
                     diffServArpAceSourceIpAddr and then compared against the
                     value of this object."
        ::= { diffServArpAceEntry 5 }

diffServArpAceDestIpAddr OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The specified destination IP address. The packet's
                     destination address is AND'ed with the value of
                     diffServArpAceDestIpAddrBitmask and then compared
                     against the value of this object."
        ::= { diffServArpAceEntry 6 }

diffServArpAceDestIpAddrBitmask OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The specified destination IP address mask."
        ::= { diffServArpAceEntry 7 }

diffServArpAceSourceMacAddr OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (6))
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Indicates the 48-bit destination MAC address. The
                     specified source MAC of the packet. The packet's
                     source MAC address is AND'ed with the value of
                     aceArpSourceMacAddrBitmask and then compared against
                     the value of this object. This object cannot be
                     configured when the status of the entry,
                     diffServArpAceStatus, is active(1)."
        ::= { diffServArpAceEntry 8 }

diffServArpAceSourceMacAddrBitmask OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (6))
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The specified source MAC address mask.
                    This object cannot be configured when the status of the
                    entry, diffServArpAceStatus, is active(1)."
        ::= { diffServArpAceEntry 9 }

diffServArpAceDestMacAddr OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (6))
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Indicates the 48-bit destination MAC address.
                     The specified destination MAC of the packet.
                     The packet's destination MAC address is AND'ed with the
                     value of aceArpDestMacAddrBitmask and then compared
                     against the value of this object. This object cannot be
                     configured when the status of the entry,
                     diffServArpAceStatus, is active(1)."
        ::= { diffServArpAceEntry 10 }

diffServArpAceDestMacAddrBitmask OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (6))
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The specified destination MAC address mask.
                     This object cannot be configured when the status of the
                     entry, diffServArpAceStatus, is active(1)."
        ::= { diffServArpAceEntry 11 }

diffServArpAceLogStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Indicates whether to log messages against the packets.
                     This object cannot be configured when the status of the
                     entry, diffServArpAceStatus, is active(1)."
        ::= { diffServArpAceEntry 12 }

diffServArpAceStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
	    DESCRIPTION
			"The status of this conceptual row entry.
            This object is used to manage the
			creation and deletion of conceptual rows.

			The status column has six defined values:

			     - 'active', which indicates that the conceptual row is
			     available for use by the managed device;

			     - 'notInService', which indicates that the conceptual
			     row exists in the agent, but is unavailable for use by
			     the managed device (see NOTE below);

			     - 'notReady', which indicates that the conceptual row
			     exists in the agent, but is missing information
			     necessary in order to be available for use by the
			     managed device;

			     - 'createAndGo', which is supplied by a management
			     station wishing to create a new instance of a
			     conceptual row and to have its status automatically set
			     to active, making it available for use by the managed
			     device;

			     - 'createAndWait', which is supplied by a management
			     station wishing to create a new instance of a
			     conceptual row (but not make it available for use by
			     the managed device); and,

			     - 'destroy', which is supplied by a management station
			     wishing to delete all of the instances associated with
			     an existing conceptual row.

			Whereas five of the six values (all except 'notReady') may
			be specified in a management protocol set operation, only
			three values will be returned in response to a management
			protocol retrieval operation:  'notReady', 'notInService' or
			'active'.  That is, when queried, an existing conceptual row
			has only three states:  it is either available for use by
			the managed device (the status column has value 'active');
			it is not available for use by the managed device, though
			the agent has sufficient information to make it so (the
			status column has value 'notInService'); or, it is not
			available for use by the managed device, and an attempt to
			make it so would fail because the agent has insufficient
			information (the state column has value 'notReady').

            For a detailed description of this object, please refer to
            SNMPv2-TC MIB."
        ::= { diffServArpAceEntry 13 }

diffServArpTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DiffServArpEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual table of all of diffServArpEntry."
        ::= { diffServMgt 24 }

diffServArpEntry OBJECT-TYPE
        SYNTAX      DiffServArpEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual row for diffServArpTable."
        INDEX       { diffServArpAclName }
        ::= { diffServArpTable 1 }

DiffServArpEntry ::= SEQUENCE
{
    diffServArpAclName      DisplayString
}

diffServArpAclName OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(1..16))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The name of an ACL. Within a feature, a unique name is
                     used to identify the list to which the entry belongs
                     in the device."
        ::= { diffServArpEntry 1 }

diffServTcamMgt     OBJECT IDENTIFIER ::= { diffServMgt 25 }

diffServTcamTotalPolicyControlEntries OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The total number of policy control entries."
        ::= { diffServTcamMgt 1 }

diffServTcamFreePolicyControlEntries OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The free number of policy control entries."
        ::= { diffServTcamMgt 2 }

diffServTcamUtilization OBJECT-TYPE
        SYNTAX      Integer32(0..10000)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "TCAM utilization in hundredths of a percent."
        ::= { diffServTcamMgt 3 }

diffServTcamEntriesUsedBySystem OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The number of policy control entries used by system."
        ::= { diffServTcamMgt 4 }

diffServTcamEntriesUsedByUser OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The number of policy control entries used by user."
        ::= { diffServTcamMgt 5 }

--
-- securityMgt
--

-- Management for security, e.g. user security and port security.

privateVlanMgt      OBJECT IDENTIFIER ::= { securityMgt 1 }
portSecurityMgt     OBJECT IDENTIFIER ::= { securityMgt 2 }
radiusMgt           OBJECT IDENTIFIER ::= { securityMgt 4 }
tacacsMgt           OBJECT IDENTIFIER ::= { securityMgt 5 }
sshMgt              OBJECT IDENTIFIER ::= { securityMgt 6 }
aclMgt              OBJECT IDENTIFIER ::= { securityMgt 7 }
ipFilterMgt         OBJECT IDENTIFIER ::= { securityMgt 9 }
userAuthMgt         OBJECT IDENTIFIER ::= { securityMgt 10 }
dot1xMgt            OBJECT IDENTIFIER ::= { securityMgt 11 }
aaaMgt              OBJECT IDENTIFIER ::= { securityMgt 12 }
networkAccessMgt    OBJECT IDENTIFIER ::= { securityMgt 13 }
macAuthMgt          OBJECT IDENTIFIER ::= { securityMgt 14 }
webAuthMgt          OBJECT IDENTIFIER ::= { securityMgt 15 }

--
-- SYS_CPNT_COMMUNITY_PRIVATE_VLAN (use PVLAN_MGR API) start

privateVlanStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This controls whether private VLAN is enabled."
        ::= { privateVlanMgt 1 }

privateVlanUplinkPorts OBJECT-TYPE
        SYNTAX      PortList
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This is the list of uplink ports for private VLAN.
                    They should not overlap with privateVlanDownlinkPorts.
                    0 will be displayed if the privateVlanStatus is disabled.
                    You must enable the privateVlanStatus before setting this variable."
        ::= { privateVlanMgt 2 }

privateVlanDownlinkPorts OBJECT-TYPE
        SYNTAX      PortList
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This is the list of downlink ports for private VLAN.
                    They should not overlap with privateVlanUplinkPorts.
                    Multiple port setting is permitted.
                    0 will be displayed if the privateVlanStatus is disabled.
                    You must enable the privateVlanStatus before setting this variable."
        ::= { privateVlanMgt 3 }

privateVlanVlanTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PrivateVlanVlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION   "A table containing private VLAN information on the
                       VLANs which currently exist."
        ::= { privateVlanMgt 4 }

privateVlanVlanEntry OBJECT-TYPE
        SYNTAX      PrivateVlanVlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION  "A conceptual row containing the private VLAN
                      information on the VLANs for a particular management
                      domain."
        INDEX       { privateVlanVlanIndex }
        ::= { privateVlanVlanTable 1 }

PrivateVlanVlanEntry ::= SEQUENCE
{
   privateVlanVlanIndex             Integer32,
   privateVlanVlanType              INTEGER,
   privateVlanAssoicatedPrimaryVlan Integer32
}

privateVlanVlanIndex OBJECT-TYPE
         SYNTAX      Integer32(1..4094)
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION "The VLAN ID of this private VLAN."
         ::= { privateVlanVlanEntry 1 }

privateVlanVlanType OBJECT-TYPE
         SYNTAX     INTEGER
                    {
                     invalid(1),
                     primary(2),
                     isolated(3),
                     community(4)
                     }
         MAX-ACCESS read-create
         STATUS     current
         DESCRIPTION "The VLAN type as defined for Private VLAN feature.
                      Set the value to invalid(1) to destroy an entry. Set
                      other values to create an entry. If an index
                      already exists, set others to modifiy it. Note that a VLAN's
                      private VLAN type cannot be changed once it has
                      any port members."
         ::= { privateVlanVlanEntry 2 }

privateVlanAssoicatedPrimaryVlan OBJECT-TYPE
         SYNTAX      Integer32(0..4094)
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
            "The VLAN ID of the associated primary VLAN used for
            the private VLAN feature if privateVlanVlanType has the
            value of isolated(3), community(4). If privateVlanVlanType
            has the value of primary(2), then this object has the value of 0.

            Note that one isolated VLAN can only be associated
            with one unique primary VLAN. One primary VLAN can only
            be associated with one isolated VLAN.

            One primary VLAN can be associated with multiple community VLANs;
            one community VLAN can only be associated with one unique primary VLAN."
         ::= { privateVlanVlanEntry 3 }


--
-- Table for configuring secondary VLAN on private ports
--

privateVlanPrivatePortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PrivateVlanPrivatePortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
             "A table containing information on the configuration of
              secondary VLANs on the device ports."
        ::= { privateVlanMgt 5 }

privateVlanPrivatePortEntry OBJECT-TYPE
        SYNTAX      PrivateVlanPrivatePortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "A conceptual row containing information of the
            configuration of secondary VLANs for each port. An entry
            is created by the managed system for each interface which
            can be configured as a private port for Private VLAN
            feature."
        INDEX      { privateVlanPrivatePortIfIndex }
        ::= { privateVlanPrivatePortTable 1 }

PrivateVlanPrivatePortEntry ::= SEQUENCE
{
     privateVlanPrivatePortIfIndex        Integer32,
     privateVlanPrivatePortSecondaryVlan  Integer32
}

privateVlanPrivatePortIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This is defined as the ifIndex."
        ::= { privateVlanPrivatePortEntry 1 }

privateVlanPrivatePortSecondaryVlan OBJECT-TYPE
        SYNTAX      Integer32(0..4094)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
              "The VLAN ID of the secondary VLAN configured on this
              private port. A private port is a port that allows
              ingress traffic of the secondary VLAN as well as
              egress traffic of its associated primary VLAN, but
              blocks the egress traffic of the isolated VLAN while
              allowing the egress traffic of the community
              or twoWayCommunity VLAN depending on the type of the
              secondary VLAN.

              Note that a port can join a secondary VLAN only after
              this secondary VLAN has been associated with a primary
              VLAN, i.e., the cpvlanVlanAssociatedPrimaryVlan has a
              non-zero value. The default value of 0 for this object
              means this port has not yet joined a secondary VLAN."
        DEFVAL     { 0 }
        ::= { privateVlanPrivatePortEntry 2 }

--
-- Table for remapping secondary VLAN to primary VLAN on promiscuous
-- ports for Private VLAN feature
--

privateVlanPromPortTable OBJECT-TYPE
        SYNTAX     SEQUENCE OF PrivateVlanPromPortEntry
        MAX-ACCESS not-accessible
        STATUS     current
        DESCRIPTION "A table containing secondary VLAN to primary VLAN remapping
                    information on ports of the device."
        ::= { privateVlanMgt 6 }

privateVlanPromPortEntry OBJECT-TYPE
        SYNTAX      PrivateVlanPromPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A conceptual row containing secondary VLAN to primary
                    VLAN remapping information for each port.
                    An entry is created by the managed system for each interface
                     which can be configured as a promiscuous port for the
                     private VLAN feature."
        INDEX      { privateVlanPromPortIfIndex }
        ::= { privateVlanPromPortTable 1 }

PrivateVlanPromPortEntry ::= SEQUENCE
{
    privateVlanPromPortIfIndex          Integer32,
    privateVlanPromPortPrimaryVlanId    Integer32,
    privateVlanPromPortSecondaryRemap   OCTET STRING,
    privateVlanPromPortSecondaryRemap2k OCTET STRING,
    privateVlanPromPortSecondaryRemap3k OCTET STRING,
    privateVlanPromPortSecondaryRemap4k OCTET STRING
}

privateVlanPromPortIfIndex OBJECT-TYPE
    SYNTAX       Integer32
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION  "This is defined as ifIndex."
    ::= { privateVlanPromPortEntry 1 }

privateVlanPromPortPrimaryVlanId OBJECT-TYPE
    SYNTAX      Integer32(0..4094)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The primary VLAN ID of the promiscous port."
    ::= { privateVlanPromPortEntry 2 }

privateVlanPromPortSecondaryRemap OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN in the
            management domain on this port. The first octet
            corresponds to VLANs with VlanIndexOrZero values of 0
            through 7; the second octet to VLANs 8 through 15; etc.
            The most significant bit of each octet corresponds to
            the lowest value VlanIndexOrZero in that octet.

            Note that if the length of this string is less than
            128 octets, any 'missing' octets are assumed to contain
            the value zero. An NMS may omit any zero-valued octets
            from the end of this string in order to reduce SetPDU
            size, and the agent may also omit zero-valued trailing
            octets, to reduce the size of GetResponse PDUs."
    ::= { privateVlanPromPortEntry 3 }

privateVlanPromPortSecondaryRemap2k OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN for
            VLANs with VlanIndexOrZero values of 1024 through 2047
            in the management domain on this port. The first octet
            corresponds to VLANs with VlanIndexOrZero values of 1024
            through 1031; the second octet to VLANs 1032 through
            1039; etc. The most significant bit of each octet
            corresponds to the lowest value VlanIndexOrZero in
            that octet.

            Note that if the length of this string is less than
            128 octets, any 'missing' octets are assumed to contain
            the value zero. An NMS may omit any zero-valued octets
            from the end of this string in order to reduce SetPDU
            size, and the agent may also omit zero-valued trailing
            octets, to reduce the size of GetResponse PDUs.

            This object is only instantiated on devices which support
            the range of VlanIndexOrZero up to 4095."
    ::= { privateVlanPromPortEntry 4 }

privateVlanPromPortSecondaryRemap3k OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN for
            VLANs with VlanIndexOrZero values of 2048 through 3071
            in the management domain on this port. The first octet
            corresponds to VLANs with VlanIndexOrZero values of 2048
            through 2055; the second octet to VLANs 2056 through
            2063; etc. The most significant bit of each octet
            corresponds to the lowest value VlanIndexOrZero in
            that octet.

            Note that if the length of this string is less than
            128 octets, any 'missing' octets are assumed to contain
            the value zero. An NMS may omit any zero-valued octets
            from the end of this string in order to reduce SetPDU
            size, and the agent may also omit zero-valued trailing
            octets, to reduce the size of GetResponse PDUs.

            This object is only instantiated on devices which support
            the range of VlanIndexOrZero up to 4095."
    ::= { privateVlanPromPortEntry 5 }

privateVlanPromPortSecondaryRemap4k OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..128))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "A string of octets containing one bit per VLAN for
            VLANs with VlanIndexOrZero values of 3072 through 4095
            in the management domain on this port. The first octet
            corresponds to VLANs with VlanIndexOrZero values of 3072
            through 3079; the second octet to VLANs 3080 through
            3087; etc. The most significant bit of each octet
            corresponds to the lowest value VlanIndexOrZero in
            that octet.

            Note that if the length of this string is less than
            128 octets, any 'missing' octets are assumed to contain
            the value zero. An NMS may omit any zero-valued octets
            from the end of this string in order to reduce SetPDU
            size, and the agent may also omit zero-valued trailing
            octets, to reduce the size of GetResponse PDUs.

            This object is only instantiated on devices which support
            the range of VlanIndexOrZero up to 4095."
    ::= { privateVlanPromPortEntry 6 }
-- SYS_CPNT_COMMUNITY_PRIVATE_VLAN (use PVLAN_MGR API) end

privateVlanSessionTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF PrivateVlanSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Contains the settings for private VLAN Session."
    ::= { privateVlanMgt 8 }

privateVlanSessionEntry   OBJECT-TYPE
    SYNTAX      PrivateVlanSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A conceptual row in the privateVlanSession table."
    INDEX { privateVlanSessionId }
    ::= { privateVlanSessionTable 1 }

PrivateVlanSessionEntry::= SEQUENCE
{
    privateVlanSessionId                            INTEGER,
    privateVlanSessionUplinkPorts                   PortList,
    privateVlanSessionDownlinkPorts                 PortList,
    privateVlanSessionStatus                        ValidStatus
}

privateVlanSessionId              OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The session ID that may specifiy certain entry in the table which contains private
                 VLAN session information."
    ::= { privateVlanSessionEntry 1 }

privateVlanSessionUplinkPorts      OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "This is the list of uplink ports for a session of private VLAN. They should not
                 overlap with the privateVlanSessionPortDownlink of the same session, and they
                 also should not overlap with the privateVlanSessionPortUplink and the
                 privateVlanSessionPortDownlink of other session."
    ::= { privateVlanSessionEntry 2 }

privateVlanSessionDownlinkPorts      OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "This is the list of downlink ports for a session of private VLAN. They should not
                 overlap with the privateVlanSessionPortUplink of the same session, and they also
                 should not overlap with the privateVlanSessionPortUplink and the
                 privateVlanSessionPortDownlink of other session."
    ::= { privateVlanSessionEntry 3 }

privateVlanSessionStatus     OBJECT-TYPE
    SYNTAX      ValidStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Set this to valid(1) to create an entry. Sets this to
                 invalid(2) to destroy an entry."
    ::= { privateVlanSessionEntry 4 }

privateVlanUplinkToUplink     OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    blocking(1),
                    forwarding(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Sets this to blocking(2) to deny the traffic of uplink
                 ports between different sessions. Set this to forwarding(1)
                 to allow the traffic of uplink ports between different
                 sessions."
    ::= { privateVlanMgt 9 }

portSecPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PortSecPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port security(MAC binding) Table."
        ::= { portSecurityMgt 1 }

portSecPortEntry OBJECT-TYPE
        SYNTAX      PortSecPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The entry of portSecPortTable."
        INDEX       { portSecPortIndex }
        ::= { portSecPortTable 1 }

PortSecPortEntry ::= SEQUENCE
{
      portSecPortIndex      Integer32,
      portSecPortStatus     EnabledStatus,
      portSecAction         INTEGER,
      portSecMaxMacCount       Integer32
}

portSecPortIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and the trunk (excluding trunk members) interface of
                     the portTable. The interface identified by a particular value
                     of this index is the same interface as identified by the same
                     value of ifIndex in the IF-MIB."
        ::= { portSecPortEntry 1 }

portSecPortStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Set enabled(1) to enable port security and set disabled(2) to
                     disable port security."
        ::= { portSecPortEntry 2  }

portSecAction OBJECT-TYPE
        SYNTAX        INTEGER
                      {
                        none(1),
                        trap(2),
                        shutdown(3),
                        trapAndShutdown(4)
                      }
        MAX-ACCESS    read-write
        STATUS        current
        DESCRIPTION  "The corresponding actions that will take place when a
                      port is under intrusion, when this variable is set to
                      none(1), no action will be performed, when this variable is
                      set to trap(2), a swPortSecurityTrap trap will be sent,
                      when this variable is set to shutdown(3), the port will
                      shutdown, when this variable is set to
                      trapAndShutdown(4), a swPortSecurityTrap will be sent
                      and the port will shutdown."
        ::= { portSecPortEntry 3  }

portSecMaxMacCount OBJECT-TYPE
        SYNTAX       Integer32(0..1024)
        MAX-ACCESS   read-write
        STATUS       current
        DESCRIPTION  "The maximun number of MAC addresses that will be learned and locked.
                      When we change the value of this variable, if the
                      portSecPortStatus is enabled, we will discard all secure MAC
                      and begin to learn again, until the number of MAC has reached
                      this value, and only the secure MAC addresses can enter
                      this port. If the portSecPortStatus is disabled, we will begin
                      to learn the MAC, and auto enabled the portSecPortStatus when
                      the MAC has reached this value."
        ::= { portSecPortEntry 4 }

--
-- radiusMgt
--

-- Management for Remote Authentication Dial-In User Service (RADIUS).
--SYS_ADPT_MAX_NBR_OF_RADIUS_SERVERS=1: single server
--SYS_ADPT_MAX_NBR_OF_RADIUS_SERVERS>1: multiple server

radiusServerGlobalAuthPort OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Aauthentication port number for RADIUS server.
                     When specified radius server do not set
                     aauthentication port number, this value is used."
        ::= { radiusMgt 1 }

radiusServerGlobalAcctPort OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Accounting port number of RADIUS server.
                    When specified radius server do not set
                    accounting port number, this value is used."
        ::= { radiusMgt 2 }

radiusServerGlobalKey OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..48))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Key for RADIUS. This variable can only be written.
                     When this variable is read, it always returns a
                     zero-length string.
                     When specified radius server do not set
                     key, this value will be assigned into the specified
                     radius server."
        ::= { radiusMgt 3 }

radiusServerGlobalRetransmit OBJECT-TYPE
        SYNTAX      INTEGER (1..30)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Maximum number of retransmissions for RADIUS.
                     When specified radius server do not set
                     maximum number of retransmissions, this value is used."
        ::= { radiusMgt 4 }

radiusServerGlobalTimeout OBJECT-TYPE
        SYNTAX      INTEGER (1..65535)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Timeout for RADIUS.
                     When specified radius server do not set
                     timeout, this value is used."
        ::= { radiusMgt 5 }

--radiusServerTable

radiusServerTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RadiusServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The table for RADIUS server."
        ::= { radiusMgt 7 }

radiusServerEntry OBJECT-TYPE
        SYNTAX      RadiusServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual row for radiusServerTable."
        INDEX       { radiusServerIndex }
        ::= { radiusServerTable 1 }

RadiusServerEntry ::= SEQUENCE
{
   radiusServerIndex                  Integer32,
   radiusServerAddress                IpAddress,
   radiusServerAuthPortNumber         Integer32,
   radiusServerAcctPortNumber         Integer32,
   radiusServerKey                    DisplayString,
   radiusServerRetransmit             Integer32,
   radiusServerTimeout                Integer32,
   radiusServerStatus                 ValidStatus
}

radiusServerIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The RADIUS server index in the table."
        ::= { radiusServerEntry 1 }

radiusServerAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "IP address of a RADIUS server."
        ::= { radiusServerEntry 2 }

radiusServerAuthPortNumber OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Authentication port number of RADIUS server."
        ::= { radiusServerEntry 3 }

radiusServerAcctPortNumber OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Accounting port number of RADIUS server."
        ::= { radiusServerEntry 4 }

radiusServerKey OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..48))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Key for RADIUS. This variable can only be written.
                     When this variable is read, it always returns a
                     zero-length string."
        ::= { radiusServerEntry 5 }

radiusServerRetransmit OBJECT-TYPE
        SYNTAX      Integer32 (1..30)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Timeout for RADIUS."
        ::= { radiusServerEntry 6 }

radiusServerTimeout OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Timeout for RADIUS."
        ::= { radiusServerEntry 7 }

radiusServerStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Setting this to valid(1) creates an entry.
                     Setting this to invalid(2) destroys an entry."
        ::= { radiusServerEntry 8 }

--
-- tacacsMgt
--

-- Management for Terminal Access Controller Access Control System plus (TACACS+).

-- Global server setting
tacacsPlusServerGlobalPortNumber OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "TCP port number of TACACS+ server.
                     When specified TACACS+ server do not set
                     TCP port number, this this value is used."
        ::= { tacacsMgt 2 }

tacacsPlusServerGlobalKey OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..48))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The encryption key used to encrpt the traffic between 
                     client and TACACS+ server. Do not use blank spaces in 
                     the string. This variable can only be set. When this 
                     variable is read, it always returns a zero-length string.
                     When specified TACACS+ server do not set the encryption 
                     key , this value will be assigned into the specified 
                     TACACS+ server."
        ::= { tacacsMgt 3 }

tacacsPlusServerTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF TacacsPlusServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The table for TACACS+ server."
        ::= { tacacsMgt 4 }

tacacsPlusServerEntry OBJECT-TYPE
        SYNTAX      TacacsPlusServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual row for tacacsPlusServerTable."
        INDEX       { tacacsPlusServerIndex }
        ::= { tacacsPlusServerTable 1 }

TacacsPlusServerEntry ::= SEQUENCE
{
   tacacsPlusServerIndex            Integer32,
   tacacsPlusServerAddress          IpAddress,
   tacacsPlusServerPortNumber       Integer32,
   tacacsPlusServerKey	            DisplayString,
   tacacsPlusServerStatus           ValidStatus
}

tacacsPlusServerIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "TACACS+ server index."
        ::= { tacacsPlusServerEntry 1 }

tacacsPlusServerAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "IP address of a TACACS+ server."
        ::= { tacacsPlusServerEntry 2 }

tacacsPlusServerPortNumber OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "TCP port number of a TACACS+ server."
        ::= { tacacsPlusServerEntry 3 }

tacacsPlusServerKey OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..48))
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The encryption key used to encrpt the traffic between client and
                     TACACS+ server. Do not use blank spaces in the string. This
                     variable can only be set. When this variable is read, it always
                     returns a zero-length string."
        ::= { tacacsPlusServerEntry 4 }

tacacsPlusServerStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Setting this to valid(1) creates an entry.
                     Setting this to invalid(2) destroys an entry."
        ::= { tacacsPlusServerEntry 8 }

--
-- sshMgt
--

-- Management for Secure Shell Configuration

sshServerStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The status of Secure Shell Server. Set this value to
                     enabled(1) to enable SSH server, set this value to
                     disabled(2) to disable the SSH server."
        ::= { sshMgt 1 }

sshServerMajorVersion  OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The major version of the SSH Server."
        ::= { sshMgt 2 }

sshServerMinorVersion  OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The minor version of the SSH Server."
        ::= { sshMgt 3 }

sshTimeout OBJECT-TYPE
        SYNTAX      INTEGER(1..120)
        UNITS       "seconds"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The time interval that the router waits for the SSH
                     client to respond. The range is 1-120."
        ::= { sshMgt 4 }

sshAuthRetries OBJECT-TYPE
        SYNTAX      INTEGER(1..5)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The number of attempts after which the interface is reset.
                     The range is 1-5."
        ::= { sshMgt 5 }

sshConnInfoTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF SshConnInfoEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The table for Secure Shell Connection."
        ::= { sshMgt 6 }

sshConnInfoEntry OBJECT-TYPE
        SYNTAX      SshConnInfoEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual row for sshConnInfoTable."
        INDEX       { sshConnID }
        ::= { sshConnInfoTable 1 }

SshConnInfoEntry ::= SEQUENCE
{
--both sshv1 & sshv2 start
   sshConnID             Integer32,
   sshConnMajorVersion   Integer32,
   sshConnMinorVersion   Integer32,
   sshConnStatus         INTEGER,
--both sshv1 & sshv2 end
--both sshv1 & sshv2 start
   sshConnUserName       DisplayString,
   sshDisconnect         INTEGER,
--both sshv1 & sshv2 end
--sshv2 only start
   sshConnEncryptionTypeStr DisplayString
--sshv2 only end
}

--both sshv1 & sshv2 start
sshConnID OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The connection ID of the Secure Shell Connection."
        ::= { sshConnInfoEntry 1 }

sshConnMajorVersion OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The SSH major version."
        ::= { sshConnInfoEntry 2 }

sshConnMinorVersion OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The SSH minor version."
        ::= { sshConnInfoEntry 3 }

sshConnStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                      negotiationStart(1),
                      authenticationStart(2),
                      sessionStart(3)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The SSH connection State. negotiationStart(1) means the
                     SSH is in its negotiation start state, authenticationStart(2)
                     means the SSH is in authentication start state, sessionStart(3)
                     means the SSH is in session start State."
        ::= { sshConnInfoEntry 5 }

--both sshv1 & sshv2 end


--both sshv1 & sshv2 start


sshConnUserName OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(1..8))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The user name of the connection."
        ::= { sshConnInfoEntry 6 }

sshDisconnect OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                      noDisconnect(1),
                      disconnect(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Set the variable to disconnect the connection,
                     noDisconnect(1) will always be obtained when reading this variable."
        ::= { sshConnInfoEntry 7 }

--both sshv1 & sshv2 end

--sshv2 only start
sshConnEncryptionTypeStr  OBJECT-TYPE
SYNTAX      DisplayString(SIZE(0..64))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The encryption type of the SSH."
        ::= { sshConnInfoEntry 8 }


sshKeySize OBJECT-TYPE
        SYNTAX      INTEGER(512..896)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The SSH server key size."
        ::= { sshMgt 7 }


sshRsaHostKey1 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA host key segment 1."
        ::= { sshMgt 8 }

sshRsaHostKey2 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA host key segment 2."
        ::= { sshMgt 9 }

sshRsaHostKey3 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA host key segment 3."
        ::= { sshMgt 10 }

sshRsaHostKey4 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA host key segment 4."
        ::= { sshMgt 11 }

sshRsaHostKey5 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA host key segment 5."
        ::= { sshMgt 12 }

sshRsaHostKey6 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA host key segment 6."
        ::= { sshMgt 13 }

sshRsaHostKey7 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA host key segment 7."
        ::= { sshMgt 14 }

sshRsaHostKey8 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA host key segment 8."
        ::= { sshMgt 15 }

sshDsaHostKey1 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA host key segment 1."
        ::= { sshMgt 16 }

sshDsaHostKey2 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA host key segment 2."
        ::= { sshMgt 17 }

sshDsaHostKey3 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA host key segment 3."
        ::= { sshMgt 18 }

sshDsaHostKey4 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA host key segment 4."
        ::= { sshMgt 19 }

sshDsaHostKey5 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA host key segment 5."
        ::= { sshMgt 20 }

sshDsaHostKey6 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA host key segment 6."
        ::= { sshMgt 21 }

sshDsaHostKey7 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA host key segment 7."
        ::= { sshMgt 22 }

sshDsaHostKey8 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA host key segment 8."
        ::= { sshMgt 23 }

sshHostKeyGenAction OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        noGen(1),
                        genRsaKey(2),
                        genDsaKey(3),
                        genBothKeys(4)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This variable is for host key generating.

                    For the set behavior:
                    Set it to genRsaKey(2) to generate the RSA host key,
                    and to genDsaKey(3) to generate the DSA host key,
                    if genBothKeys(4) is set, both RSA and DSA host key are
                    generated.

                    For the get behavior:
                    You will get genRsaKey(2), genDsaKey(3) or
                    genBothKeys(4) when the key gen action is in progress.
                    otherwise, you will get noGen(1)."
        ::= { sshMgt 24 }

sshHostKeyGenStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        unknown(1),
                        success(2),
                        failure(3)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The result of the last KeyGen status.
                     if no key gen action has been performed.
                     you will get unknown(1) status."
        ::= { sshMgt 25 }

sshHostKeySaveAction OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        noSave(1),
                        save(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "To save host key from memory to flash.

                     For the set behavior:
                     Set it to save(2) to perform the save operation.

                     For the get behavior:
                     You will get save(1) when the save action is in progress.
                     Otherwise, you will get noSave(1)."
        ::= { sshMgt 26 }

sshHostKeySaveStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        unknown(1),
                        success(2),
                        failure(3)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The result of the last savekey status.
                     If no save action has been performed,
                     you will get unknown(1) status."
        ::= { sshMgt 27 }

sshHostKeyDelAction  OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        noDel(1),
                        delRsaKey(2),
                        delDsaKey(3),
                        delBothKeys(4)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "To delete the host key.

                     For the set behavior:
                     Set it to delRsaKey(2) to delete the RSA host key,
                     to delDsaKey(3) to delete the DSA host key,
                     or to delBothKeys(4) to delete both RSA and DSA host key.

                     For the get behavior:
                     You will get delRsaKey(2), delDsaKey(3) or  delBothKeys(4)
                     when the delete operation is in progress.
                     Otherwise, you will get noDel(1)."
        ::= { sshMgt 28 }

sshUserTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF SshUserEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual table of all of sshUserEntry."
        ::= { sshMgt 29 }

sshUserEntry OBJECT-TYPE
        SYNTAX      SshUserEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual row for sshUserTable."
        INDEX       { IMPLIED sshUserName}
        ::= { sshUserTable 1 }

SshUserEntry ::= SEQUENCE
{
    sshUserName             DisplayString,
    sshUserRsaKey1          KeySegment,
    sshUserRsaKey2          KeySegment,
    sshUserRsaKey3          KeySegment,
    sshUserRsaKey4          KeySegment,
    sshUserRsaKey5          KeySegment,
    sshUserRsaKey6          KeySegment,
    sshUserRsaKey7          KeySegment,
    sshUserRsaKey8          KeySegment,
    sshUserDsaKey1          KeySegment,
    sshUserDsaKey2          KeySegment,
    sshUserDsaKey3          KeySegment,
    sshUserDsaKey4          KeySegment,
    sshUserDsaKey5          KeySegment,
    sshUserDsaKey6          KeySegment,
    sshUserDsaKey7          KeySegment,
    sshUserDsaKey8          KeySegment,
    sshUserKeyDelAction     INTEGER
}

sshUserName OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(1..8))
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "User Name."
        ::= { sshUserEntry 1 }

sshUserRsaKey1 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA user key segment 1."
        ::= { sshUserEntry 2 }

sshUserRsaKey2 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA user key segment 2."
        ::= { sshUserEntry 3 }

sshUserRsaKey3 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA user key segment 3."
        ::= { sshUserEntry 4 }

sshUserRsaKey4 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA user key segment 4."
        ::= { sshUserEntry 5 }

sshUserRsaKey5 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA user key segment 5."
        ::= { sshUserEntry 6 }

sshUserRsaKey6 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA user key segment 6."
        ::= { sshUserEntry 7 }

sshUserRsaKey7 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA user key segment 7."
        ::= { sshUserEntry 8 }

sshUserRsaKey8 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The RSA user key segment 8."
        ::= { sshUserEntry 9 }

sshUserDsaKey1 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA user key segment 1."
        ::= { sshUserEntry 10 }

sshUserDsaKey2 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA user key segment 2."
        ::= { sshUserEntry 11 }

sshUserDsaKey3 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA user key segment 3."
        ::= { sshUserEntry 12 }

sshUserDsaKey4 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA user key segment 4."
        ::= { sshUserEntry 13 }

sshUserDsaKey5 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA user key segment 5."
        ::= { sshUserEntry 14 }

sshUserDsaKey6 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA user key segment 6."
        ::= { sshUserEntry 15 }

sshUserDsaKey7 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA user key segment 7."
        ::= { sshUserEntry 16 }

sshUserDsaKey8 OBJECT-TYPE
        SYNTAX      KeySegment
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The DSA user key segment 8."
        ::= { sshUserEntry 17 }

sshUserKeyDelAction  OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        noDel(1),
                        delRsaKey(2),
                        delDsaKey(3),
                        delBothKeys(4)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "To delete the user key.

                     For the set behavior:
                     Set it to delRsaKey(2) to delete the RSA user key,
                     to delDsaKey(3) to delete the DSA user key,
                     or to delBothKeys(4) to delete both RSA and DSA user key.

                     For the get behavior:
                     You will get delRsaKey(2), delDsaKey(3) or  delBothKeys(4)
                     when the delete operation is in progress.
                     Otherwise, you will get noDel(1)."
        ::= { sshUserEntry 18 }

sshRsaHostKeySHA1FingerPrint OBJECT-TYPE
       SYNTAX     DisplayString(SIZE(65))
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION "The SHA1 finger print of the RSA host key."
       ::= { sshMgt 30 }

sshRsaHostKeyMD5FingerPrint OBJECT-TYPE
       SYNTAX     DisplayString(SIZE(47))
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION "The MD5 finger print of RSA host key."
       ::= { sshMgt 31 }

sshDsaHostKeySHA1FingerPrint OBJECT-TYPE
       SYNTAX     DisplayString(SIZE(65))
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION "The SHA1 finger print of the DSA host key."
       ::= { sshMgt 32 }

sshDsaHostKeyMD5FingerPrint OBJECT-TYPE
       SYNTAX     DisplayString(SIZE(47))
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION "The MD5 finger print of the DSA host key."
       ::= { sshMgt 33 }
--sshv2 only end

--
-- aaaMgt
--

aaaMethodTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF AaaMethodEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Contains the settings needed for accounting."
        ::= { aaaMgt 1 }

aaaMethodEntry OBJECT-TYPE
        SYNTAX      AaaMethodEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A conceptual row in the aaaMethodTable."
        INDEX      { aaaMethodIndex }
        ::= { aaaMethodTable 1 }

AaaMethodEntry ::= SEQUENCE {
        aaaMethodIndex                  Integer32,
        aaaMethodName                   DisplayString,
        aaaMethodGroupName              DisplayString,
        aaaMethodMode                   INTEGER,
        aaaMethodStatus                 ValidStatus,
        aaaMethodClientType             INTEGER,
        aaaMethodPrivilegeLevel         INTEGER
}

aaaMethodIndex OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION  "Specifies the index for the entry."
        ::= { aaaMethodEntry 1 }

aaaMethodName OBJECT-TYPE
        SYNTAX       DisplayString(SIZE(1..255))
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION "Name for the method."
        ::= { aaaMethodEntry 2 }

aaaMethodGroupName OBJECT-TYPE
        SYNTAX       DisplayString(SIZE(1..255))
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION "Name for the server to use, pointing to aaaRadiusGroupName
                     or aaaTacacsPlusGroupName."
        ::= { aaaMethodEntry 3 }

aaaMethodMode OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                       start-stop(1)
                    }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "start-stop(1),sends a 'start' accounting notice at the beginning of a process and
        a 'stop' accounting notice at the end of a process. The 'start' accounting record
        is sent in the background. The requested user process begins regardless of whether or not
        the 'start' accounting notice was received by the accounting server."
        ::= { aaaMethodEntry 4 }

aaaMethodStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Set to 1 to initiate the aaaMethodTable, 2 to destroy the table."
        ::= { aaaMethodEntry 5 }

aaaMethodClientType OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                       dot1x(1), exec(2)
                    }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "dot1x(1): Provides accounting service for 802.1x activity;
                     exec(2): Provides accounting service for EXEC connection
                     such as Telnet, SSH or console."
        ::= { aaaMethodEntry 6 }

aaaMethodPrivilegeLevel OBJECT-TYPE
        SYNTAX       INTEGER (0..15)
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION  "Specifies the privilege level for the entry.
                      When aaaMethodClientType is in the mode of command(3),
                      the privilege level is enabled to be accessed."
        ::= { aaaMethodEntry 7 }

aaaRadiusGroupTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF AaaRadiusGroupEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Uses a subset of RADIUS servers for accounting as defined by the server group"
        ::= { aaaMgt 2 }

aaaRadiusGroupEntry OBJECT-TYPE
        SYNTAX      AaaRadiusGroupEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A conceptual row of aaaRadiusGroupEntry."
        INDEX      { aaaRadiusGroupIndex }
        ::= { aaaRadiusGroupTable 1 }

AaaRadiusGroupEntry ::= SEQUENCE
{
        aaaRadiusGroupIndex          Integer32,
        aaaRadiusGroupServerBitMap   OCTET STRING,
        aaaRadiusGroupName           DisplayString,
        aaaRadiusGroupStatus         ValidStatus
}

aaaRadiusGroupIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Specifies the index for the entry."
        ::= { aaaRadiusGroupEntry 1 }

aaaRadiusGroupServerBitMap OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (1))
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Identifies which RADIUS sever to use, each bit points to
                     one RADIUS server. 80 (1000 0000) enables server 1,
                     C0 (11000000) enables server 1 and 2, and 
                     F8 (1111 10000) enables server 1 to 5."
        ::= { aaaRadiusGroupEntry 2 }

aaaRadiusGroupName OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Uses a subset of servers for accounting as
        defined by the server group. The same name as aaaTacasPlusGroupName is not allowed."
        ::= { aaaRadiusGroupEntry 3 }

aaaRadiusGroupStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Set to 1 to initiate the aaaRadiusGroupTable, 2 to destroy the table."
        ::= { aaaRadiusGroupEntry 4 }

aaaTacacsPlusGroupTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF AaaTacacsPlusGroupEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Uses a subset of TACACS+ servers for accounting as defined by the server group"
        ::= { aaaMgt 3 }

aaaTacacsPlusGroupEntry OBJECT-TYPE
        SYNTAX      AaaTacacsPlusGroupEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A conceptual row of aaaTacacsPlusGroupEntry."
        INDEX      { aaaTacacsPlusGroupIndex }
        ::= { aaaTacacsPlusGroupTable 1 }

AaaTacacsPlusGroupEntry ::= SEQUENCE
{
        aaaTacacsPlusGroupIndex          Integer32,
        aaaTacacsPlusGroupServerBitMap   OCTET STRING,
        aaaTacacsPlusGroupName           DisplayString,
        aaaTacacsPlusGroupStatus         ValidStatus
}

aaaTacacsPlusGroupIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Specifies the index for the entry."
        ::= { aaaTacacsPlusGroupEntry 1 }

aaaTacacsPlusGroupServerBitMap OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (1))
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Identifies which TACACS+ sever to use."
        ::= { aaaTacacsPlusGroupEntry 2 }

aaaTacacsPlusGroupName OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Uses a subset of servers for accounting as
        defined by the server group. We can't have the same name as aaaRadiusGroupName"
        ::= { aaaTacacsPlusGroupEntry 3 }

aaaTacacsPlusGroupStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Set to 1 to initiate the aaaRadiusGroupTable, 2 to destroy the table."
        ::= { aaaTacacsPlusGroupEntry 4 }

aaaUpdate OBJECT-TYPE
        SYNTAX      Integer32 (0..2147483647)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Specifies the periodic interim accounting records to be 
                    sent to the accounting server and periodic intervals to 
                    send accounting update records (in minutes). 0 is disable."
        ::= { aaaMgt 4 }

aaaAccountTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF AaaAccountEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Specifies an interface or a set of interfaces that the
                     accounting method list will be applied to."
        ::= { aaaMgt 5 }

aaaAccountEntry OBJECT-TYPE
        SYNTAX      AaaAccountEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A conceptual row of aaaAccountTable."
        INDEX      { aaaAccountIfIndex }
        ::= { aaaAccountTable 1 }

AaaAccountEntry ::= SEQUENCE {
        aaaAccountIfIndex          Integer32,
        aaaAccountMethodName       DisplayString,
        aaaAccountProtocol         INTEGER,
        aaaAccountStatus           ValidStatus
}

aaaAccountIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Defined as the ifIndex"
        ::= { aaaAccountEntry 1 }

aaaAccountMethodName OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Specifies the name of the list of accounting methods to use.
        If no method name is specified, the system uses the default."
        ::= { aaaAccountEntry 2 }

aaaAccountProtocol OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Get the protocol type of a list method to know which server (RADIUS or TACACS+) is in use."
        ::= { aaaAccountEntry 3 }

aaaAccountStatus OBJECT-TYPE
        SYNTAX      ValidStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Set to 1 to initiate the aaaRadiusGroupTable, 2 to destroy the table."
        ::= { aaaAccountEntry 4 }

aaaCommandPrivilegesTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF AaaCommandPrivilegesEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Contains the settings needed for command privileges."
        ::= { aaaMgt 8 }

aaaCommandPrivilegesEntry OBJECT-TYPE
        SYNTAX      AaaCommandPrivilegesEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A conceptual row in the aaaCommandPrivilegesTable."
        INDEX      { aaaCommandPrivilegesLevel, aaaCommandPrivilegesInterfaceIndex }
        ::= { aaaCommandPrivilegesTable 1 }

AaaCommandPrivilegesEntry ::= SEQUENCE {
        aaaCommandPrivilegesLevel            INTEGER,
        aaaCommandPrivilegesInterfaceIndex   INTEGER,
        aaaCommandPrivilegesMethodName       DisplayString
}

aaaCommandPrivilegesLevel OBJECT-TYPE
        SYNTAX       INTEGER (0..15)
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION  "Specifies the privilege level index for the entry."
        ::= { aaaCommandPrivilegesEntry 1 }

aaaCommandPrivilegesInterfaceIndex OBJECT-TYPE
        SYNTAX       INTEGER { console(1), vty(2) }
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION  "Specifies the interface index for the entry."
        ::= { aaaCommandPrivilegesEntry 2 }

aaaCommandPrivilegesMethodName OBJECT-TYPE
        SYNTAX       DisplayString(SIZE(1..255))
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION "Specifies the method name in the lists under
                     the mode of command privileges."
        ::= { aaaCommandPrivilegesEntry 3 }

aaaAccExecTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF AaaAccExecEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Specifies an interface or a set of interfaces that the
                     accounting method list will be applied to."
        ::= { aaaMgt 9 }

aaaAccExecEntry OBJECT-TYPE
        SYNTAX      AaaAccExecEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A conceptual row of aaaAccExecTable."
        INDEX      { aaaAccExecIndex }
        ::= { aaaAccExecTable 1 }

AaaAccExecEntry ::= SEQUENCE {
        aaaAccExecIndex            INTEGER,
        aaaAccExecMethodName       DisplayString
}

aaaAccExecIndex OBJECT-TYPE
        SYNTAX    INTEGER
                  {
                  console(1), vty(2)
                  }
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The method of accessing CLI management."
        ::= { aaaAccExecEntry 1 }

aaaAccExecMethodName OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "Specifies the name of the list of accounting methods to use.
        If no method name is specified, the system uses the default."
        ::= { aaaAccExecEntry 2 }

--
--userAuthMgt
--

userAuthEnablePassword OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..8))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set enable password or delete enable password. NULL is used to
                 delete the enable password. The password is starting with
                 alphanumeric."
    ::= { userAuthMgt 3 }

userAuthMethod OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    local(1),
                    localradius(2),
                    localradiustacacs(3),
                    localtacacs(4),
                    localtacacsradius(5),
                    radius(6),
                    radiuslocal(7),
                    radiuslocaltacacs(8),
                    radiustacacs(9),
                    radiustacacslocal(10),
                    tacacs(11),
                    tacacslocal(12),
                    tacacslocalradius(13),
                    tacacsradius(14),
                    tacacsradiuslocal(15)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set user authencation method for system."
    ::= { userAuthMgt 4 }

userAuthTable OBJECT-TYPE
    SYNTAX SEQUENCE OF UserAuthEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table is for creating the new user."
    ::= { userAuthMgt 5 }

userAuthEntry OBJECT-TYPE
    SYNTAX UserAuthEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Entries in this table correspond to the users entries in system."
    INDEX { userAuthUserName }
    ::= { userAuthTable 1 }

UserAuthEntry ::=
    SEQUENCE {
        userAuthUserName
            DisplayString,
        userAuthPassword
            DisplayString,
        userAuthPrivilege
            Integer32,
        userAuthPublicKey
            DisplayString,
        userAuthStatus
            Integer32
    }

userAuthUserName OBJECT-TYPE
    SYNTAX DisplayString (SIZE (1..8))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The name of the user. The user name is starting with alphanumeric."
    ::= { userAuthEntry 1 }

userAuthPassword OBJECT-TYPE
    SYNTAX DisplayString (SIZE (0..32))
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Specifies the user password. zero length input will set the user enrty
         without password. If the user is not exist, it will create the user
         with the giving password and privilege 0. The password is starting
         with alphanumeric."
   ::= { userAuthEntry 2 }

userAuthPrivilege OBJECT-TYPE
    SYNTAX Integer32 (0..15)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Specifies the user level. If the user is not exist, it will create
         the user with the giving privilege with none password. Privilege 15 is
         maximum privilege that only can be applied to system administrator."
    ::= { userAuthEntry 3 }

userAuthPublicKey OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "User public key, the value can be 'RSA' or 'DSA' or 'Both' or 'None'."
    ::= { userAuthEntry 4 }

userAuthStatus OBJECT-TYPE
    SYNTAX Integer32 (0..1)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "This node is used to create the user entry by '1' and to delete one
         user entry by '0'."
    ::= { userAuthEntry 5 }

aclAttachCtlMgt  OBJECT IDENTIFIER   ::= { aclMgt 13 }

aclAttachCtlIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Index for attachment control. Specifies the ACL as the target
                 to relate with the IP ACE, the MAC ACE or IPv6 ACE. The ACL
                 identified by a particular value of this index  is associated
                 with the same aclEntry as identified by the same value of
                 aclIndex."
    ::= { aclAttachCtlMgt 1 }

aclAttachCtlAceType OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    noType(0),
                    macAce(1),
                    ipAce(2),
                    ipv6Ace(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Type for attachment control. Specifies the type of
                 aclAttachCtlAceIndex to relate with the aclAttachCtlIndex.
                 When the type is macAce(1), the index of aclAceIndexList
                 is the aclMacAceEntry. When the type is ipAce(2), the index
                 of aclAceIndexList is the aclIpAceEntry. When the type is
                 ipv6Ace(3), the index of aclAceIndexList is the
                 aclIpv6AceEntry."
    ::= { aclAttachCtlMgt 2 }

aclAttachCtlAceIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Index for attachment control. Specifies the ACE to relate with
                 the aclAttachCtlIndex. When aclAttachCtlAceType is macAce(1),
                 the value of aclAttachCtlIndex is the diffServMacAceEntry. When
                 aclAttachCtlAceType is ipAce(2), the value of aclAttachCtlIndex
                 is the diffServIpAceEntry. When aclAttachCtlAceType is
                 ipv6Ace(3), the value of aclAttachCtlIndex is the
                 diffServIpv6AceEntry."
    ::= { aclAttachCtlMgt 3 }

aclAttachCtlAction OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    noAction(1),
                    attach(2),
                    detach(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Action for attachment control. When setting this object to
                 attach(2) to begin the attaching operation, a particular ACE
                 is attached to a particular ACL. When setting this object to
                 detach(3) to begin the not attached operation, then a
                 particular ACE is not attached to a particular ACL. When the
                 action is finshed whether successfully or not, or no action
                 is taken, the value of this object always is noAction(1), The
                 value of a particular ACL is specified in the
                 aclAttachCtlAceType and aclAttachCtlAceIndex."
    ::= { aclAttachCtlMgt 4 }

--
-- ipFilterMgt
--

-- ipFilterSnmpInetTable

ipFilterSnmpInetTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF IpFilterSnmpInetEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A list of IP address entries."
    ::= { ipFilterMgt 12 }

ipFilterSnmpInetEntry OBJECT-TYPE
    SYNTAX     IpFilterSnmpInetEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This entry includes an IP address range which the system
         will allow to connect to this device through SNMP."
    INDEX { ipFilterSnmpInetAddressType,
            IMPLIED ipFilterSnmpInetAddressStart}
    ::= { ipFilterSnmpInetTable 1 }

IpFilterSnmpInetEntry ::= SEQUENCE {
    ipFilterSnmpInetAddressType         InetAddressType,
    ipFilterSnmpInetAddressStart        InetAddress,
    ipFilterSnmpInetAddressEnd          InetAddress,
    ipFilterSnmpInetStatus              ValidStatus
}

ipFilterSnmpInetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The type of IP address filter.
                 Only supports IPv4 and IPv6 address types."
    ::= { ipFilterSnmpInetEntry 1 }

ipFilterSnmpInetAddressStart OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The start IP address."
    ::= { ipFilterSnmpInetEntry 2 }

ipFilterSnmpInetAddressEnd OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The end IP address."
    ::= { ipFilterSnmpInetEntry 3 }

ipFilterSnmpInetStatus OBJECT-TYPE
    SYNTAX      ValidStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Setting this to valid(1) creates an entry.
                 Setting this to invalid(2) destroys an entry."
    ::= { ipFilterSnmpInetEntry 4 }

-- ipFilterHttpInetTable

ipFilterHttpInetTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF IpFilterHttpInetEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A list of IP address entries."
    ::= { ipFilterMgt 13 }

ipFilterHttpInetEntry OBJECT-TYPE
    SYNTAX     IpFilterHttpInetEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This entry includes an IP address range which the system
         will allow to connect to this device through SNMP."
    INDEX { ipFilterHttpInetAddressType,
            IMPLIED ipFilterHttpInetAddressStart }
    ::= { ipFilterHttpInetTable 1 }

IpFilterHttpInetEntry ::= SEQUENCE {
    ipFilterHttpInetAddressType         InetAddressType,
    ipFilterHttpInetAddressStart        InetAddress,
    ipFilterHttpInetAddressEnd          InetAddress,
    ipFilterHttpInetStatus              ValidStatus
}

ipFilterHttpInetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The type of IP address filter .
                 Only supports IPv4 and IPv6 address types."
    ::= { ipFilterHttpInetEntry 1 }

ipFilterHttpInetAddressStart OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The start IP address."
    ::= { ipFilterHttpInetEntry 2 }

ipFilterHttpInetAddressEnd OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The end IP address."
    ::= { ipFilterHttpInetEntry 3 }

ipFilterHttpInetStatus OBJECT-TYPE
    SYNTAX      ValidStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Setting this to valid(1) creates an entry.
                 Setting this to invalid(2) destroys an entry."
    ::= { ipFilterHttpInetEntry 4 }

-- ipFilterTelnetInetTable

ipFilterTelnetInetTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF IpFilterTelnetInetEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A list of IP address entries."
    ::= { ipFilterMgt 14 }

ipFilterTelnetInetEntry OBJECT-TYPE
    SYNTAX     IpFilterTelnetInetEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This entry includes an IP address range which the system
         will allow them to connect to this device through SNMP."
    INDEX { ipFilterTelnetInetAddressType,
            IMPLIED ipFilterTelnetInetAddressStart }
    ::= { ipFilterTelnetInetTable 1 }

IpFilterTelnetInetEntry ::= SEQUENCE {
    ipFilterTelnetInetAddressType         InetAddressType,
    ipFilterTelnetInetAddressStart        InetAddress,
    ipFilterTelnetInetAddressEnd          InetAddress,
    ipFilterTelnetInetStatus              ValidStatus
}

ipFilterTelnetInetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The type of IP address filter .
                 Only supports IPv4 and IPv6 address types."
    ::= { ipFilterTelnetInetEntry 1 }

ipFilterTelnetInetAddressStart OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The start IP address."
    ::= { ipFilterTelnetInetEntry 2 }

ipFilterTelnetInetAddressEnd OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The end IP address."
    ::= { ipFilterTelnetInetEntry 3 }

ipFilterTelnetInetStatus OBJECT-TYPE
    SYNTAX      ValidStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Setting this to valid(1) creates an entry.
                 Setting this to invalid(2) destroys an entry."
    ::= { ipFilterTelnetInetEntry 4 }

ipFilterAllClientCtl OBJECT IDENTIFIER ::= { ipFilterMgt 15 }

ipFilterAllClientCtlInetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The type of IP address filter. Only supports IPv4 and IPv6
                 address types."
    ::= { ipFilterAllClientCtl 1 }

ipFilterAllClientCtlInetAddressStart OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The start IP address."
    ::= { ipFilterAllClientCtl 2 }

ipFilterAllClientCtlInetAddressEnd OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The end IP address."
    ::= { ipFilterAllClientCtl 3 }

ipFilterAllClientCtlAction OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    noAction(1),
                    create(2),
                    destroy(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Action for IP filter control. Set this object to create(2) to
                 create entries in the ipFilterSnmpInetTable,
                 ipFilterHttpInetTable and ipFilterTelnetInetTable. Set this
                 object to destroy(3) to destroy specified entries in the
                 ipFilterSnmpInetTable, ipFilterHttpInetTable and
                 ipFilterTelnetInetTable. When the action is finshed, whether
                 successfully or not, or no action is taken, the value of this
                 object is always noAction(1)."
    ::= { ipFilterAllClientCtl 4 }

--
-- dot1xMgt
--

-- The extension table of dot1xAuthConfigTable

dot1xAuthConfigExtTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF Dot1xAuthConfigExtEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The extension table of dot1xAuthConfigTable."
        ::= { dot1xMgt 1 }

dot1xAuthConfigExtEntry OBJECT-TYPE
        SYNTAX      Dot1xAuthConfigExtEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The entry of dot1xAuthConfigExtTable."
        AUGMENTS       { dot1xAuthConfigEntry }
        ::= { dot1xAuthConfigExtTable 1 }

Dot1xAuthConfigExtEntry ::= SEQUENCE
{
      dot1xAuthConfigExtOperMode              INTEGER,
      dot1xAuthConfigExtMultiHostMaxCnt       Integer32,
      dot1xAuthConfigExtPortIntrusionAction   INTEGER
}

dot1xAuthConfigExtOperMode OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        singleHost(1),
                        multiHost(2),
                        macBasedAuth(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The operation mode of dot1x port which allows host
                     connection to 802.1x-authorized ports."
        ::= { dot1xAuthConfigExtEntry 1 }

dot1xAuthConfigExtMultiHostMaxCnt OBJECT-TYPE
        SYNTAX      Integer32(1..1024)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The maximum number of hosts when the
                     dot1xAuthConfigExtOperMode is multiHost(2). When the
                     operation Mode is singleHost(1), we can ignore this
                     variables."
        DEFVAL      { 5 }
        ::= { dot1xAuthConfigExtEntry 2  }

dot1xAuthConfigExtPortIntrusionAction      OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    block-traffic(1),
                    guest-vlan(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Responses to intrusion when the authentication is failed;
                 block-traffic(1) means that to block traffic when the authentication is failed and
                 guest-vlan(2) means that to join to a guest VLAN when the authentication is failed."
    ::= { dot1xAuthConfigExtEntry 3 }

dot1xEapolPassThrough OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "When this variable is enabled(1), EAPOL frames will
                     be forwarded to all ports where the Spanning Tree
                     status is forwarding. When this variable is
                     disabled(2), EAPOL frames will be discarded. EAPOL
                     Pass-Through operates when the global status of
                     802.1X is disabled."
        DEFVAL      { disabled }
        ::= { dot1xMgt 3 }

--
-- networkAccessPortTable
--

networkAccessPortTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF NetworkAccessPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A table contains the information of network access about every port."
    ::= { networkAccessMgt 2 }

networkAccessPortEntry   OBJECT-TYPE
    SYNTAX      NetworkAccessPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A conceptual row in the networkAccessPort table."
    INDEX { networkAccessPortPortIndex }
    ::= { networkAccessPortTable 1 }

NetworkAccessPortEntry ::= SEQUENCE
{
    networkAccessPortPortIndex              Integer32,
    networkAccessPortDynamicVlan            EnabledStatus,
    networkAccessPortMaxMacCount            INTEGER,
    networkAccessPortMode                   EnabledStatus,
    networkAccessPortMacFilter              INTEGER,
    networkAccessPortGuestVlan              INTEGER,
    networkAccessPortLinkDetectionStatus    EnabledStatus,
    networkAccessPortLinkDetectionMode      INTEGER,
    networkAccessPortLinkDetectionAciton    INTEGER,
    networkAccessPortDynamicQos             EnabledStatus
}

networkAccessPortPortIndex      OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The port and the trunk (excluding trunk members) interface of the
                 portTable. The interface identified by a particular value of this port
                 index is the same interface identified by the same value of
                 ifIndex in the IF-MIB."
    ::= { networkAccessPortEntry 1 }

networkAccessPortDynamicVlan OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Sets enabled(1) to enable dynamic VLAN assigment and
                 sets disabled(2) to disable dynamic VLAN assigment."
    ::= { networkAccessPortEntry 2 }

networkAccessPortMaxMacCount      OBJECT-TYPE
    SYNTAX      INTEGER (0..1024)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the maximum number of authenticated MAC address."
    ::= { networkAccessPortEntry 3 }

networkAccessPortMode OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the secure port mode. enabled(1) means that Mac address
                 authentication is used and disabled(2) means that the authentication is disabled."
    ::= { networkAccessPortEntry 4 }

networkAccessPortMacFilter OBJECT-TYPE
    SYNTAX      INTEGER (0..64)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the MAC filter ID, Set this variable to zero to
                 disable MAC filter."
    ::= { networkAccessPortEntry 5 }

networkAccessPortGuestVlan      OBJECT-TYPE
    SYNTAX      INTEGER (0..4094)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the guest VLAN ID. To disable the VLAN, set the value to 0."
    ::= { networkAccessPortEntry 6 }

networkAccessPortLinkDetectionStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set this object to enabled(1) to enable link detection.
                 Set this object to disabled(2) to disable link detection."
    ::= { networkAccessPortEntry 7 }

networkAccessPortLinkDetectionMode OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    linkUp(1),
                    linkDown(2),
                    linkUpDown(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the detection event for a port. Set this object
                 to linkUp(1) to detect a link-up event. Set this object
                 to linkDown(2) to detect a link-down event. Set this
                 object to linkUpDown(3) to detect both link up and
                 link down events."
    ::= { networkAccessPortEntry 8 }

networkAccessPortLinkDetectionAciton OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    trap(1),
                    shutDown(2),
                    trapAndShutDown(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the action to take when a networkAccessPortLinkDetection
                 event is triggered. Set this object to trap(1) to send a trap
                 when a networkAccessPortLinkDetection event is triggered.
                 Set this object to shutDown(2) to shut down the port when a
                 networkAccessPortLinkDetection event is triggered. Set this object
                 to trapAndShutDown(3) to send a trap and shut down the port when a
                 networkAccessPortLinkDetection event is triggered."
    ::= { networkAccessPortEntry 9 }

networkAccessPortDynamicQos OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set this object to enabled(1) to enable Dynamic QoS.
                 Set this object to disabled(2) to disable Dynamic QoS."
    ::= { networkAccessPortEntry 10 }

--
-- networkAccessClearMacAddressMgt
--

networkAccessClearMacAddressMgt           OBJECT IDENTIFIER ::= { networkAccessMgt 3 }

networkAccessClearMacAddressAttribute     OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    all        (1),
                    static     (2),
                    dynamic    (3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Attribute for clearing Mac address. Specifies the certain attribute
                 in Mac address table. all(1) indicates both reauthorized and learnt
                 secure MAC address; static(2) indicates reauthorized MAC address;
                 dynamic(3) indicates learnt secure MAC address."
    ::= { networkAccessClearMacAddressMgt 1 }

networkAccessClearMacAddressMacAddress     OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies MAC address in the MAC address table for clearing
                 MAC address. '000000' represents that no MAC address is specified."

    ::= { networkAccessClearMacAddressMgt 2 }

networkAccessClearMacAddressPort     OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The specifies port in the MAC address table for clearing MAC address.
                 '0' represents that no port is specified."

    ::= { networkAccessClearMacAddressMgt 3 }

networkAccessClearMacAddressAction     OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    noclear     (1),
                    clear       (2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Action for clearing MAC address . When setting this object to clear(2)
                           to begin the clearing MAC address operation, a particular MAC address
                           is cleared from the MAC address table. When the action is finshed whether
                           or not it is successful or no action is taken, the value of this object
                           is always noclear(1)."

    ::= { networkAccessClearMacAddressMgt 4 }

--
-- networkAccessMacAddressTable
--

networkAccessMacAddressTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF NetworkAccessMacAddressEntry
    MAX-ACCESS  not-accessible
	STATUS      current
	DESCRIPTION "Contains the information of network access MAC addresses."
	::= { networkAccessMgt 4 }

networkAccessMacAddressEntry   OBJECT-TYPE
    SYNTAX      NetworkAccessMacAddressEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A conceptual row in the networkAccessMacAddress table."
    INDEX { networkAccessMacAddressAddress, networkAccessMacAddressPort }
    ::= { networkAccessMacAddressTable 1 }

NetworkAccessMacAddressEntry ::= SEQUENCE
{
    networkAccessMacAddressAddress                       MacAddress,
    networkAccessMacAddressPort                          INTEGER,
    networkAccessMacAddressInetAddressType               InetAddressType,
    networkAccessMacAddressRadiusServerInetAddress       InetAddress,
    networkAccessMacAddressTime                          DisplayString,
    networkAccessMacAddressAttribute                     INTEGER
}

networkAccessMacAddressAddress      OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Specifies the authenticated MAC address."
    ::= { networkAccessMacAddressEntry 1 }

networkAccessMacAddressPort      OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Specifies the port of authenticated MAC address."
    ::= { networkAccessMacAddressEntry 2 }

networkAccessMacAddressInetAddressType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This object indicates the type of IP address denoted in
                 networkAccessMacAddressRadiusServerInetAddress type."
    ::= { networkAccessMacAddressEntry 3 }

networkAccessMacAddressRadiusServerInetAddress      OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Displays the IP address of radius server that authenticates
                 the specified Mac address."
    ::= { networkAccessMacAddressEntry 4 }

networkAccessMacAddressTime      OBJECT-TYPE
    SYNTAX      DisplayString(SIZE(12))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Displays the authentication time of the authenticated MAC address.
                 The following form is a text string; 'yyyy MMm DDd HHh MMm SSs'.
                 'yyyy' is a four-digit year. 'MM' is a month. A single-digit month is
                 preceded by a zero. 'DD' is the day of a month. A single-digit day
                 is preceded by the value zero. 'HH', 'MM' and 'SS' are hour,
                 minute, and second respectively. A single-digit hour, minute,
                 and second are preceded by a zero value. An example is:
                 '2001y 01m 01d 00h 04m 43s'."
    ::= { networkAccessMacAddressEntry 5 }

networkAccessMacAddressAttribute       OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    static     (1),
                    dynamic    (2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Displays the attribute of an authenticated MAC address.
                 static(1) indicates resauthorized secure MAC address.
                 dynamic(2) indicates learnt secure MAC address."
    ::= { networkAccessMacAddressEntry 6 }

networkAccessAging       OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set this object to enabled(1) to enable MAC address aging feature.
                 Set this object to disabled(2) to disable MAC address aging feature."
    ::= { networkAccessMgt 5 }

--
-- networkAccessMacFilterWithMaskTable
--

networkAccessMacFilterWithMaskTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF NetworkAccessMacFilterWithMaskEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Contains the settings for MAC filter."
 ::= { networkAccessMgt 6 }

networkAccessMacFilterWithMaskEntry OBJECT-TYPE
    SYNTAX      NetworkAccessMacFilterWithMaskEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A conceptual row in the networkAccessMacFilterWithMaskTable."
    INDEX { networkAccessMacFilterWithMaskID,
            networkAccessMacFilterWithMaskMacAddress,
            networkAccessMacFilterWithMaskMacAddressMask }
    ::= { networkAccessMacFilterWithMaskTable 1 }

NetworkAccessMacFilterWithMaskEntry ::= SEQUENCE
{
    networkAccessMacFilterWithMaskID                INTEGER,
    networkAccessMacFilterWithMaskMacAddress        MacAddress,
    networkAccessMacFilterWithMaskMacAddressMask    MacAddress,
    networkAccessMacFilterWithMaskStatus            INTEGER
}

networkAccessMacFilterWithMaskID OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Specifies the MAC filter ID."
    ::= { networkAccessMacFilterWithMaskEntry 1 }

networkAccessMacFilterWithMaskMacAddress OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Specifies the MAC address to be filtered."
    ::= { networkAccessMacFilterWithMaskEntry 2 }

networkAccessMacFilterWithMaskMacAddressMask OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Specifies the MAC mask to be filtered."
    ::= { networkAccessMacFilterWithMaskEntry 3 }

networkAccessMacFilterWithMaskStatus OBJECT-TYPE
    SYNTAX      ValidStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Set this object to valid(1) to create an entry.
                 Set this object to invalid(2) to destroy an entry."
    ::= { networkAccessMacFilterWithMaskEntry 4 }

macAuthReauthTime     OBJECT-TYPE
    SYNTAX      Integer32 (120..1000000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the reauthentication time period."
    ::= { macAuthMgt 1 }

--
-- macAuthPortTable
--

macAuthPortTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF MacAuthPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Contains the settings for mac authentication of each port."
    ::= { macAuthMgt 2 }

macAuthPortEntry   OBJECT-TYPE
    SYNTAX      MacAuthPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A conceptual row in the macAuthPort table."
    INDEX { macAuthPortIndex }
    ::= { macAuthPortTable  1 }

MacAuthPortEntry ::= SEQUENCE
{
    macAuthPortIndex              Integer32,
    macAuthPortMaxMacCount        INTEGER,
    macAuthPortIntrusionAction    INTEGER
}

macAuthPortIndex      OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The port and the trunk (including trunk members) interface of the
                 port table. The interface identified by a particular value of this
                 index is the same interface identified by the same value
                 of ifIndex in the IF-MIB."
    ::= { macAuthPortEntry  1 }

macAuthPortMaxMacCount      OBJECT-TYPE
    SYNTAX      INTEGER (0..1024)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the maximum number of authenticated MAC addresses for MAC authentication."
    ::= { macAuthPortEntry 2 }

macAuthPortIntrusionAction      OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    block-traffic(1),
                    pass-traffic(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Responses to intrusion when the authentication is failed.
                 block-traffic(1) : denies network access to an unauthorized client;
                 pass-traffic(2) : allows unauthorized clients to the access network."
    ::= { macAuthPortEntry  3 }

webAuthSystemAuthControl     OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Sets enabled(1) to enable WebAuth feature and
                 sets disabled(2) to disable WebAuth feature."
    ::= { webAuthMgt 1 }

webAuthSessionTimeout     OBJECT-TYPE
    SYNTAX      INTEGER (0|300..3600)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Successfully authenticated users can use Internet
                 service for a certain period. Whenever this period expires,
                 users need to be re-authenticated. This period is
                 called the session time.
                 Set this value to 0 to disable the session timeout."
    ::= { webAuthMgt 5 }

webAuthQuietPeriod    OBJECT-TYPE
    SYNTAX      INTEGER (1..180)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the re-authentication interval when the authentication
             fail attempts reach the webAuthLoginAttempts value. Unauthenticated
             user won't be authenticated during this period."
    ::= { webAuthMgt 6 }

webAuthLoginAttempts    OBJECT-TYPE
    SYNTAX      INTEGER (1..3)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the counter that configures the authentication fail times
                 for a client. If authentication fail times reaches the specified
                 value, the client are not allowed to login for some period."
    ::= { webAuthMgt 7 }

--
-- webAuthReauthenticateMgt
--

webAuthReauthenticateMgt             OBJECT IDENTIFIER ::= { webAuthMgt 8 }

webAuthReauthenticatePort     OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the port to re-authenticate for all of its
                 authenticated hosts."
    ::= { webAuthReauthenticateMgt 1 }

webAuthReauthenticateInetAddressType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies host type to re-authenticate."
    ::= { webAuthReauthenticateMgt 2 }

webAuthReauthenticateInetAddress     OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specificies host to re-authenticate."
    ::= { webAuthReauthenticateMgt 3 }

webAuthReauthenticateAction     OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    noReauth     (1),
                    reauth       (2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Action for WebAuth re-authenication. When setting this object to
                 reauth(2) to begin the re-authenticated operation, a particular
                 user is re-authenticated. When the action is finshed whether it is
                 successfully, or no action is taken, the value of this
                 object is always noReauth(1)."
    ::= { webAuthReauthenticateMgt 4 }

--
-- webAuthPortConfigTable
--

webAuthPortConfigTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF WebAuthPortConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Contains the settings for web authentication of each port."
    ::= { webAuthMgt 9 }

webAuthPortConfigEntry   OBJECT-TYPE
    SYNTAX      WebAuthPortConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A conceptual row in the webAuthPortConfigTable."
    INDEX { webAuthPortConfigPortIndex }
    ::= { webAuthPortConfigTable  1 }

WebAuthPortConfigEntry ::= SEQUENCE
{
    webAuthPortConfigPortIndex                     INTEGER,
    webAuthPortConfigStatus                        INTEGER,
    webAuthPortConfigAuthenticatedHostCount        INTEGER
}

webAuthPortConfigPortIndex      OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The port number of the port that may specify certain entry in the table which contains web                            authentication information."
    ::= { webAuthPortConfigEntry  1 }

webAuthPortConfigStatus     OBJECT-TYPE
    SYNTAX     EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Sets enabled(1) to enable web authentication feature for each port and
                 sets disabled(2) to disable web authentication for each port."
    ::= { webAuthPortConfigEntry 2 }

webAuthPortConfigAuthenticatedHostCount      OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Displays the authenticated host counts for each port"
    ::= { webAuthPortConfigEntry 3 }

--
-- webAuthPortInfoTable
--

webAuthPortInfoTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF WebAuthPortInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Contains the information for web authentication of each port."
    ::= { webAuthMgt 10 }

webAuthPortInfoEntry   OBJECT-TYPE
    SYNTAX      WebAuthPortInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A conceptual row in the webAuthPortTable."
    INDEX { webAuthPortInfoPortIndex, webAuthPortInfoPortAuthSuccessIndex}
    ::= { webAuthPortInfoTable 1 }

WebAuthPortInfoEntry ::= SEQUENCE
{
    webAuthPortInfoPortIndex                  INTEGER,
    webAuthPortInfoPortAuthSuccessIndex       INTEGER,
    webAuthPortInfoInetAddressType            InetAddressType,
    webAuthPortInfoInetAddress                InetAddress,
    webAuthPortInfoRemainingSessiontime       INTEGER,
    webAuthPortInfoStatus                     INTEGER
}

webAuthPortInfoPortIndex      OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The port number for which this entry contains web authentication information."
    ::= { webAuthPortInfoEntry  1 }

webAuthPortInfoPortAuthSuccessIndex      OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The authentication success number of port for which this entry contains web authentication information."
    ::= { webAuthPortInfoEntry  2 }

webAuthPortInfoInetAddressType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This object indicates the type of IP address denoted in webAuthPortInfoIpAddress type."
    ::= { webAuthPortInfoEntry  3 }

webAuthPortInfoInetAddress      OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The IP address which may specify the entry containing web authentication information."
    ::= { webAuthPortInfoEntry  4 }

webAuthPortInfoRemainingSessiontime      OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
   DESCRIPTION "The remaining session time for authenticated hosts. During this
                period, they may use internet resource. When the session time expires, they
                will need to re-authenticate again."

    ::= { webAuthPortInfoEntry 5 }

webAuthPortInfoStatus    OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    authenticated      (1)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Displays the web authentication status for each port.
                 authenticated (1) means the user is authenticated."
    ::= { webAuthPortInfoEntry 6 }

--
-- sysLogMgt
--

-- Management for system log. This configures the logging
-- of events inside the switch.

sysLogStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Whether the system log is enabled."
        ::= { sysLogMgt 1 }

sysLogHistoryFlashLevel OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Severity level for logging to flash."
        ::= { sysLogMgt 2 }

sysLogHistoryRamLevel OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Severity level for logging to RAM."
        ::= { sysLogMgt 3 }

--
--remoteLogMgt
--

remoteLogMgt OBJECT IDENTIFIER ::= { sysLogMgt 6 }

remoteLogStatus OBJECT-TYPE
       SYNTAX      EnabledStatus
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION "Whether the remote log system is enabled."
       ::= { remoteLogMgt 1 }

remoteLogLevel OBJECT-TYPE
        SYNTAX      Integer32 (0..7)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Severity level for remote log."
        ::= { remoteLogMgt 2 }

remoteLogFacilityType OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                      localUse0(16),
                      localUse1(17),
                      localUse2(18),
                      localUse3(19),
                      localUse4(20),
                      localUse5(21),
                      localUse6(22),
                      localUse7(23)
                     }
        MAX-ACCESS   read-write
        STATUS       current
        DESCRIPTION " The facility type for remote log."
        ::= { remoteLogMgt 3 }

--remoteLogServerInetTable

remoteLogServerInetTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RemoteLogServerInetEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table for storing the remote log server list."
        ::= { remoteLogMgt 7 }

remoteLogServerInetEntry OBJECT-TYPE
        SYNTAX      RemoteLogServerInetEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A conceptual row for remoteLogServerInetTable."
        INDEX { remoteLogServerInetAddressType,
                IMPLIED remoteLogServerInetAddress}
        ::= { remoteLogServerInetTable 1 }

RemoteLogServerInetEntry ::= SEQUENCE
{
    remoteLogServerInetAddressType  InetAddressType,
    remoteLogServerInetAddress      InetAddress,
    remoteLogServerStatus ValidStatus
}

remoteLogServerInetAddressType OBJECT-TYPE
    SYNTAX       InetAddressType
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION  "Indicates the type of address
                 denoted in remoteLogServerInetAddress type.
                 Only ipv4(1), ipv6(2) and ipv6z(4)
                 types are supported."

    ::= { remoteLogServerInetEntry 1 }

remoteLogServerInetAddress OBJECT-TYPE
    SYNTAX       InetAddress
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION "The IP address of the remote log Server."
    ::= { remoteLogServerInetEntry 2 }

remoteLogServerStatus OBJECT-TYPE
         SYNTAX      ValidStatus
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION  "Setting this to valid(1) creates an entry.
                       Setting this to invalid(2) destroys an entry."
         ::= { remoteLogServerInetEntry 3 }

--
-- smtpMgt
--

smtpMgt   OBJECT IDENTIFIER ::= { sysLogMgt 7 }

smtpStatus OBJECT-TYPE
    SYNTAX       EnabledStatus
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION "Set enabled(1) to enable the SMTP, set disabled(2) to disable
                 the SMTP."
    ::= { smtpMgt 1 }

smtpSeverityLevel OBJECT-TYPE
    SYNTAX       Integer32 (0..7)
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION "Specify the SMTP minimum severity level to send the event message."
    ::= { smtpMgt 2 }

smtpSourceEMail OBJECT-TYPE
    SYNTAX       DisplayString (SIZE(0..41))
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION "SMTP source email address,
                the sender's mail address that appears
                in the 'From' field of the mail."
    ::= { smtpMgt 3 }

--smtpServerIpTable

smtpServerIpTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF SmtpServerIpEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The SMTP server IP table.
                    The maximum servers to be added is 3."
       ::= { smtpMgt 4 }

smtpServerIpEntry OBJECT-TYPE
       SYNTAX      SmtpServerIpEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "A conceptual row of the smtpServerIpTable."
       INDEX  { smtpServerIp }
       ::= { smtpServerIpTable 1 }

SmtpServerIpEntry ::= SEQUENCE
{
    smtpServerIp     IpAddress,
    smtpServerIpStatus ValidStatus
}

smtpServerIp OBJECT-TYPE
       SYNTAX      IpAddress
       MAX-ACCESS  accessible-for-notify
       STATUS      current
       DESCRIPTION "SMTP mail server's IP address."
       ::= { smtpServerIpEntry 1 }

smtpServerIpStatus OBJECT-TYPE
       SYNTAX      ValidStatus
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION "Setting this to valid(1) creates an entry.
                       Setting this to invalid(2) destroys an entry."
       ::= { smtpServerIpEntry 2 }

--smtpDestEMailTable

smtpDestEMailTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF SmtpDestEMailEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The table of the destination e-mail address.
                    The maximum numbers of destination email address to be added is 5."
       ::= { smtpMgt 5 }

smtpDestEMailEntry OBJECT-TYPE
       SYNTAX      SmtpDestEMailEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "A conceptual row of the smtpDestEMailTable."
       INDEX  { smtpDestEMail }
       ::= { smtpDestEMailTable 1 }

SmtpDestEMailEntry ::= SEQUENCE
{
    smtpDestEMail     DisplayString,
    smtpDestEMailStatus ValidStatus
}

smtpDestEMail OBJECT-TYPE
       SYNTAX      DisplayString (SIZE(0..41))
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "SMTP destination e-mail address."
       ::= { smtpDestEMailEntry 1 }

smtpDestEMailStatus OBJECT-TYPE
       SYNTAX      ValidStatus
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION "Setting this to valid(1) creates an entry.
                       Setting this to invalid(2) destroys an entry."
       ::= { smtpDestEMailEntry 2 }

--
-- lineMgt
--

-- Management for line. This includes management for
-- serial line (RS232 port) and Telnet.

consoleMgt           OBJECT IDENTIFIER ::= { lineMgt 1 }
telnetMgt            OBJECT IDENTIFIER ::= { lineMgt 2 }
vtyMgt               OBJECT IDENTIFIER ::= { lineMgt 3 }

--consoleMgt

consoleDataBits OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                      databits7(1),
                      databits8(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Number of data bits."
        ::= { consoleMgt 1 }

consoleParity OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                     partyNone(1),
                     partyEven(2),
                     partyOdd(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Defines the generation of a parity bit."
        ::= { consoleMgt 2 }

consoleBaudRate OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                     baudRate9600(1),
                     baudRate19200(2),
                     baudRate38400(3),
                     baudRate57600(4),
                     baudRate115200(5)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Baud rate: Valid values are 115200, 57600, 38400,
                     19200, and 9600."
        ::= { consoleMgt 3 }

consoleStopBits OBJECT-TYPE
        SYNTAX     INTEGER
                   {
                    stopbits1(1),
                    stopbits2(2)
                   }
        MAX-ACCESS read-write
        STATUS     current
        DESCRIPTION "The console stop bits, valid values are stopbits1(1) or stopbits2(2)"
        ::= { consoleMgt 4 }

consoleExecTimeout OBJECT-TYPE
        SYNTAX      Integer32 (0..65535)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "In a serial console, use the consoleExecTimeout
                     variable to set the interval that the EXEC command
                     interpreter waits until user input is detected;
                     set the value to 0 to disable it."
        ::= { consoleMgt 5 }

consolePasswordThreshold OBJECT-TYPE
        SYNTAX      Integer32 (0..120)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The number of failed console logon attempts that may be
                     made before the system will not accept a further attempt
                     in the time specified by consoleSilentTime. A value of 0
                     disables the functionality."
        ::= { consoleMgt 6 }

consoleSilentTime OBJECT-TYPE
        SYNTAX      Integer32 (0..65535)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The length of time that the management console is
                     inaccessible after the number of failed logon
                     attempts has reached consolePasswordThreshold. A value
                     of 0 disables the functionality."

        ::= { consoleMgt 7 }

--to set login timeout seconds
consoleLoginResponseTimeout OBJECT-TYPE
        SYNTAX      Integer32(0..300)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION  "Console login response timeout setting.
                     Valid range is 0 to 300. Setting to 0 means disabled."
        ::= { consoleMgt 10 }

-- telnetMgt

telnetStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "To enable or disable the telnet function. Any new telnet
                     request will be rejected and all current telnet sessions
                     will be terminated if this status is set to disabled(2)."
        DEFVAL      { enabled }
        ::= { telnetMgt 4 }

telnetPortNumber OBJECT-TYPE
        SYNTAX      Integer32 (1..65535)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The telnet session port number."
        DEFVAL { 23 }
        ::= { telnetMgt 5 }

-- vtyMgt

vtyExecTimeout OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the interval that the system waits for user input
                 before terminating the current session."
    ::= { vtyMgt 1 }

vtyPasswordThreshold OBJECT-TYPE
    SYNTAX      Integer32 (0..120)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The number of failed logon attempts that may be made before the
                 system will not accept a further attempt to log on."
    ::= { vtyMgt 2 }

vtyLoginResponseTimeout OBJECT-TYPE
    SYNTAX      Integer32(0..300)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Login response timeout setting. Setting to 0 means disabled."
    ::= { vtyMgt 3 }

vtyMaxSession OBJECT-TYPE
    SYNTAX      Integer32 (0..4)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The maximum number of allowed sessions."
    DEFVAL      { 4 }
    ::= { vtyMgt 4 }

vtySilentTime OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The time the system waits before etablishing a new session
                 after the number of failed logins reaches the specified limit."
    ::= { vtyMgt 5 }

--
-- sysTimeMgt
--

sntpMgt          OBJECT IDENTIFIER ::= { sysTimeMgt 1 }

sntpStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set enabled(1) to enable the SNTP, set disabled(2) to disable
                 the SNTP."
    ::= { sntpMgt 1 }

sntpServiceMode OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    unicast(1)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Service mode."
    ::= { sntpMgt 2 }

sntpPollInterval OBJECT-TYPE
    SYNTAX      Integer32(16..16384)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Polling interval."
    ::= { sntpMgt 3 }

sntpServerTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF SntpServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for SNTP servers. IP addresses
                     must occupy contiguous indexes, starting from 1.
                     If a removed entry is not the last entry, the table
                     will be shifted to contiguous indexes automatically."
        ::= { sntpMgt 4 }

sntpServerEntry OBJECT-TYPE
        SYNTAX      SntpServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for SNTP servers."
        INDEX       { sntpServerIndex }
        ::= { sntpServerTable 1 }

SntpServerEntry ::= SEQUENCE
{
    sntpServerIndex Integer32,
    sntpServerInetAddressType       InetAddressType,
    sntpServerInetAddress           InetAddress,
    sntpServerStatus                ValidStatus
}


sntpServerIndex OBJECT-TYPE
    SYNTAX      Integer32 (1..3)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of a server."
    ::= { sntpServerEntry 1 }

sntpServerInetAddressType OBJECT-TYPE
    SYNTAX       InetAddressType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION  "Indicates the type of address
                 denoted in sntpServerInetAddress type.
                 Only ipv4(1), ipv6(2) and ipv6z(4)
                 types are supported."

    ::= { sntpServerEntry 4 }

sntpServerInetAddress OBJECT-TYPE
    SYNTAX       InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The IP address of a time server."
    ::= { sntpServerEntry 5 }

sntpServerStatus OBJECT-TYPE
         SYNTAX      ValidStatus
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION  "Setting this to valid(1) creates an entry.
                       Setting this to invalid(2) destroys an entry."
         ::= { sntpServerEntry 6 }

sysCurrentTime OBJECT-TYPE
     SYNTAX      DisplayString(SIZE(20))
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION "This is a text string in the following form, based on Unix:
                  'Mmm _d hh:mm:ss yyyy'. 'Mmm' are the first three letters
                  of the English name of the month. '_d' is the day of month.
                  A single-digit day is preceded by a space. 'hh:mm:ss' is
                  a 24-hour representations of hours, minutes, and seconds.
                  A single-digit hour is preceded by a zero. 'yyyy' is a
                  four-digit year. An example is: 'Jan  1 02:03:04 2002'."
     ::= { sysTimeMgt 2 }

sysTimeZone OBJECT-TYPE
     SYNTAX      DisplayString(SIZE(6))
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION "This is a text string in the following form: '[s]hh:mm'.
                  '[s]' is a plus-or-minus sign. For UTC, this is omitted.
                  For a positive offset, this is '+'. For a negative offset,
                  this is '-'. 'hh:mm' in the hour and minute offset from UTC.
                  A single-digit hour is preceded by a zero. When
                  sysTimeZonePredefined object is set to any value other than
                  none(1), this object will be empty string."
     ::= { sysTimeMgt 3 }

sysTimeZoneName OBJECT-TYPE
     SYNTAX      DisplayString(SIZE(1..30))
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION "The name of the time zone. When sysTimeZonePredefined object
                  is set to any value other than none(1), this object will be
                  empty string."
     ::= { sysTimeMgt 4 }

--
-- fileMgt
--

-- Management for File System Manipulate, including files copy, display and delete.

fileCopyMgt OBJECT IDENTIFIER ::= { fileMgt 1 }
fileInfoMgt OBJECT IDENTIFIER ::= { fileMgt 2 }
fileAutoUpgradeMgt OBJECT IDENTIFIER ::= { fileMgt 4 }

--
-- This performs the copy operation.
--

fileCopySrcOperType OBJECT-TYPE
    SYNTAX     INTEGER
               {
                 file(1),
                 runningCfg(2),
                 startUpCfg(3),
                 tftp(4),
                 unit(5),
                 http(6),
                 ftp(7)
                }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The Copy Operation that we want to perform on the
                 fileCopyDestOperType, this operation is similar to the CLI
                 command 'copy fileCopySrcOperType fileCopyDestOperType'.
                 file(1) means we want to perform the 'copy file fileCopyDestType'
                 operation, runningCfg(2) means we want to perform the
                 'copy running-config fileCopyDestOperType' operation,
                 startUpCfg(3) means we want to perform the
                 'copy startup-config fileCopyDestOperType' operation, tftp(4) means
                 we want to perform the 'copy tftp fileCopyDestOperType' operation,
                 unit(5) is only available in stacking systems, in which we
                 can copy files from one unit to another unit and it means
                 we want to perform the 'copy unit fileCopyDestOperType' operation.
                 http(6) means we can read the status of the transfer via
                 HTTP protocol, but can not change the status.
                 ftp(7) means we want to perform 'copy ftp fileCopyDestOperType'
                 operation.

                 The possible permutations are as follows: (1) copy file file;
                 (2) copy file runningCfg; (3) copy file startUpCfg;
                 (4) copy file tftp; (5) copy file unit (for stacking systems only);
                 (6) copy runningCfg file; (7) copy runningCfg startUpCfg;
                 (8) copy runningCfg tftp; (9) copy startupCfg file;
                 (10) copy startupCfg runningCfg; (11)copy startupCfg tftp;
                 (12) copy tftp file; (13) copy tftp runningCfg;
                 (14) copy tftp startUpCfg; (15) copy unit file;
                 (16) copy file ftp; (17) copy running-config ftp;
                 (18) copy startup-config ftp; (19) copy ftp file;
                 (20) copy ftp running-config; (21) copy ftp startup-config"
    ::= { fileCopyMgt 1}

fileCopySrcFileName OBJECT-TYPE
    SYNTAX     DisplayString (SIZE(0..127))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The source file name for fileCopyMgt when a copy
        operation is next requested via this MIB.  This value is set to
        a zero length string when no file name has been specified.
        Note: If the fileCopySrcOperType is runningCfg(2) or startUpCfg(3),
        this variable can be ignored."
    ::= { fileCopyMgt 2 }

fileCopyDestOperType OBJECT-TYPE
    SYNTAX     INTEGER
               {
                 file(1),
                 runningCfg(2),
                 startUpCfg(3),
                 tftp(4),
                 unit(5),
                 http(6),
                 ftp(7)
                }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The Copy Operation that we want to perform on
                 fileCopySrcOperType, this operation is similar to the CLI
                 command 'copy fileCopySrcOperType fileCopyDestOperType'.
                 file(1) means we want to perform the 'copy fileCopySrcType file '
                 operation, runningCfg(2) means we want to perform the
                 'copy fileCopySrcOperType running-config ' operation,
                 startUpCfg(3) means we want to perform the
                 'copy fileCopySrcOperType startup-config ' operation, tftp(4) means
                 we want to perform the 'copy fileCopySrcOperType tftp' operation,
                 unit(5) is only available in stacking systems in which we
                 can copy files from one unit to another unit. It means
                 we want to perform the 'copy fileCopySrcOperType unit' operation.
                 http(6) means we can read the status of the transfer via
                 HTTP protocol, but can not change the status.
                 ftp(7) means we want to perform 'copy fileCopySrcOperType ftp'
                 operation.

                 The possible permutations are as follows: (1) copy file file;
                 (2) copy file runningCfg; (3) copy file startUpCfg;
                 (4) copy file tftp; (5) copy file unit (for stacking system only);
                 (6) copy runningCfg file; (7) copy runningCfg startUpCfg;
                 (8) copy runningCfg tftp; (9) copy startupCfg file;
                 (10) copy startupCfg runningCfg; (11) copy startupCfg tftp;
                 (12) copy tftp file; (13) copy tftp runningCfg;
                 (14) copy tftp startUpCfg; (15) copy unit file;
                 (16) copy file ftp; (17) copy running-config ftp;
                 (18) copy startup-config ftp; (19) copy ftp file;
                 (20) copy ftp running-config; (21) copy ftp startup-config"
    ::= { fileCopyMgt 3 }

fileCopyDestFileName  OBJECT-TYPE
    SYNTAX     DisplayString (SIZE(0..127))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The destination file name for fileCopyMgt when a
        copy operation is next requested via this MIB.  This value is set to
        a zero length string when no file name has been specified.
        Note: If the fileCopyDestOperType is runningCfg(2) or startupCfg(3),
        this variable can be ignored."
    ::= { fileCopyMgt 4 }

fileCopyFileType  OBJECT-TYPE
    SYNTAX     INTEGER {
                  opcode(1),
                  config(2),
                  bootRom(3),
                  loader(5)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Type of file to copy in fileCopyMgt. opcode(1) indicates operation
         code, config(2) indicates configuration file, bootRom(3) indicates
         diagnostic image file and loader(5) indicates loader image file. If
         the fileCopySrcOperType or fileCopyDestOperType is either runningCfg(2)
         or startupCfg(3), this variable can be ignored. bootRom(3) and
         loader(5) can be set only when the fileCopySrcOperType is tftp(4) and
         fileCopyDestOperType is file(1)."
    ::= { fileCopyMgt 5 }

fileCopyUnitId OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the switch unit for stackable devices.
                When performing the 'copy unit file' or 'copy file unit' action,
                if neither fileCopySrcOperType nor fileCopyDestOperType
        		is unit(5), this variable can be ignored."
    ::= { fileCopyMgt 7 }

fileCopyAction OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    notCopying(1),
                    copy(2),
                    abort(4)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set this object to copy(2) to begin the copy operation.
                 When the device is not copying, this object will have a value
                 of notCopying(1). Set this object to abort(4) to abort
                 a transfer."
    ::= { fileCopyMgt 8 }

fileCopyStatus  OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    fileCopyTftpIllegalOperation(5),
                    fileCopyTftpUnkownTransferId(6),
                    fileCopyTftpFileExisted(7),
                    fileCopyTftpNoSuchUser(8),
                    fileCopyTftpSendError(10),
                    fileCopyTftpReceiverError(11),
                    fileCopyTftpSocketOpenError(12),
                    fileCopyTftpSocketBindError(13),
                    fileCopyTftpUserCancel(14),
                    fileCopyParaError(16),
                    fileCopyBusy(17),
                    fileCopyUnknown(18),
                    fileCopyReadFileError(19),
                    fileCopySetStartupError(20),
                    fileCopyFileSizeExceed(21),
                    fileCopyMagicWordError(22),
                    fileCopyImageTypeError(23),
                    fileCopyHeaderChecksumError(24),
                    fileCopyImageChecksumError(25),
                    fileCopyWriteFlashFinish(26),
                    fileCopyWriteFlashError(27),
                    fileCopyWriteFlashProgramming(28),
                    fileCopyError(29),
                    fileCopySuccess(30),
                    fileCopyCompleted(31),
--
-- ES4612-20-00499, 2008-12-09, support FTPS
--
                    fileCopyFileNotFound(41),
                    fileCopyServerPermissionDenied(42),
                    fileCopyStorageFull(43),
                    fileCopyConnectError(44),
                    fileCopyServerNotInService(45),
                    fileCopyDataConnectionOpenError(46),
                    fileCopyLogInError(47),
                    fileCopyInvalidFileName(48),
                    fileCopyServerNotAcceptProvidedCiphers(49),
                    fileCopyServerNotSupportFtps(50),
                    fileCopyFileUnavailable(51),
                    fileCopyUnclassifiedError(52),
                    fileCopyTimeout(53),
                    fileCopyProjectIdError(54),
                    fileCopyFileNumExceed(55),
                    fileCopySameVersion(56),
                    fileCopyFileLenZero(57)
                }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The status of the last copy procedure, if any.  This
        object will have a value of fileCopyUnknown(18) if no
        copy operation has been performed."
    ::= { fileCopyMgt 9 }

fileCopyServerInetAddressType OBJECT-TYPE
     SYNTAX      InetAddressType
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION "Internet address type of the remote server. Only ipv4(1)
                  type is supported."
     ::= { fileCopyMgt 20 }

fileCopyServerInetAddress OBJECT-TYPE
     SYNTAX      InetAddress
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION "Internet address of the remote server."
     ::= { fileCopyMgt 21 }

fileCopyServerUserName OBJECT-TYPE
     SYNTAX      DisplayString (SIZE(0..127))
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION "Login user name for the remote server. When this variable is
                  empty, the system will use 'anonymous' as user name to log in
                  to the remote server."
     ::= { fileCopyMgt 22 }

fileCopyServerPassword OBJECT-TYPE
     SYNTAX      DisplayString (SIZE(0..127))
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION "Login password for the remote server. This variable can only
                  be written. When this variable is read, it always returns a
                  zero-length string."
     ::= { fileCopyMgt 23 }

--
-- This mangement performs the display and delete operation.
--

fileInfoTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF FileInfoEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "This table contain the information of the file system;
                 we can also perform the delete, set startup file operation."

    ::= { fileInfoMgt 1 }

fileInfoEntry OBJECT-TYPE
    SYNTAX       FileInfoEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "A conceptually row for fileInfoTable."
    INDEX       { fileInfoUnitID, IMPLIED fileInfoFileName}
    ::= { fileInfoTable 1 }

FileInfoEntry ::= SEQUENCE
    {
        fileInfoUnitID                  Integer32,
        fileInfoFileName                DisplayString,
        fileInfoFileType                INTEGER,
        fileInfoIsStartUp               TruthValue,
        fileInfoFileSize                Integer32,
        fileInfoCreationTime            DisplayString,
        fileInfoDelete                  INTEGER
    }

fileInfoUnitID OBJECT-TYPE
    SYNTAX       Integer32
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "The switch unit in a stacking system, in a
                 non-stacking system, this value is always 1."
    ::= { fileInfoEntry 1 }

fileInfoFileName OBJECT-TYPE
    SYNTAX       DisplayString (SIZE (1..32))
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "The file Name of the file System in the device."
    ::= { fileInfoEntry 2 }

fileInfoFileType OBJECT-TYPE
    SYNTAX       INTEGER
                 {
                    diag(1),
                    runtime(2),
                    syslog(3),
                    cmdlog(4),
                    config(5),
                    postlog(6),
                    private(7),
                    certificate(8),
                    webarchive(9)
                 }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The file type of the file System in the device."
    ::= { fileInfoEntry 3 }

fileInfoIsStartUp OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION "This flag indicate whether this file is a startup file. Set this
                 object to true(1) to indicate that this is a startup file. Setting this
                 object to false(2) is a invalid operation."
    ::= { fileInfoEntry 4 }

fileInfoFileSize OBJECT-TYPE
    SYNTAX       Integer32
    UNITS        "bytes"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The sizes( in bytes) of the file."
    ::= { fileInfoEntry 5 }

fileInfoCreationTime OBJECT-TYPE
    SYNTAX       DisplayString(SIZE(20))
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The creation time of the file, This is a text string in the
                 following form, based on Unix: 'Mmm _d hh:mm:ss yyyy'. 'Mmm'
                 are the first three letters of the English name of the month.
                 '_d' is the day of month. A single-digit day is preceded by
                 a space. 'hh:mm:ss' is a 24-hour representations of hours,
                 minutes, and seconds. A single-digit hour is preceded by a
                 zero. 'yyyy' is the four-digit year. An example is:
                 'Jan  1 02:03:04 2002'."
    ::= { fileInfoEntry 6 }

fileInfoDelete OBJECT-TYPE
    SYNTAX       INTEGER
                 {
                  noDelete(1),
                  delete(2)
                 }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION "Write this object to delete(2) to delete a file, when
                 read, this always return noDelete(1)."
    ::= { fileInfoEntry 7 }

--fileAutoDownloadResultTable

fileAutoDownloadResultTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF FileAutoDownloadResultEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "This table contains file auto download result information."
    ::= { fileMgt 3 }

fileAutoDownloadResultEntry OBJECT-TYPE
    SYNTAX       FileAutoDownloadResultEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "A conceptual row for fileAutoDownloadResultTable."
    INDEX       {fileAutoDownloadResultUnitID}
    ::= { fileAutoDownloadResultTable 1 }

FileAutoDownloadResultEntry ::= SEQUENCE
    {
        fileAutoDownloadResultUnitID                  Integer32,
        fileAutoDownloadResultAction				  INTEGER,
        fileAutoDownloadResultStatus                  INTEGER
    }

fileAutoDownloadResultUnitID OBJECT-TYPE
    SYNTAX       Integer32
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "The switch unit in a stacking system, in a
                 non-stacking system, this value is always 1."
    ::= { fileAutoDownloadResultEntry 1 }

fileAutoDownloadResultAction OBJECT-TYPE
    SYNTAX       INTEGER
                 {
	                  notCopying(1),
	                  copying(2)
                 }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The status of the auto download action.
    			 value copying(2) will be obtained if the auto download action is currently processing,
    			 or value notCopying(1) will be obtained if no auto download action is currently processing.

    			 You can check the download result through the fileAutoDownloadResultStatus object
    			 after the download action has finished.

    			 Please note that this object is read-only, since the auto download action is triggered
    			 automatically by the system when an image file or a config file is set as startup setting
    			 through the fileInfoIsStartUp, restartOpCodeFile or restartConfigFile objects,
    			 but not set by the user manually through this fileAutoDownloadResultAction object."
    ::= { fileAutoDownloadResultEntry 2 }

fileAutoDownloadResultStatus OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    fileCopyTftpIllegalOperation(5),
                    fileCopyTftpUnkownTransferId(6),
                    fileCopyTftpFileExisted(7),
                    fileCopyTftpNoSuchUser(8),
                    fileCopyTftpSendError(10),
                    fileCopyTftpReceiverError(11),
                    fileCopyTftpSocketOpenError(12),
                    fileCopyTftpSocketBindError(13),
                    fileCopyTftpUserCancel(14),
                    fileCopyParaError(16),
                    fileCopyBusy(17),
                    fileCopyUnknown(18),
                    fileCopyReadFileError(19),
                    fileCopySetStartupError(20),
                    fileCopyFileSizeExceed(21),
                    fileCopyMagicWordError(22),
                    fileCopyImageTypeError(23),
                    fileCopyHeaderChecksumError(24),
                    fileCopyImageChecksumError(25),
                    fileCopyWriteFlashFinish(26),
                    fileCopyWriteFlashError(27),
                    fileCopyWriteFlashProgramming(28),
                    fileCopyError(29),
                    fileCopySuccess(30),
                    fileCopyCompleted(31),
--
-- ES4612-20-00499, 2008-12-09, support FTPS
--
                    fileCopyFileNotFound(41),
                    fileCopyServerPermissionDenied(42),
                    fileCopyStorageFull(43),
                    fileCopyConnectError(44),
                    fileCopyServerNotInService(45),
                    fileCopyDataConnectionOpenError(46),
                    fileCopyLogInError(47),
                    fileCopyInvalidFileName(48),
                    fileCopyServerNotAcceptProvidedCiphers(49),
                    fileCopyServerNotSupportFtps(50),
                    fileCopyFileUnavailable(51),
                    fileCopyUnclassifiedError(52),
                    fileCopyTimeout(53),
                    fileCopyProjectIdError(54),
                    fileCopyFileNumExceed(55),
                    fileCopySameVersion(56),
                    fileCopyFileLenZero(57)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The last auto download result status.
                 value fileCopyUnknown(18) will be obtained
                 if no download action has been performed before.
                 The listed values are identical to fileCopyStatus."
    ::= { fileAutoDownloadResultEntry 3 }

--
--dnsMgt
--

--dnsHostTable
dnsDomainLookup OBJECT-TYPE
    SYNTAX       EnabledStatus
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION "To enable the IP Domain Naming System (DNS)-based host name-to-address translation."
    ::= { dnsMgt 1 }

dnsDomainName OBJECT-TYPE
    SYNTAX       DisplayString(SIZE(0..255))
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION "To define a default domain name to complete
                unqualified host names (names without a dotted-decimal domain name)."
    ::= { dnsMgt 2 }

--dnsCacheTable
dnsCacheTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF DnsCacheEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "To display the RRs in DNS cache."
    ::= { dnsMgt 7 }

dnsCacheEntry OBJECT-TYPE
    SYNTAX       DnsCacheEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "A conceptual row for the dnsCacheTable."
    INDEX       { dnsCacheIndex }
    ::= { dnsCacheTable 1 }

DnsCacheEntry ::= SEQUENCE
    {
        dnsCacheIndex           Integer32,
        dnsCacheFlag            Integer32,
        dnsCacheType            INTEGER,
        dnsCacheTtl             Integer32,
        dnsCacheDomain          DisplayString,
        dnsCacheInetAddressType InetAddressType,
        dnsCacheInetAddress     InetAddress
    }

dnsCacheIndex OBJECT-TYPE
    SYNTAX       Integer32
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "The entry sequence number."
    ::= { dnsCacheEntry 1 }

dnsCacheFlag OBJECT-TYPE
    SYNTAX       Integer32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "Always get 4, means this record is unreliable."
    ::= { dnsCacheEntry 2 }

dnsCacheType OBJECT-TYPE
    SYNTAX       INTEGER
                 {
                    address(1),
                    cname(2)
                 }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "Cache Type: address(1); cname(2)."
    ::= { dnsCacheEntry 3 }

dnsCacheTtl OBJECT-TYPE
    SYNTAX       Integer32(0..876000)
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The DNS cache TTL."
    ::= { dnsCacheEntry 5 }

dnsCacheDomain OBJECT-TYPE
    SYNTAX       DisplayString(SIZE(1..255))
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "The DNS cache domain."
    ::= { dnsCacheEntry 6 }

dnsCacheInetAddressType OBJECT-TYPE
    SYNTAX       InetAddressType
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION  "Indicates the type of address
                 denoted in dnsHostAddrInetAddress type.
                 Only ipv4(1) and ipv6(2) types are supported."
    ::= { dnsCacheEntry 7 }

dnsCacheInetAddress OBJECT-TYPE
    SYNTAX       InetAddress
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION "IP address of DNS cache item."
    ::= { dnsCacheEntry 8 }

dnsHostTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF DnsHostEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "The conceptual table of dnsHostEntry.
                 The dnsHostTable and dnsHostAddrTable are used to define
                 static host name-to-address mapping."
    ::= { dnsMgt 8 }

dnsHostEntry OBJECT-TYPE
    SYNTAX       DnsHostEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "A conceptual row for the dnsHostTable."
    INDEX       { dnsHostIndex }
    ::= { dnsHostTable 1 }

DnsHostEntry ::= SEQUENCE
    {
        dnsHostIndex          Integer32,
        dnsHostName           DisplayString,
        dnsHostStatus         ValidStatus
    }

dnsHostIndex OBJECT-TYPE
    SYNTAX       Integer32
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "The entry sequence number."
    ::= { dnsHostEntry 1 }

dnsHostName OBJECT-TYPE
    SYNTAX       DisplayString(SIZE(1..255))
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION "Host name."
    ::= { dnsHostEntry 2 }

dnsHostStatus OBJECT-TYPE
    SYNTAX       ValidStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION "Setting this to valid(1) creates an entry.
                 Setting this to invalid(2) destroys an entry."
    ::= { dnsHostEntry 3 }

--dnsHostAddrTable
dnsHostAddrTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF DnsHostAddrEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "The conceptual table of dnsHostAddrEntry.
                 The dnsHostTable and dnsHostAddrTable are used to define
                 static host name-to-address mapping."
    ::= { dnsMgt 9 }

dnsHostAddrEntry OBJECT-TYPE
    SYNTAX       DnsHostAddrEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "A conceptual row for the dnsHostAddrTable."
    INDEX       { dnsHostIndex, dnsHostAddrInetAddressType,
                  IMPLIED dnsHostAddrInetAddress}
    ::= { dnsHostAddrTable 1 }

DnsHostAddrEntry ::= SEQUENCE
{
        dnsHostAddrInetAddressType    InetAddressType,
        dnsHostAddrInetAddress        InetAddress,
        dnsHostAddrStatus             ValidStatus
}

dnsHostAddrInetAddressType OBJECT-TYPE
    SYNTAX       InetAddressType
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "Indicates the type of address
                 denoted in dnsHostAddrInetAddress type.
                 Only ipv4(1), ipv6(2) and ipv6z(4) type are supported."
    ::= { dnsHostAddrEntry 1 }

dnsHostAddrInetAddress OBJECT-TYPE
    SYNTAX       InetAddress
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "Specifies the address of the host.
                 Adding one address to two different hosts is not allowed."
    ::= { dnsHostAddrEntry 2 }

dnsHostAddrStatus OBJECT-TYPE
    SYNTAX       ValidStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION "Setting this to valid(1) creates an entry.
                 Setting this to invalid(2) destroys an entry."
    ::= { dnsHostAddrEntry 3 }

--dnsDomainListTable
dnsDomainListTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF DnsDomainListEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "This table defines a list of default domain names to complete unqualified host names."
    ::= { dnsMgt 10 }

dnsDomainListEntry OBJECT-TYPE
    SYNTAX       DnsDomainListEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "A conceptual row for the dnsDomainListTable."
    INDEX       { dnsDomainListIndex }
    ::= { dnsDomainListTable 1 }

DnsDomainListEntry ::= SEQUENCE
    {
        dnsDomainListIndex      Integer32,
        dnsDomainListName       DisplayString,
        dnsDomainListStatus     ValidStatus
    }

dnsDomainListIndex OBJECT-TYPE
    SYNTAX       Integer32
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "The entry sequence number."
    ::= { dnsDomainListEntry 1 }

dnsDomainListName OBJECT-TYPE
    SYNTAX       DisplayString(SIZE(1..255))
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION "Domain name."
    ::= { dnsDomainListEntry 2 }

dnsDomainListStatus OBJECT-TYPE
    SYNTAX       ValidStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION "Setting this to valid(1) creates an entry.
                 Setting this to invalid(2) destroys an entry."
    ::= { dnsDomainListEntry 3 }

dnsNameServerInetTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF DnsNameServerInetEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "Specifies the address of one or more name servers to use for
                 name and address resolution."
    ::= { dnsMgt 11 }

dnsNameServerInetEntry OBJECT-TYPE
    SYNTAX       DnsNameServerInetEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "A conceptual row for dnsNameServerInetTable."
    INDEX       { dnsNameServerInetAddressType, IMPLIED dnsNameServerInetAddress }
    ::= { dnsNameServerInetTable 1 }

DnsNameServerInetEntry ::= SEQUENCE
{
    dnsNameServerInetAddressType    InetAddressType,
    dnsNameServerInetAddress        InetAddress,
    dnsNameServerInetStatus         ValidStatus
}

dnsNameServerInetAddressType OBJECT-TYPE
    SYNTAX       InetAddressType
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION  "Type of address. Only ipv4(1), ipv6(2) and ipv6z(4) types are
                  supported."
    ::= { dnsNameServerInetEntry 1 }

dnsNameServerInetAddress OBJECT-TYPE
    SYNTAX       InetAddress
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION "IP address of name server."
    ::= { dnsNameServerInetEntry 2 }

dnsNameServerInetStatus OBJECT-TYPE
    SYNTAX      ValidStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Setting this to valid(1) creates an entry.
                 Setting this to invalid(2) destroys an entry."
    ::= { dnsNameServerInetEntry 3 }

--
-- This mangement automatically upgrades image.
--

fileAutoUpgradeOpCodeStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set this variable to enabled(1) to enable the device to
                 automatically upgrade the current software image when a new
                 version is detected. Set this variable to disabled(2) to
                 disable this feature."
    ::= { fileAutoUpgradeMgt 1 }

fileAutoUpgradeOpCodePath OBJECT-TYPE
    SYNTAX      DisplayString(SIZE(0..255))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The URL (Universal Resource Location) of the image file
                 location for automatic upgrades. The URL schema can be set to
                 TFTP or FTP. The Hostname is the IP address of the server. The
                 last character of the URL is always a '/' and the filename must
                 not be included in the URL."
    ::= { fileAutoUpgradeMgt 2 }

fileAutoUpgradeOpCodeFileName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..127))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The file name of the image file."
    ::= { fileAutoUpgradeMgt 3 }

--
-- PSE Port Table
--

pethPsePortExtTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF PethPsePortExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of objects that display and control the power characteristics
        of power Ethernet ports on a Power Source Entity (PSE) device.
        This group will be implemented in managed power Ethernet switches and
        mid-span devices. Values of all read-write objects in this table are
        persistent at restart/reboot."
    REFERENCE   "IEEE 802.3af, POWER-ETHERNET-MIB.pethPsePortTable"
    ::= { poeMgt 6 }

pethPsePortExtEntry OBJECT-TYPE
    SYNTAX      PethPsePortExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A set of objects that display and control the power characteristics of
        a power Ethernet PSE port."
    AUGMENTS    { pethPsePortEntry }
    ::= { pethPsePortExtTable 1 }

PethPsePortExtEntry ::= SEQUENCE
{
    pethPsePortExtMirroredDllPdRequestedPowerValue          INTEGER,
    pethPsePortExtDllPseAllocatedPowerValue                 INTEGER,
    pethPsePortTimeRange                                    DisplayString,
    pethPsePortTimeRangeStatus                              INTEGER,
    pethPsePortExtMaximumPowerValue                         INTEGER,
    pethPsePortExtUsedPowerValue                            INTEGER
}

pethPsePortExtMirroredDllPdRequestedPowerValue OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Returns the PD requested power value received from the remote system.
        The definition and encoding of PD requested power value is the same as
        described in pethPdPortDllPdRequestedPowerValue."
    REFERENCE
        "IEEE Std 802.3at Section 30.9.1.1.18
        aMirroredDLLPDRequestedPowerValue"
    ::= { pethPsePortExtEntry 4 }

pethPsePortExtDllPseAllocatedPowerValue OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Returns the PSE allocated power value that the local system has
        currently allocated to the remote system. The PSE allocated power value
        is the maximum input average power that the PSE wants the PD to ever
        draw under this allocation if it is accepted. The PSE allocated power
        value is encoded according to Equation (33-20), where X is the decimal
        value of pethPsePortExtDllPseAllocatedPowerValue."
    REFERENCE
        "IEEE Std 802.3at Section 30.9.1.1.20
        aDLLPSEAllocatedPowerValue"
    ::= { pethPsePortExtEntry 6 }

pethPsePortTimeRange OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..16))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The name of the time range entry bound to the port.
                     This object should be equal to one of the timeRangeName
                     objects in timeRangeTable. The object works when
                     pethPsePortAdminEnable is enabled(1)."
        ::= { pethPsePortExtEntry 11 }

pethPsePortTimeRangeStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        none(0),
                        active(1),
                        inactive(2)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "If no time range entry is bound to the port, value of this
                     object is none(0). If PoE time range of the port is active,
                     value of this object is active(1). If PoE time range of
                     the port is inactive, value of this object is inactive(2)."
        ::= { pethPsePortExtEntry 12 }

pethPsePortExtMaximumPowerValue OBJECT-TYPE
    SYNTAX      INTEGER (3000..30000)
    UNITS       "milliwatts"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Returns the user-configurable maximum power value that
        the local system has currently allocated to the remote system.
        The units of this variable is milliwatts."
    ::= { pethPsePortExtEntry 13 }

pethPsePortExtUsedPowerValue OBJECT-TYPE
    SYNTAX      INTEGER
    UNITS       "milliwatts"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Returns the currently used power value that
        the local system is delivering to the remote system.
        The units of this variable is milliwatts."
    ::= { pethPsePortExtEntry 14 }

--
-- mcastStormMgt
--

mcastStormMgt OBJECT IDENTIFIER ::= { stormMgt 1 }

mcastStormTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF McastStormEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table to manage the control of multicast storms for ports."
        ::= { mcastStormMgt 1 }

mcastStormEntry OBJECT-TYPE
        SYNTAX      McastStormEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual row of multiStormTable."
        INDEX       { mcastStormIfIndex }
        ::= { mcastStormTable 1 }

McastStormEntry ::= SEQUENCE
{
    mcastStormIfIndex      Integer32,
    mcastStormStatus       EnabledStatus,
    mcastStormOctetRate    Integer32
}

mcastStormIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and the trunk (including trunk members) interface of
                     the portTable. The interface identified by a particular value
                     of this index is the same interface as identified by the same
                     value of ifIndex in the IF-MIB."
        ::= { mcastStormEntry 1 }

mcastStormStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Whether multicast storm protection is enabled."
        ::= { mcastStormEntry 2 }

mcastStormOctetRate OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Multicast storm threshold as octets per second.
                     If this entry is for a trunk, this is the value
                     for each member port."
        ::= { mcastStormEntry 5 }

--
-- bcastStormMgt
--

-- Management for broadcast storm control for ports.

bcastStormMgt OBJECT IDENTIFIER ::= { stormMgt 3 }
bcastStormTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF BcastStormEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table to manage the control of broadcast storms for ports."
        ::= { bcastStormMgt 1 }

bcastStormEntry OBJECT-TYPE
        SYNTAX      BcastStormEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The conceptual row of bcastStormTable."
        INDEX       { bcastStormIfIndex }
        ::= { bcastStormTable 1 }

BcastStormEntry ::= SEQUENCE
{
    bcastStormIfIndex      Integer32,
    bcastStormStatus       EnabledStatus,
    bcastStormOctetRate    Integer32
}

bcastStormIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port and the trunk (including trunk members) interface of
                     the portTable. The interface identified by a particular value
                     of this index is the same interface as identified by the same
                     value of ifIndex in the IF-MIB."
        ::= { bcastStormEntry 1 }

bcastStormStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Whether broadcast storm protection is enabled."
        ::= { bcastStormEntry 2 }

bcastStormOctetRate OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Broadcast storm threshold as octets per second.
                     If this entry is for a trunk, this is the value
                     for each member port."
        ::= { bcastStormEntry 5 }

--
-- unknownUcastStormMgt
--

unknownUcastStormMgt OBJECT IDENTIFIER ::=  {stormMgt 4 }

unknownUcastStormTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF UnknownUcastStormEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Table to manage the unknown unicast storm control."
    ::= { unknownUcastStormMgt 1 }

unknownUcastStormEntry OBJECT-TYPE
    SYNTAX      UnknownUcastStormEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The conceptual row of unknownUcastStormTable."
    INDEX       { unknownUcastStormIfIndex }
    ::= { unknownUcastStormTable 1 }

UnknownUcastStormEntry ::= SEQUENCE
{
    unknownUcastStormIfIndex    Integer32,
    unknownUcastStormStatus     EnabledStatus,
    unknownUcastStormOctetRate  INTEGER
}

unknownUcastStormIfIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The port or trunk interface of the portTable. The interface
                 identified by a particular value of this index is the same
                 interface as identified by the same value of ifIndex in the
                 IF-MIB."
    ::= { unknownUcastStormEntry 1 }

unknownUcastStormStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates that the unknown unicast
                 storm protection is enabled/disabled."
    ::= { unknownUcastStormEntry 2 }

unknownUcastStormOctetRate OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates the byte rate of the storm protection."
    ::= { unknownUcastStormEntry 5 }

--
-- Auto Traffic Control ASE3528B-E1-FLF-P5-00011
--

atcMgt OBJECT IDENTIFIER ::= { stormMgt 5 }

atcBcastStormTcApplyTime OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates the timing when the ATC (Auto
                 Traffic Control) is activated after the broadcast traffic
                 being detected as the storm."
    ::= { atcMgt 1 }

atcBcastStormTcReleaseTime OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates the timing when the ATC is released
                 after the broadcast traffic being detected as no storm."
    ::= { atcMgt 2 }

atcBcastStormTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AtcBcastStormEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The table contains the Auto Traffic Control configuration
                 and the status for broadcast traffic."
    ::= { atcMgt 3 }

atcBcastStormEntry OBJECT-TYPE
    SYNTAX      AtcBcastStormEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The conceptual row of the table."
    INDEX       { atcBcastStormIfIndex }
    ::= { atcBcastStormTable 1 }

AtcBcastStormEntry ::= SEQUENCE
{
    atcBcastStormIfIndex                Integer32,
    atcBcastStormEnable                 EnabledStatus,
    atcBcastStormAutoRelease            EnabledStatus,
    atcBcastStormSampleType             INTEGER,
    atcBcastStormCurrentTrafficRate     Integer32,
    atcBcastStormAlarmFireThreshold     Integer32,
    atcBcastStormAlarmClearThreshold    Integer32,
    atcBcastStormTcAction               INTEGER,
    atcBcastStormAlarmFireTrapStatus    EnabledStatus,
    atcBcastStormAlarmClearTrapStatus   EnabledStatus,
    atcBcastStormTcApplyTrapStatus      EnabledStatus,
    atcBcastStormTcReleaseTrapStatus    EnabledStatus,
    atcBcastStormControlRelease         EnabledStatus
}

atcBcastStormIfIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION "The specified port on which the ATC is applied."
    ::= { atcBcastStormEntry 1 }

atcBcastStormEnable OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the ATC of the broadcast
                 traffic is applied."
    ::= { atcBcastStormEntry 2 }

atcBcastStormAutoRelease OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the Auto-Release feature
                 of ATC is applied."
    ::= { atcBcastStormEntry 3 }

atcBcastStormSampleType OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    packet-rate(1),
                    octet-rate(2),
                    percent(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates the unit of traffic rate and threshold."
    ::= { atcBcastStormEntry 4 }

atcBcastStormCurrentTrafficRate OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The parameter indicates the current broadcast traffic rate."
    ::= { atcBcastStormEntry 5 }

atcBcastStormAlarmFireThreshold OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates that if the current broadcast traffic rate
                exceeds the specified threshold, it will be treated as the storm."
    ::= { atcBcastStormEntry 6 }

atcBcastStormAlarmClearThreshold OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates that if the current broadcast traffic
                 falls below the specified threshold it will be treated as the
                 normal traffic."
    ::= { atcBcastStormEntry 7 }

atcBcastStormTcAction OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    rate-control(1),
                    shutdown(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates the protecting action which
                 ATC will applied to the specified port."
    ::= { atcBcastStormEntry 8 }

atcBcastStormAlarmFireTrapStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the trap has
                 to be sent when the broadcast storm has been detected."
    ::= { atcBcastStormEntry 9 }

atcBcastStormAlarmClearTrapStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the trap has
                 to be sent when the broadcast storm has been detected as
                 the normal traffic."
    ::= { atcBcastStormEntry 10 }

atcBcastStormTcApplyTrapStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the trap has to be sent when
                 the ATC is activated."
    ::= { atcBcastStormEntry 11 }

atcBcastStormTcReleaseTrapStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the trap has to be sent when
                 the ATC is released."
    ::= { atcBcastStormEntry 12 }

atcBcastStormControlRelease OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the Control Release feature
                 of ATC is applied."
    ::= { atcBcastStormEntry 13 }

atcMcastStormTcApplyTime OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates the timing when the ATC (Auto
                 Traffic Control) is activated after the broadcast traffic
                 being detected as the storm."
    ::= { atcMgt 4 }

atcMcastStormTcReleaseTime OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates the timing when the ATC is released
                 after the broadcast traffic being detected as no storm."
    ::= { atcMgt 5 }

atcMcastStormTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AtcMcastStormEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The table contains the Auto Traffic Control configuration
                 and the status for mulicast traffic."
    ::= { atcMgt 6 }

atcMcastStormEntry OBJECT-TYPE
    SYNTAX      AtcMcastStormEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The conceptual row of the table."
    INDEX       { atcMcastStormIfIndex }
    ::= { atcMcastStormTable 1 }

AtcMcastStormEntry ::= SEQUENCE
{
    atcMcastStormIfIndex                Integer32,
    atcMcastStormEnable                 EnabledStatus,
    atcMcastStormAutoRelease            EnabledStatus,
    atcMcastStormSampleType             INTEGER,
    atcMcastStormCurrentTrafficRate     Integer32,
    atcMcastStormAlarmFireThreshold     Integer32,
    atcMcastStormAlarmClearThreshold    Integer32,
    atcMcastStormTcAction               INTEGER,
    atcMcastStormAlarmFireTrapStatus    EnabledStatus,
    atcMcastStormAlarmClearTrapStatus   EnabledStatus,
    atcMcastStormTcApplyTrapStatus      EnabledStatus,
    atcMcastStormTcReleaseTrapStatus    EnabledStatus,
    atcMcastStormControlRelease         EnabledStatus
}

atcMcastStormIfIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION "The specified port on which the ATC is applied."
    ::= { atcMcastStormEntry 1 }

atcMcastStormEnable OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the ATC of the mulicast
                 traffic is applied."
    ::= { atcMcastStormEntry 2 }

atcMcastStormAutoRelease OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the Auto-Release feature
                 of ATC is applied."
    ::= { atcMcastStormEntry 3 }

atcMcastStormSampleType OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    packet-rate(1),
                    octet-rate(2),
                    percent(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates the unit of traffic rate and threshold."
    ::= { atcMcastStormEntry 4 }

atcMcastStormCurrentTrafficRate OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The parameter indicates the current mulicast traffic rate."
    ::= { atcMcastStormEntry 5 }

atcMcastStormAlarmFireThreshold OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates that if the current mulicast traffic rate
                exceeds the specified threshold, it will be treated as the storm."
    ::= { atcMcastStormEntry 6 }

atcMcastStormAlarmClearThreshold OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates that if the current mulicast traffic
                 falls below the specified threshold it will be treated as the
                 normal traffic."
    ::= { atcMcastStormEntry 7 }

atcMcastStormTcAction OBJECT-TYPE
    SYNTAX      INTEGER
                {
                    rate-control(1),
                    shutdown(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates the protecting action which
                 ATC will applied to the specified port."
    ::= { atcMcastStormEntry 8 }

atcMcastStormAlarmFireTrapStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the trap has
                 to be sent when the mulicast storm has been detected."
    ::= { atcMcastStormEntry 9 }

atcMcastStormAlarmClearTrapStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the trap has
                 to be sent when the mulicast storm has been detected as
                 the normal traffic."
    ::= { atcMcastStormEntry 10 }

atcMcastStormTcApplyTrapStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the trap has to be sent when
                 the ATC is activated."
    ::= { atcMcastStormEntry 11 }

atcMcastStormTcReleaseTrapStatus OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the trap has to be sent when
                 the ATC is released."
    ::= { atcMcastStormEntry 12 }

atcMcastStormControlRelease OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The parameter indicates whether the Control Release feature
                 of ATC is applied."
    ::= { atcMcastStormEntry 13 }

--
-- sysResourceMgt
--

-- monitor the configuration changes for the product

        cpuStatus               OBJECT IDENTIFIER ::= { sysResourceMgt 2 }
        memoryStatus            OBJECT IDENTIFIER ::= { sysResourceMgt 3 }

-- cpuStatus

         cpuCurrentUti            OBJECT-TYPE
            SYNTAX      INTEGER(1..100)
            UNITS       "%"
            ACCESS      read-only
            STATUS      current
            DESCRIPTION
                "The current CPU utilization in percent in the past 5 seconds."
            ::= { cpuStatus 1 }

        cpuStatMaxUti            OBJECT-TYPE
            SYNTAX      INTEGER(1..100)
            UNITS       "%"
            ACCESS      read-only
            STATUS      current
            DESCRIPTION
                "The maximum CPU utilization in percent in the past 60 seconds."
            ::= { cpuStatus 2 }

        cpuStatAvgUti            OBJECT-TYPE
            SYNTAX      INTEGER(1..100)
            UNITS       "%"
            ACCESS      read-only
            STATUS      current
            DESCRIPTION
                "The average CPU utilization in percent in the past 60 seconds."
            ::= { cpuStatus 3 }

        cpuPeakTime            OBJECT-TYPE
            SYNTAX      DisplayString
            ACCESS      read-only
            STATUS      current
            DESCRIPTION
                "The time when the CPU utilization reaches cpuUtiRisingThreshold
                 in the format of 'Mmm _d hh:mm:ss yyyy' as defined
                 in sysCurrentTime of this MIB."
            ::= { cpuStatus 4 }

        cpuPeakDuration       OBJECT-TYPE
            SYNTAX      INTEGER
            UNITS       "second"
            ACCESS      read-only
            STATUS      current
            DESCRIPTION
                "The duration from the CPU utilization reaches cpuUtiRisingThreshold
                 to reaches cpuUtiFallingThreshold, in seconds."
            ::= { cpuStatus 5 }

        cpuUtiRisingThreshold            OBJECT-TYPE
            SYNTAX      INTEGER(1..100)
            UNITS       "%"
            ACCESS      read-write
            STATUS      current
            DESCRIPTION
                "The rising threshold of the cpu utilization."
            ::= { cpuStatus 6 }

        cpuUtiFallingThreshold           OBJECT-TYPE
            SYNTAX      INTEGER(1..100)
            UNITS       "%"
            ACCESS      read-write
            STATUS      current
            DESCRIPTION
                "The falling threshold of the cpu utilization."
            ::= { cpuStatus 7 }

-- memoryStatus

         memoryTotal    OBJECT-TYPE
            SYNTAX      INTEGER
            ACCESS      read-only
            STATUS      current
            DESCRIPTION
                "The total amount of the memory in kilobytes."
            ::= { memoryStatus 1 }

          memoryAllocated       OBJECT-TYPE
            SYNTAX      INTEGER
            ACCESS      read-only
            STATUS      current
            DESCRIPTION
                "The amount of the memory allocated in kilobytes."
            ::= { memoryStatus 2 }

          memoryFreed    OBJECT-TYPE
            SYNTAX      INTEGER
            ACCESS      read-only
            STATUS      current
            DESCRIPTION
                "The amount of the free memory in kilobytes."
            ::= { memoryStatus 3 }

         memoryFreedInPercent         OBJECT-TYPE
            SYNTAX      INTEGER(1..100)
            ACCESS      read-only
            STATUS      current
            DESCRIPTION
                "the memory freed in proportion to the total memory."
            ::= { memoryStatus 4 }

         memoryUtiRisingThreshold            OBJECT-TYPE
            SYNTAX      INTEGER(1..100)
            UNITS       "%"
            ACCESS      read-write
            STATUS      current
            DESCRIPTION
                 "The rising threshold of the memory utilization."
            ::= { memoryStatus 5 }

         memoryUtiFallingThreshold            OBJECT-TYPE
            SYNTAX      INTEGER(1..100)
            UNITS       "%"
            ACCESS      read-write
            STATUS      current
            DESCRIPTION
                 "The falling threshold of the memory utilization."
            ::= { memoryStatus 6 }

--
-- mvrMgt
--

mvrStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Parameter to enable or disable MVR(Multicast VLAN
                     Registration) on the device. NOTE: IGMP Snooping
                     must be enabled first before enabling MVR and MVR
                     will be disabled when IGMP Snooping is disabled."
        ::= { mvrMgt 1 }

mvrVlanId OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "To set VLAN for MVR.The VLAN identified by a particular
                     value of this index is the same VLAN as identified by the
                     same value of dot1qVlanIndex in the Q-BRIDGE-MIB."
        ::= { mvrMgt 2 }

mvrMaxGroups  OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The maximum number of MVR groups."
        ::= { mvrMgt 3 }

mvrCurrentGroups   OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The current number of MVR groups."
        ::= { mvrMgt 4 }

mvrGroupsCtl      OBJECT IDENTIFIER   ::= { mvrMgt 5 }

mvrGroupsCtlId   OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The start of a contiguous range of MVR group
                     addresses."
        ::= { mvrGroupsCtl 1 }

mvrGroupsCtlCount   OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The range count for configuring MVR group addresses."
        ::= { mvrGroupsCtl 2 }

mvrGroupsCtlAction   OBJECT-TYPE
        SYNTAX      INTEGER
        {
            noAction(0),
            create(1),
            destory(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Sets the configure action for a contiguous range of MVR group
                     addresses. The start addresses is the current value of
                     mvrGroupsCtlId and the range count is the current value of
                     mvrGroupsCtlCount. Set this object to create(2) to
                     create MVR group addresses. Set this object
                     to destory(3) to delete MVR group addresses. When
                     the action is complete, this object becomes noAction(1)."
        ::= { mvrGroupsCtl 3 }

mvrGroupTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF MvrGroupEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The table for configuring the MVR group."
       ::= { mvrMgt 6 }

mvrGroupEntry OBJECT-TYPE
       SYNTAX      MvrGroupEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The entry for configuring the MVR group."
       INDEX  {mvrGroupId}
       ::= { mvrGroupTable 1 }

MvrGroupEntry ::= SEQUENCE
{
    mvrGroupId IpAddress,
    mvrGroupActive INTEGER,
    mvrGroupStatus INTEGER
}

mvrGroupId OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The multicast address of the MVR group."
        ::= { mvrGroupEntry 1 }

mvrGroupActive   OBJECT-TYPE
        SYNTAX      INTEGER
        {
            active(1),
            inactive(2)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "To indicate if the group has a member or not. If there are no
                     members, the status is inactive(2); otherwise the status
                     is active(1)."
        ::= { mvrGroupEntry 2 }

mvrGroupStatus   OBJECT-TYPE
        SYNTAX      INTEGER
        {
            valid(1),
            invalid(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting this to valid(1) creates an entry. Setting this
                     to invalid(2) destroys an entry."
        ::= { mvrGroupEntry 3 }

mvrGroupStaticTable   OBJECT-TYPE
        SYNTAX      SEQUENCE OF MvrGroupStaticEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The table for configuring the static members of the
                     MVR group."
        ::= { mvrMgt 7 }

mvrGroupStaticEntry OBJECT-TYPE
       SYNTAX      MvrGroupStaticEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The entry for configuring the static members of the
                    MVR group."
       INDEX  {mvrGroupStaticAddress}
       ::= { mvrGroupStaticTable 1 }

MvrGroupStaticEntry ::= SEQUENCE
{
    mvrGroupStaticAddress   IpAddress,
    mvrGroupStaticPorts     PortList,
    mvrGroupStaticStatus    INTEGER

}

mvrGroupStaticAddress  OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The multicast address of the MVR group."
        ::= { mvrGroupStaticEntry 1 }

mvrGroupStaticPorts  OBJECT-TYPE
        SYNTAX      PortList
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The set of ports configured by management in this entry.
                     Ports entered in this list will be the static members
                     of this MVR group."
        ::= { mvrGroupStaticEntry 2 }

mvrGroupStaticStatus  OBJECT-TYPE
        SYNTAX      INTEGER
        {
            valid(1),
            invalid(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting this to valid(1) creates an entry. Setting this
                     to invalid(2) destroys an entry."
        ::= { mvrGroupStaticEntry 3 }

mvrGroupCurrentTable   OBJECT-TYPE
        SYNTAX      SEQUENCE OF MvrGroupCurrentEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The table for the current members of the MVR group."
        ::= { mvrMgt 8 }

mvrGroupCurrentEntry OBJECT-TYPE
       SYNTAX      MvrGroupCurrentEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The entry for the current members of the MVR group."
       INDEX  {mvrGroupCurrentAddress}
       ::= { mvrGroupCurrentTable 1 }

MvrGroupCurrentEntry ::= SEQUENCE
{
    mvrGroupCurrentAddress  IpAddress,
    mvrGroupCurrentPorts          PortList,
    mvrGroupCurrentReceiverVlan   Integer32
}

mvrGroupCurrentAddress   OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The multicast address of the MVR group."
        ::= { mvrGroupCurrentEntry 1 }

mvrGroupCurrentPorts   OBJECT-TYPE
        SYNTAX      PortList
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The complete set of ports currently associated with this
                     MVR group."
        ::= { mvrGroupCurrentEntry 2 }

mvrGroupCurrentReceiverVlan   OBJECT-TYPE
        SYNTAX      Integer32(0..4094)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This object indicates the receiver VLAN of the MVR group.
                     None of receiver VLAN belong to the MVR group when
                     the value of this object is 0."
        ::= { mvrGroupCurrentEntry 3 }

mvrPortTable   OBJECT-TYPE
        SYNTAX      SEQUENCE OF MvrPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The table for configuring the MVR port."
        ::= { mvrMgt 9 }

mvrPortEntry OBJECT-TYPE
       SYNTAX      MvrPortEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The entry for configuring the MVR port."
       INDEX  {mvrIfIndex}
       ::= { mvrPortTable 1 }

MvrPortEntry ::= SEQUENCE
{
    mvrIfIndex  InterfaceIndex,
    mvrPortType INTEGER,
    mvrPortImmediateLeave   EnabledStatus,
    mvrPortActive   INTEGER

}

mvrIfIndex   OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The port interface of the portTable. The interface
                     identified by a particular value of this index is the
                     same interface as identified by the same value of ifIndex
                     in the IF-MIB."
        ::= { mvrPortEntry 1 }

mvrPortType   OBJECT-TYPE
        SYNTAX      INTEGER
        {
            none(0),
            source(1),
            receiver(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "For configuring the MVR port type. To disable the MVR
                     port type, use the none(0)."
        ::= { mvrPortEntry 2 }

mvrPortImmediateLeave   OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "To enable immediate leave on MVR port."
        ::= { mvrPortEntry 3 }

mvrPortActive   OBJECT-TYPE
        SYNTAX      INTEGER
        {
            active(1),
            inactive(2)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "To indicate if the port is associated with the MVR group.
                     If the port is the MVR receiver port or the MVR source
                     port in MVR vlan, the status is active(1); otherwise
                     the status is inactive(2)."
        ::= { mvrPortEntry 4 }

mvrRunningStatus OBJECT-TYPE
        SYNTAX  TruthValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Describes the running status of MVR (Multicast VLAN Registration)
                     to the switch. A value of true(1) indicates that all necessary
                     conditions in the MVR environment are satisfied. A value of false(2)
                     indicates that some necessary conditions in the MVR environment are
                     not satisfied."
        ::= { mvrMgt 10 }

mvrReceiverVlanId OBJECT-TYPE
        SYNTAX      Integer32(0..4094)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "To set receiver VLAN for MVR.The VLAN identified by a particular
                     value of this index is the same VLAN as identified by the
                     same value of dot1qVlanIndex in the Q-BRIDGE-MIB. To disable the
                     VLAN, set the value to 0."
        ::= { mvrMgt 12 }

mvrMaxReceiverGroups  OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The maximum number of MVR receiver groups."
        ::= { mvrMgt 13 }

mvrCurrentReceiverGroups   OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The current number of MVR receiver groups."
        ::= { mvrMgt 14 }

mvrReceiverGroupTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF MvrReceiverGroupEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The table for configuring the MVR receiver group."
       ::= { mvrMgt 15 }

mvrReceiverGroupEntry OBJECT-TYPE
       SYNTAX      MvrReceiverGroupEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The entry for configuring the MVR receiver group."
       INDEX  {mvrReceiverGroupId}
       ::= { mvrReceiverGroupTable 1 }

MvrReceiverGroupEntry ::= SEQUENCE
{
    mvrReceiverGroupId      IpAddress,
    mvrReceiverGroupActive  INTEGER,
    mvrReceiverGroupStatus  INTEGER
}

mvrReceiverGroupId OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The multicast address of a MVR receiver group."
        ::= { mvrReceiverGroupEntry 1 }

mvrReceiverGroupActive   OBJECT-TYPE
        SYNTAX      INTEGER
        {
            active(1),
            inactive(2)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicate whether the receiver group has a member or not. If there
                     are no members, the status will be inactive(2); if there are members,
                     the status will be active(1)."
        ::= { mvrReceiverGroupEntry 2 }

mvrReceiverGroupStatus   OBJECT-TYPE
        SYNTAX      INTEGER
        {
            valid(1),
            invalid(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting this to valid(1) creates an entry. Setting this
                     to invalid(2) destroys an entry."
        ::= { mvrReceiverGroupEntry 3 }

mvrReceiverGroupStaticTable   OBJECT-TYPE
        SYNTAX      SEQUENCE OF MvrReceiverGroupStaticEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The table for configuring static members of the
                     MVR receiver group."
        ::= { mvrMgt 16 }

mvrReceiverGroupStaticEntry OBJECT-TYPE
       SYNTAX      MvrReceiverGroupStaticEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The entry for configuring static members of the
                    MVR receiver group."
       INDEX  {mvrReceiverGroupStaticAddress}
       ::= { mvrReceiverGroupStaticTable 1 }

MvrReceiverGroupStaticEntry ::= SEQUENCE
{
    mvrReceiverGroupStaticAddress   IpAddress,
    mvrReceiverGroupStaticPorts     PortList,
    mvrReceiverGroupStaticStatus    INTEGER

}

mvrReceiverGroupStaticAddress  OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The multicast address of a MVR receiver group."
        ::= { mvrReceiverGroupStaticEntry 1 }

mvrReceiverGroupStaticPorts  OBJECT-TYPE
        SYNTAX      PortList
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The set of ports configured by management in this entry.
                     Ports entered in this list will be the static members
                     of this MVR receiver group."
        ::= { mvrReceiverGroupStaticEntry 2 }

mvrReceiverGroupStaticStatus  OBJECT-TYPE
        SYNTAX      INTEGER
        {
            valid(1),
            invalid(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting this to valid(1) creates an entry. Setting this
                     to invalid(2) destroys an entry."
        ::= { mvrReceiverGroupStaticEntry 3 }

mvrReceiverGroupCurrentTable   OBJECT-TYPE
        SYNTAX      SEQUENCE OF MvrReceiverGroupCurrentEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The table for the current members of a MVR receiver group."
        ::= { mvrMgt 17 }

mvrReceiverGroupCurrentEntry OBJECT-TYPE
       SYNTAX      MvrReceiverGroupCurrentEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION "The entry for the current members of a MVR receiver group."
       INDEX  {mvrReceiverGroupCurrentAddress}
       ::= { mvrReceiverGroupCurrentTable 1 }

MvrReceiverGroupCurrentEntry ::= SEQUENCE
{
    mvrReceiverGroupCurrentAddress  IpAddress,
    mvrReceiverGroupCurrentPorts    PortList
}

mvrReceiverGroupCurrentAddress   OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The multicast address of a MVR receiver group."
        ::= { mvrReceiverGroupCurrentEntry 1 }

mvrReceiverGroupCurrentPorts   OBJECT-TYPE
        SYNTAX      PortList
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The complete set of ports currently associated with a
                     MVR receiver group."
        ::= { mvrReceiverGroupCurrentEntry 2 }

--
-- dhcpSnoopMgt
--

-- Management of DHCP snooping and IP souce guard.

dhcpSnoopGlobal         OBJECT IDENTIFIER ::= { dhcpSnoopMgt 1 }
dhcpSnoopVlan           OBJECT IDENTIFIER ::= { dhcpSnoopMgt 2 }
dhcpSnoopInterface      OBJECT IDENTIFIER ::= { dhcpSnoopMgt 3 }
dhcpSnoopBindings       OBJECT IDENTIFIER ::= { dhcpSnoopMgt 4 }
dhcpSnoopStatistics     OBJECT IDENTIFIER ::= { dhcpSnoopMgt 5 }

dhcpSnoopEnable  OBJECT-TYPE
        SYNTAX     EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This object indicates whether the DHCP Snooping feature is
                     enabled."
        ::= { dhcpSnoopGlobal 1 }

dhcpSnoopVerifyMacAddressEnable     OBJECT-TYPE
        SYNTAX     EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This object indicates whether DHCP Snooping Mac address
                     verification is enabled."
        ::= { dhcpSnoopGlobal 2 }

dhcpSnoopInformationOptionEnable  OBJECT-TYPE

        SYNTAX     EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This object indicates whether the DHCP snooping information option(option 82) feature is
                     enabled."
        ::= { dhcpSnoopGlobal 3 }

dhcpSnoopInformationOptionPolicy     OBJECT-TYPE
        SYNTAX     INTEGER
                    {
                        drop(1),
                        keep(2),
                        replace(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This object indicates which reforwarding policy shall be used for DHCP
                     snooping information option(option 82). A value of drop(1) means to drop
                     the DHCP request packet which has the information option(option 82).
                     A value of keep(2) means to keep the existing information option(option 82)
                     of the DHCP request packet. A value of replace(3), which is the default value,
                     means to replace the existing information option(option 82) of the DHCP
                     request packet."
        ::= { dhcpSnoopGlobal 4 }

dhcpSnoopBindingsTableCtlAction OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        noAction(1),
                        store(2),
                        clear(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Set this to store(2) to store DHCP snooping binding entries to flash.
                     Set this to clear(3) to clear DHCP snooping binding entries from flash.
                     noAction(1) will always be obtained when reading this variable."
        ::= { dhcpSnoopGlobal 5 }

--
dhcpSnoopVlanConfigTable    OBJECT-TYPE
        SYNTAX      SEQUENCE OF DhcpSnoopVlanConfigEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table contains DHCP Snooping configurations of existing VLANs."
        ::= { dhcpSnoopVlan 1 }

dhcpSnoopVlanConfigEntry    OBJECT-TYPE
        SYNTAX      DhcpSnoopVlanConfigEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An instance contains the configuration to enable
                     or disable DHCP Snooping at each existing VLAN."
        INDEX       { dhcpSnoopVlanIndex }
        ::= { dhcpSnoopVlanConfigTable 1 }

DhcpSnoopVlanConfigEntry  ::= SEQUENCE
{
        dhcpSnoopVlanIndex      VlanIndex,
        dhcpSnoopVlanEnable     EnabledStatus
}

dhcpSnoopVlanIndex      OBJECT-TYPE
        SYNTAX      VlanIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This object indicates the VLAN ID on which DHCP Snooping
                     feature is configured."
        ::= { dhcpSnoopVlanConfigEntry 1 }

dhcpSnoopVlanEnable     OBJECT-TYPE
        SYNTAX     EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This object indicates whether DHCP Snooping is enabled in
                     this VLAN."
        ::= { dhcpSnoopVlanConfigEntry 2 }

--
dhcpSnoopPortConfigTable    OBJECT-TYPE
        SYNTAX      SEQUENCE OF DhcpSnoopPortConfigEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table provides the mechanism to configure the trust
                     state of each port or trunk for DHCP Snooping purpose."
        ::= { dhcpSnoopInterface 1 }

dhcpSnoopPortConfigEntry    OBJECT-TYPE
        SYNTAX      DhcpSnoopPortConfigEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An instance contains the configuration to enable or disable
                     trust state of each port or trunk for DHCP Snooping purpose."
        INDEX       { dhcpSnoopPortIfIndex }
        ::= { dhcpSnoopPortConfigTable 1 }

DhcpSnoopPortConfigEntry    ::= SEQUENCE
{
        dhcpSnoopPortIfIndex        InterfaceIndex,
        dhcpSnoopPortTrustEnable    EnabledStatus
}

dhcpSnoopPortIfIndex        OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The ifIndex value of the port or trunk."
        ::= { dhcpSnoopPortConfigEntry 1 }

dhcpSnoopPortTrustEnable    OBJECT-TYPE
        SYNTAX     EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This object indicates whether the port or trunk is trusted
                     for DHCP Snooping purpose."
        ::= { dhcpSnoopPortConfigEntry 2 }
--
dhcpSnoopBindingsTable      OBJECT-TYPE
        SYNTAX      SEQUENCE OF DhcpSnoopBindingsEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table contains the DHCP bindings information learnt by
                     the device."
        ::= { dhcpSnoopBindings 1 }

dhcpSnoopBindingsEntry      OBJECT-TYPE
        SYNTAX      DhcpSnoopBindingsEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An instance contains the Mac address, IP address type,
                     IP address, VLAN number, interface number, leased time and
                     status."
        INDEX       { dhcpSnoopBindingsVlanIndex, dhcpSnoopBindingsMacAddress }
        ::= { dhcpSnoopBindingsTable 1 }

DhcpSnoopBindingsEntry      ::= SEQUENCE
{
        dhcpSnoopBindingsVlanIndex      VlanIndex,
        dhcpSnoopBindingsMacAddress     MacAddress,
        dhcpSnoopBindingsAddrType       InetAddressType,
        dhcpSnoopBindingsEntryType      INTEGER,
        dhcpSnoopBindingsIpAddress      IpAddress,
        dhcpSnoopBindingsPortIfIndex    InterfaceIndex,
        dhcpSnoopBindingsLeaseTime      Unsigned32
}

dhcpSnoopBindingsVlanIndex      OBJECT-TYPE
        SYNTAX      VlanIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This object indicates the VLAN which a DHCP client host
                     belongs to."
        ::= { dhcpSnoopBindingsEntry 1 }

dhcpSnoopBindingsMacAddress     OBJECT-TYPE
        SYNTAX      MacAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This object indicates the MAC address of a DHCP client
                     host."
        ::= { dhcpSnoopBindingsEntry 2 }

dhcpSnoopBindingsAddrType       OBJECT-TYPE
        SYNTAX      InetAddressType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This object indicates the type of IP address denoted in
                     dhcpSnoopBindingsIpAddress type."
        ::= { dhcpSnoopBindingsEntry 3 }

dhcpSnoopBindingsEntryType      OBJECT-TYPE
        SYNTAX      INTEGER { dynamic(1), static(2) }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This object indicates that this binding is obtained from
                     dynamically learning or is a static configuraion."
        ::= { dhcpSnoopBindingsEntry 4 }

dhcpSnoopBindingsIpAddress      OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This object indicates the allocated IP address of
                     a DHCP client host."
        ::= { dhcpSnoopBindingsEntry 5 }

dhcpSnoopBindingsPortIfIndex    OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This object indicates the port or trunk where a DHCP client
                     host connects to."
        ::= { dhcpSnoopBindingsEntry 6 }

dhcpSnoopBindingsLeaseTime      OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This object indicates the leased time of this DHCP
                     bindings."
        ::= { dhcpSnoopBindingsEntry 7 }

--

dhcpSnoopTotalForwardedPkts     OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the total number of packets subjected to
                     DHCP Snooping is forwarded."
        ::= { dhcpSnoopStatistics 1 }

dhcpSnoopUntrustedPortDroppedPkts   OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the number of packets subjected to DHCP Snooping
                     is dropped because they come from untrusted interface."
        ::= { dhcpSnoopStatistics 3 }

--
-- clusterMgt
--

clusterEnable  OBJECT-TYPE
    SYNTAX     EnabledStatus
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Enables or disables clustering on the device."
    ::= { clusterMgt 1 }

clusterCommanderEnable  OBJECT-TYPE
    SYNTAX     EnabledStatus
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Enables or disables the device as commander in a cluster."
    ::= { clusterMgt 2 }

clusterIpPool  OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The start internal IP address of a cluster pool."
    ::= { clusterMgt 4 }

clusterClearCandidateTable  OBJECT-TYPE
    SYNTAX     INTEGER
    					 {
    					     noClear(1),
    					     clear(2)
    					 }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Setting this object to clear(2) starts to clear the candidate table."
    ::= { clusterMgt 5 }

clusterRole  OBJECT-TYPE
    SYNTAX     INTEGER
               {
                   commander(1),
                   candidate(2),
                   activeMember(3),
                   disabled(5)
               }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The current role of the device in a cluster.
             commander(1)   : The switch is the controlling device in a
                              cluster.
             candidate(2)   : The switch has been discovered by the commander,
                              but it has not been manually configured
                              for access from the commander.
             activeMember(3): The switch has been manually configured for access
                              from the commander and it is active
                              in the cluster.
             disabled(5)     : The switch has clustering disabled."
    ::= { clusterMgt 6 }

clusterMemberCount  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The total number of members in a cluster."
    ::= { clusterMgt 7 }

clusterCandidateCount  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The total number of candidates in a cluster."
    ::= { clusterMgt 8 }

clusterCandidateTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF ClusterCandidateEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table listing cluster candidates."
    ::= { clusterMgt 9 }

clusterCandidateEntry OBJECT-TYPE
    SYNTAX     ClusterCandidateEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A conceptual row containing the information of the candidate."
    INDEX { clusterCandidateMacAddr}
    ::= { clusterCandidateTable 1 }

ClusterCandidateEntry ::=
    SEQUENCE {
                clusterCandidateMacAddr  MacAddress,
                clusterCandidateDesc     DisplayString,
                clusterCandidateRole     INTEGER
    }

clusterCandidateMacAddr OBJECT-TYPE
       SYNTAX     MacAddress
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "The MAC address of the candidate."
       ::= {clusterCandidateEntry  1 }

clusterCandidateDesc OBJECT-TYPE
       SYNTAX     DisplayString (SIZE (0..42))
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The description of the candidate."
       ::= {clusterCandidateEntry  3 }

clusterCandidateRole OBJECT-TYPE
       SYNTAX     INTEGER
                  {
                      candidate(2),
                      activeMember(3),
                      inactiveMember(4)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The role of the candidate.
                candidate(2)     : The switch is discovered by the commander,
                                   but it has not been manually configured for
                                   access from the commander.
                activeMember(3)  : The switch is manually configured for access
                                   from the commander and it is active in the
                                   cluster.
                inactiveMember(4): The switch is manually configured for access
                                   from the commander, but it is inactive in
                                   the cluster."
       ::= {clusterCandidateEntry  4 }

clusterMemberTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF ClusterMemberEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table listing clustering members."
    ::= { clusterMgt 10 }

clusterMemberEntry OBJECT-TYPE
    SYNTAX     ClusterMemberEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
          "A conceptual row containing the information of the member."
    INDEX { clusterMemberId}
    ::= { clusterMemberTable 1 }

ClusterMemberEntry ::=
    SEQUENCE {
                clusterMemberId       Unsigned32,
                clusterMemberMacAddr  MacAddress,
                clusterMemberDesc     DisplayString,
                clusterMemberActive   INTEGER
             }

clusterMemberId OBJECT-TYPE
       SYNTAX     Unsigned32
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "The ID of the member."
       ::= {clusterMemberEntry  1 }

clusterMemberMacAddr OBJECT-TYPE
       SYNTAX     MacAddress
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The MAC address of the member."
       ::= {clusterMemberEntry  2 }

clusterMemberDesc OBJECT-TYPE
       SYNTAX     DisplayString(SIZE (0..42))
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The description of the member."
       ::= {clusterMemberEntry  3 }

clusterMemberActive OBJECT-TYPE
       SYNTAX     INTEGER
                  {
                      activeMember(3),
                      inactiveMember(4)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The active status of the member.
                activeMember(3)  : The switch is manually configured for access
                                   from the commander and it is active in the
                                   cluster.
                inactiveMember(4): The switch is manually configured for access
                                   from the commander, but it is inactive in
                                   the cluster."
       ::= {clusterMemberEntry  4 }

clusterMemberAddCtl  OBJECT IDENTIFIER ::= { clusterMgt 11 }

clusterMemberAddCtlMacAddr  OBJECT-TYPE
    SYNTAX     MacAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The MAC address of the device associated with clusterMemberAddCtlAction."
    ::= { clusterMemberAddCtl 1 }

clusterMemberAddCtlId  OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The member id associated with clusterMemberAddCtlAction."
    ::= { clusterMemberAddCtl 2 }

clusterMemberAddCtlAction  OBJECT-TYPE
    SYNTAX     INTEGER
               {
                   noAdd(1),
                   add(2)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Adds the device to members that can be accessed from the commander.
         The MAC of the device is the current value of
         clusterMemberAddCtlMacAddr and the assigned member ID is the current
         value of clusterMemberAddCtlId. Set this object to add(2) to begin
         adding the member."
    ::= { clusterMemberAddCtl 5 }

clusterMemberRemoveCtl  OBJECT IDENTIFIER ::= { clusterMgt 12 }

clusterMemberRemoveCtlId  OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "The member ID associated with clusterMemberRemoveCtlAction."
    ::= { clusterMemberRemoveCtl 1 }

clusterMemberRemoveCtlAction  OBJECT-TYPE
    SYNTAX     INTEGER
               {
                   noRemove(1),
                   remove(2)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Removes the device from members that can be accessed from the commander.
         The member ID is the current value of clusterMemberRemoveCtlId.
         Set this object to remove(2) to begin removing the member."
    ::= { clusterMemberRemoveCtl 2 }

--
-- ipSrcGuardMgt
--

ipSrcGuardConfigTable       OBJECT-TYPE
        SYNTAX      SEQUENCE OF IpSrcGuardConfigEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table contains the configurations to enable or disable
                     IP Source Guard at each port or trunk."
        ::= { ipSrcGuardMgt 1 }

ipSrcGuardConfigEntry       OBJECT-TYPE
        SYNTAX      IpSrcGuardConfigEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An instance contains the configuration to enable
                     or disable IP Source Guard at each port or trunk."
        INDEX       { ipSrcGuardPortIfIndex }
        ::= { ipSrcGuardConfigTable 1 }

IpSrcGuardConfigEntry       ::= SEQUENCE
{
        ipSrcGuardPortIfIndex       InterfaceIndex,
        ipSrcGuardMode              INTEGER,
        ipSrcGuardMaxBinding        Integer32
}

ipSrcGuardPortIfIndex       OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This object idents the port or trunk which is capable of
                     IP Source Guard feature."
        ::= { ipSrcGuardConfigEntry 1 }

ipSrcGuardMode      OBJECT-TYPE
        SYNTAX      INTEGER { diabled(0), srcIp(1), srcIpMac(2) }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This object indicates whether Ip Source Guard is enabled
                     at this interface. If the value equals 0, it means Ip Source
                     Guard  is disabled. If the value equals 1, it means Ip Source
                     Guard is enabled, and packets are filtered by checking source ip.
                     If the value equals 2, it means Ip Source Guard is enabled
                     and packets are filtered by checking source ip and source mac."
        ::= { ipSrcGuardConfigEntry 2 }

ipSrcGuardMaxBinding     OBJECT-TYPE
        SYNTAX      Integer32 (1..5)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Limits maximum binding entries for this interface."
        ::= { ipSrcGuardConfigEntry 3 }
--
ipSrcGuardAddrTable     OBJECT-TYPE
        SYNTAX      SEQUENCE OF IpSrcGuardAddrEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table contains the IP Source Guard bindings information
                     learnt by the device."
        ::= { ipSrcGuardMgt 2 }

ipSrcGuardAddrEntry     OBJECT-TYPE
        SYNTAX      IpSrcGuardAddrEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An instance contains the Mac address, IP address type,
                     IP address, VLAN number, interface number, leased time and
                     status."
        INDEX   { ipSrcGuardBindingsVlanIndex, ipSrcGuardBindingsMacAddress }
        ::= { ipSrcGuardAddrTable 1 }

IpSrcGuardAddrEntry     ::= SEQUENCE
{
        ipSrcGuardBindingsVlanIndex         VlanIndex,
        ipSrcGuardBindingsMacAddress        MacAddress,
        ipSrcGuardBindingsAddrType          InetAddressType,
        ipSrcGuardBindingsEntryType         INTEGER,
        ipSrcGuardBindingsIpAddress         IpAddress,
        ipSrcGuardBindingsPortIfIndex       InterfaceIndex,
        ipSrcGuardBindingsLeaseTime         Unsigned32,
        ipSrcGuardBindingsStatus         RowStatus
}
ipSrcGuardBindingsVlanIndex      OBJECT-TYPE
        SYNTAX      VlanIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This object indicates the VLAN which a DHCP client host
                     belongs to."
        ::= { ipSrcGuardAddrEntry 1 }

ipSrcGuardBindingsMacAddress     OBJECT-TYPE
        SYNTAX      MacAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This object indicates the MAC address of a DHCP client
                     host."
        ::= { ipSrcGuardAddrEntry 2 }

ipSrcGuardBindingsAddrType       OBJECT-TYPE
        SYNTAX      InetAddressType
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "This object indicates the type of IP address denoted in
                     ipSrcGuardBindingsIpAddress type."
        ::= { ipSrcGuardAddrEntry 3 }

ipSrcGuardBindingsEntryType     OBJECT-TYPE
        SYNTAX      INTEGER { dynamic(1), static(3) }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This object indicates that this binding is obtained from
                     dynamically learning or is a static configuraion."
        ::= { ipSrcGuardAddrEntry 4 }

ipSrcGuardBindingsIpAddress     OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "This object indicates the allocated IP address of
                     a DHCP client host."
        ::= { ipSrcGuardAddrEntry 5 }

ipSrcGuardBindingsPortIfIndex   OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "This object indicates the port or trunk where a DHCP client
                     host connects to."
        ::= { ipSrcGuardAddrEntry 6 }

ipSrcGuardBindingsLeaseTime     OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This object indicates the leased time of this DHCP
                     bindings."
        ::= { ipSrcGuardAddrEntry 7 }

ipSrcGuardBindingsStatus     OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The status of this conceptual row entry. This object issued to
                     manage the creation and deletion of conceptual rows.
                     The status column has six defined values:  - 'active', which
                     indicates that the conceptual row is available for use by the
                     managed device;  - 'notInService', which indicates that the
                     conceptual row exists in the agent, but is unavailable for use
                     by the managed device."
        ::= { ipSrcGuardAddrEntry 8 }

--
-- upnpMgt
--

upnpStatus     OBJECT-TYPE
    SYNTAX      EnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Sets enabled(1) to enable UPnP device, and sets disabled(2) to
                 disable UPnP device."
    ::= { upnpMgt 1 }

upnpAdvertisingDuration     OBJECT-TYPE
    SYNTAX      Integer32 (60..86400)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The interval(in seconds) between available UPnP device advertising
                 messages sent by the switch."
    ::= { upnpMgt 2 }

upnpTtl    OBJECT-TYPE
    SYNTAX      INTEGER (1..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the TTL value of the UPnP advertising messages sent by
                 the switch. When the TTL value is greater than 1, it is possible
                 to send UPnP advertising messages to traverse multiple routers;
                 at the same time, the UPnP device will send an IGMP Join message
                 to the traverse multiple routers so that the routers will forward
                 multicast messages to the UPnP device."
    ::= { upnpMgt 3 }

--
-- dynamicArpInspectionMgt
--

daiGlobal           OBJECT IDENTIFIER ::= { dynamicArpInspectionMgt 1 }
daiVlan             OBJECT IDENTIFIER ::= { dynamicArpInspectionMgt 2 }
daiInterface        OBJECT IDENTIFIER ::= { dynamicArpInspectionMgt 3 }
daiLog              OBJECT IDENTIFIER ::= { dynamicArpInspectionMgt 4 }
daiStatistics       OBJECT IDENTIFIER ::= { dynamicArpInspectionMgt 5 }

daiGlobalStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Set enabled(1) to enable dynamic ARP inspection.
                     Set disabled(2) to disable dynamic ARP inspection."
        ::= { daiGlobal 1 }

daiGlobalSrcMacValidation OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Set enabled(1) to enable validation of source MAC address.
                     Set disabled(2) to disable validation of source MAC
                     address."
        ::= { daiGlobal 2 }

daiGlobalDestMacValidation OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Set enabled(1) to enable validation of destination
                     MAC address. Set disabled(2) to disable validation
                     of destination MAC address."
        ::= { daiGlobal 3 }

daiGlobalIpAddrValidation OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Set enabled(1) to enable validation of IP address.
                     Set disabled(2) to disable validation of IP address."
        ::= { daiGlobal 4 }

daiGlobalLogNumber OBJECT-TYPE
        SYNTAX      Integer32(0..256)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The number of log buffers for saving log message.
                     The value 0 means not generating system messages."
        ::= { daiGlobal 5 }

daiGlobalLogInterval OBJECT-TYPE
        SYNTAX      Integer32(0..86400)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The value of the time interval for saving log messages."
        ::= { daiGlobal 6 }

daiGlobalAdditionalValidStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The vaule of this object is disabled(2) when the status of
                     daiGlobalSrcMacValidation, daiGlobalDestMacValidation,
                     and daiGlobalIpAddrValidation are disabled; enabled(1)
                     when one or more of these variables are enabled."
        ::= { daiGlobal 7 }

daiVlanTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DaiVlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table contains dynamic ARP inspection configurations
                     for existing VLANs."
        ::= { daiVlan 1 }

daiVlanEntry OBJECT-TYPE
        SYNTAX      DaiVlanEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An instance containing the configuration of dynamic ARP
                     inspection for each existing VLAN."
        INDEX       { daiVlanIndex }
        ::= { daiVlanTable 1 }

DaiVlanEntry  ::= SEQUENCE
{
        daiVlanIndex          VlanIndex,
        daiVlanStatus         EnabledStatus,
        daiVlanArpAclName     DisplayString,
        daiVlanArpAclStatus   INTEGER
}

daiVlanIndex OBJECT-TYPE
        SYNTAX      VlanIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This object indicates the VLAN ID on which dynamic ARP
                     inspection is configured."
        ::= { daiVlanEntry 1 }

daiVlanStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This object indicates whether dynamic ARP inspection
                     is enabled in this VLAN."
        ::= { daiVlanEntry 2 }

daiVlanArpAclName OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..15))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Specifies the ARP ACL name bound to the interface.
                     The default value of daiVlanArpAclStatus is dynamic(2)."
        ::= { daiVlanEntry 3 }

daiVlanArpAclStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        static(1),
                        dynamic(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Set to static(1) means packets not matching the ACL are
                     dropped. Set to dynamic(2) means packets not matching the
                     ACL are validated by the DHCP snooping binding table.
                     When daiVlanArpAclName is configured, the default value
                     of daiVlanArpAclStatus is dynamic(2)."
        ::= { daiVlanEntry 4 }

daiPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DaiPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table containing dynamic ARP inspection configurations
                     for port interfaces."
        ::= { daiInterface 1 }

daiPortEntry OBJECT-TYPE
        SYNTAX      DaiPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An instance containing the configuration of dynamic ARP
                     inspection at each port interface."
        INDEX       { daiPortIfIndex }
        ::= { daiPortTable 1 }

DaiPortEntry    ::= SEQUENCE
{
        daiPortIfIndex           InterfaceIndex,
        daiPortTrustStatus       EnabledStatus,
        daiPortRateLimit         Unsigned32
}

daiPortIfIndex OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The ifIndex value of the port."
        ::= { daiPortEntry 1 }

daiPortTrustStatus OBJECT-TYPE
        SYNTAX      EnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This object indicates whether the port is trusted for
                     dynamic ARP inspection."
        ::= { daiPortEntry 2 }

daiPortRateLimit OBJECT-TYPE
        SYNTAX      Unsigned32(0..2048|'FFFFFFFF'h)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The value of rate limit threshold per second of disposing
                     ARP messages. Set the value 0xFFFFFFFF as no rate limit."
        ::= { daiPortEntry 3 }

daiLogTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF DaiLogEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table containing dynamic ARP inspection log
                     information."
        ::= { daiLog 1 }

daiLogEntry OBJECT-TYPE
        SYNTAX      DaiLogEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An instance containing log information of dynamic ARP
                     inspection at each VLAN interface."
        INDEX       { daiLogIndex }
        ::= { daiLogTable 1 }

DaiLogEntry    ::= SEQUENCE
{
        daiLogIndex          Integer32,
        daiLogVlan           VlanIndex,
        daiLogPort           InterfaceIndex,
        daiLogSrcIpAddress   IpAddress,
        daiLogDestIpAddress  IpAddress,
        daiLogSrcMacAddress  MacAddress,
        daiLogDestMacAddress MacAddress
}

daiLogIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This object indicates the index of dynamic ARP
                     inspection log information."
        ::= { daiLogEntry 1 }

daiLogVlan OBJECT-TYPE
        SYNTAX      VlanIndex
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This object indicates the VLAN ID of dynamic ARP
                     inspection log information."
        ::= { daiLogEntry 2 }

daiLogPort OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This object indicates the ifIndex of dynamic ARP
                     inspection log information."
        ::= { daiLogEntry 3 }

daiLogSrcIpAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The source IP address of dynamic ARP inspection
                     log information."
        ::= { daiLogEntry 4 }

daiLogDestIpAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The destination IP address of dynamic ARP inspection
                     log information."
        ::= { daiLogEntry 5 }

daiLogSrcMacAddress OBJECT-TYPE
        SYNTAX      MacAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The source MAC address of dynamic ARP inspection
                     log information."
        ::= { daiLogEntry 6 }

daiLogDestMacAddress OBJECT-TYPE
        SYNTAX      MacAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The destination MAC address of dynamic ARP inspection
                     log information."
        ::= { daiLogEntry 7 }

daiTotalReceivedPkts OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the total number of ARP packets received
                     before rate limiting."
        ::= { daiStatistics 1 }

daiTotalDroppedPkts OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the total number of ARP packets dropped
                     due to rate limt."
        ::= { daiStatistics 2 }

daiTotalProcessedPkts OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the total number of ARP packets processed
                     by ARP inspection."
        ::= { daiStatistics 3 }

daiTotalSrcMacDroppedPkts OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the total number of ARP packets dropped
                     by source MAC address validation."
        ::= { daiStatistics 4 }

daiTotalDestMacDroppedPkts OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the total number of ARP packets dropped
                     by destination MAC address validation."
        ::= { daiStatistics 5 }

daiTotalIpAddrDroppedPkts OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the total number of ARP packets dropped
                     by IP address validation."
        ::= { daiStatistics 6 }

daiTotalArpAclDroppedPkts OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the total number of ARP packets dropped
                     by ARP ACL."
        ::= { daiStatistics 7 }

daiTotalDhcpSnoopingDroppedPkts OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the total number of ARP packets dropped
                     by DHCP snooping."
        ::= { daiStatistics 8 }

--
-- time range
--

timeRangeTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF TimeRangeEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for time range."
        ::= { timeRangeMgt 1 }

timeRangeEntry OBJECT-TYPE
        SYNTAX      TimeRangeEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for time range."
        INDEX       { timeRangeIndex }
        ::= { timeRangeTable 1 }

TimeRangeEntry ::= SEQUENCE
{
        timeRangeIndex         Integer32,
        timeRangeName          DisplayString,
        timeRangeAbsoluteTime  DisplayString,
        timeRangeStatus        ValidStatus
}

timeRangeIndex OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION "The index of time range entry."
        ::= { timeRangeEntry 1 }

timeRangeName OBJECT-TYPE
        SYNTAX       DisplayString (SIZE (1..16))
        MAX-ACCESS   read-write
        STATUS       current
        DESCRIPTION "The name of time range entry."
        ::= { timeRangeEntry 2 }

timeRangeAbsoluteTime OBJECT-TYPE
        SYNTAX       DisplayString (SIZE(0..37))
        MAX-ACCESS   read-write
        STATUS       current
        DESCRIPTION "Specifies the absolute time of the entry. This is a text
                     string in the following form, based on Unix:
                     'Mmm _d yyyy hh:mm - Mmm _d yyyy hh:mm'. 'Mmm' are the
                     first three letters of the month. '_d' is the day of month.
                     A single-digit day is preceded by a space. 'yyyy' is a
                     four-digit year. The range is from 2001 to 2100.
                     'hh:mm' is a 24-hour representation of hours and minutes.
                     A single-digit hour or minute is preceded by a zero.
                     An example is: 'Jul  1 2002 00:00 - Oct  1 2002 00:00'.
                     Uses empty to revert to default value. When there is no
                     start time, uses the format '- Mmm _d yyyy hh:mm'. When
                     there is no end time, uses the format 'Mmm _d yyyy hh:mm -'.
                     Uses empty to clear absolute time setting."
        ::= { timeRangeEntry 3 }

timeRangeStatus OBJECT-TYPE
        SYNTAX       ValidStatus
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION "Setting this to valid(1) creates an entry.
                     Setting this to invalid(2) destroys an entry."
        ::= { timeRangeEntry 4 }

timeRangePeriodicTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF TimeRangePeriodicEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table for time range rules."
        ::= { timeRangeMgt 2 }

timeRangePeriodicEntry OBJECT-TYPE
        SYNTAX      TimeRangePeriodicEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry for time range rules."
        INDEX       { timeRangePeriodicIndex, timeRangePeriodicRuleIndex }
        ::= { timeRangePeriodicTable 1 }

TimeRangePeriodicEntry ::= SEQUENCE
{
        timeRangePeriodicIndex     Integer32,
        timeRangePeriodicRuleIndex Integer32,
        timeRangePeriodicTime      DisplayString,
        timeRangePeriodicStatus    ValidStatus
}

timeRangePeriodicIndex OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION "The index of time range entry. The object
                     should exist in timeRangeIndex of timeRangeTable."
        ::= { timeRangePeriodicEntry 1 }

timeRangePeriodicRuleIndex OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION "The index of time range rule."
        ::= { timeRangePeriodicEntry 2 }

timeRangePeriodicTime OBJECT-TYPE
        SYNTAX       DisplayString(SIZE(0..21))
        MAX-ACCESS   read-write
        STATUS       current
        DESCRIPTION "Specifies the period time of the entry. This is a text
                     string in the following form, based on Unix:
                     'Ddd hh:mm - Ddd hh:mm'. 'Ddd' are the first three
                     letters of day of the week, 'Day' which means daily,
                     'Wky' which means weekday, or 'Wkd' which means weekend.
                     If 'Ddd' is one of 'Day', 'Wky', and 'Wkd', the start
                     'Ddd' should be the same as end 'Ddd'. 'hh:mm' is a
                     24-hour representation of hours and minutes. A
                     single-digit hour or minute is preceded by a zero. An
                     example is: 'Sun 00:00 - Sat 00:00'. Uses empty to revert
                     to default value."
        ::= { timeRangePeriodicEntry 3 }

timeRangePeriodicStatus OBJECT-TYPE
        SYNTAX       ValidStatus
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION "Setting this to valid(1) creates an periodic entry.
                     Setting this to invalid(2) destroys an periodic entry."
        ::= { timeRangePeriodicEntry 4 }


--
-- trap definitions
--

ipecsEs3000Traps  OBJECT IDENTIFIER ::= { ipecsEs3000Notifications  1 }
ipecsEs3000TrapsPrefix OBJECT IDENTIFIER ::= { ipecsEs3000Traps 0 }

swPowerStatusChangeTrap NOTIFICATION-TYPE
        OBJECTS     { swIndivPowerUnitIndex, swIndivPowerIndex, swIndivPowerStatus }
        STATUS      current
        DESCRIPTION "This trap is sent when the power state changes."
        ::= { ipecsEs3000TrapsPrefix 1 }

swFanFailureTrap NOTIFICATION-TYPE
        OBJECTS     { switchUnitIndex, switchFanIndex }
        STATUS   current
        DESCRIPTION "This trap is sent when the fan has failed."
        ::= { ipecsEs3000TrapsPrefix 17 }

swFanRecoverTrap NOTIFICATION-TYPE
        OBJECTS     { switchUnitIndex, switchFanIndex }
        STATUS   current
        DESCRIPTION "This trap is sent when fan failure has recovered."
        ::= { ipecsEs3000TrapsPrefix 18 }

swPortSecurityTrap NOTIFICATION-TYPE
        OBJECTS     {
                        ifIndex,
                        trapPortSecurityIntrusionMac
                    }
        STATUS      current
        DESCRIPTION "This trap is sent when the port is being intruded. This trap
                     will only be sent when the portSecActionTrap is enabled."
        ::= { ipecsEs3000TrapsPrefix 36 }

swAuthenticationFailure NOTIFICATION-TYPE
        OBJECTS     { trapLoginMode, trapLoginUsername, trapLoginIp }
        STATUS      current
        DESCRIPTION "This trap will be triggered if authentication is failed."
        ::= { ipecsEs3000TrapsPrefix 66 }

swAuthenticationSuccess NOTIFICATION-TYPE
        OBJECTS     { trapLoginMode, trapLoginUsername, trapLoginIp }
        STATUS      current
        DESCRIPTION "This trap will be triggered if authentication is successful."
        ::= { ipecsEs3000TrapsPrefix 67 }

--
-- ATC trap ASE3528B-E1-FLF-P5-00011
--

swAtcBcastStormAlarmFireTrap NOTIFICATION-TYPE
        OBJECTS     {
                        atcBcastStormIfIndex,
                        atcBcastStormSampleType,
                        atcBcastStormCurrentTrafficRate,
                        atcBcastStormAlarmFireThreshold
                    }
        STATUS      current
        DESCRIPTION
            "When the broadcast traffic is detected as the storm, this trap
             will be fired."
        ::= { ipecsEs3000TrapsPrefix 70 }

swAtcBcastStormAlarmClearTrap NOTIFICATION-TYPE
        OBJECTS     {
                        atcBcastStormIfIndex,
                        atcBcastStormSampleType,
                        atcBcastStormCurrentTrafficRate,
                        atcBcastStormAlarmClearThreshold
                    }
        STATUS      current
        DESCRIPTION
            "When the broadcast storm is detected as the normal traffic, this
             trap will be fired."
        ::= { ipecsEs3000TrapsPrefix 71 }

swAtcBcastStormTcApplyTrap NOTIFICATION-TYPE
        OBJECTS     {
                        atcBcastStormIfIndex,
                        atcBcastStormSampleType,
                        atcBcastStormCurrentTrafficRate,
                        atcBcastStormAlarmFireThreshold,
                        atcBcastStormTcApplyTime
                    }
        STATUS      current
        DESCRIPTION
            "When the ATC is activated, this trap will be fired."
        ::= { ipecsEs3000TrapsPrefix 72 }

swAtcBcastStormTcReleaseTrap NOTIFICATION-TYPE
        OBJECTS     {
                        atcBcastStormIfIndex,
                        atcBcastStormSampleType,
                        atcBcastStormCurrentTrafficRate,
                        atcBcastStormAlarmClearThreshold,
                        atcBcastStormTcReleaseTime
                    }
        STATUS      current
        DESCRIPTION
            "When the ATC is released, this trap will be fired."
        ::= { ipecsEs3000TrapsPrefix 73 }

swAtcMcastStormAlarmFireTrap      NOTIFICATION-TYPE
        OBJECTS     {
                        atcMcastStormIfIndex,
                        atcMcastStormSampleType,
                        atcMcastStormCurrentTrafficRate,
                        atcMcastStormAlarmFireThreshold
                    }
        STATUS      current
        DESCRIPTION
            "When the multicast traffic is detected as the storm, this trap
             will be fired."
        ::= { ipecsEs3000TrapsPrefix 74 }

swAtcMcastStormAlarmClearTrap NOTIFICATION-TYPE
        OBJECTS     {
                        atcMcastStormIfIndex,
                        atcMcastStormSampleType,
                        atcMcastStormCurrentTrafficRate,
                        atcMcastStormAlarmClearThreshold
                    }
        STATUS      current
        DESCRIPTION
            "When the multicast storm is detected as the normal traffic, this
             trap will be fired."
        ::= { ipecsEs3000TrapsPrefix 75 }

swAtcMcastStormTcApplyTrap NOTIFICATION-TYPE
        OBJECTS     {
                        atcMcastStormIfIndex,
                        atcMcastStormSampleType,
                        atcMcastStormCurrentTrafficRate,
                        atcMcastStormAlarmFireThreshold,
                        atcMcastStormTcApplyTime
                    }
        STATUS      current
        DESCRIPTION
            "When the ATC is activated, this trap will be fired."
        ::= { ipecsEs3000TrapsPrefix 76 }

swAtcMcastStormTcReleaseTrap NOTIFICATION-TYPE
        OBJECTS     {
                        atcMcastStormIfIndex,
                        atcMcastStormSampleType,
                        atcMcastStormCurrentTrafficRate,
                        atcMcastStormAlarmClearThreshold,
                        atcMcastStormTcReleaseTime
                    }
        STATUS      current
        DESCRIPTION
            "When the ATC is released, this trap will be fired."
        ::= { ipecsEs3000TrapsPrefix 77 }

stpBecomeRootBridgeTrap NOTIFICATION-TYPE
        OBJECTS     { trapMstInstanceId, dot1dStpDesignatedRoot }
        STATUS      current
        DESCRIPTION "The stpBecomeRootBridge trap indicates that the sending
                     agent has become the new root of the Spanning Tree; the
                     trap is sent by a bridge soon after it has been elected as
                     the new root. When spanning tree algorithm is STP or RSTP,
                     trapMstInstanceId is always 0 and meaningless."
        ::= { ipecsEs3000TrapsPrefix 86 }

stpPortEnterForwardingTrap NOTIFICATION-TYPE
        OBJECTS     { trapMstInstanceId, ifIndex }
        STATUS      current
        DESCRIPTION "The trap is sent by a bridge when any of its configured
                     ports transit from Learning state to Forwarding state.
                     When spanning tree algorithm is STP or RSTP,
                     trapMstInstanceId is always 0 and meaningless."
        ::= { ipecsEs3000TrapsPrefix 87 }

stpRootPortChangedTrap NOTIFICATION-TYPE
        OBJECTS     { trapMstInstanceId, dot1dStpRootPort }
        STATUS      current
        DESCRIPTION "The trap is sent when the root port of a bridge has
                     changed. When spanning tree algorithm is STP or RSTP,
                     trapMstInstanceId is always 0 and meaningless."
        ::= { ipecsEs3000TrapsPrefix 88 }

stpRootBridgeChangedTrap NOTIFICATION-TYPE
        OBJECTS     { trapMstInstanceId, dot1dStpDesignatedRoot }
        STATUS      current
        DESCRIPTION "The trap will be sent when the root bridge of bridges has
                     changed and the bridge sending off the trap is not the root
                     in STP topology. When spanning tree algorithm is STP or
                     RSTP, trapMstInstanceId is always 0 and meaningless."
        ::= { ipecsEs3000TrapsPrefix 89 }

swLoopbackDetectionTrap NOTIFICATION-TYPE
        OBJECTS     { staLoopbackDetectionPortIfIndex }
        STATUS   current
        DESCRIPTION "This trap will be sent when loopback BPDUs have been detected."
        ::= { ipecsEs3000TrapsPrefix 95}

autoUpgradeTrap NOTIFICATION-TYPE
        OBJECTS     {
                        fileCopyFileType,
                        trapAutoUpgradeResult,
                        trapAutoUpgradeNewVer
                    }
        STATUS      current
        DESCRIPTION "This trap is sent when auto upgrade is executed."
        ::= { ipecsEs3000TrapsPrefix 104 }

swCpuUtiRisingNotification NOTIFICATION-TYPE
        STATUS      current
        DESCRIPTION
              "This notification indicates that the CPU utilization has risen
               from cpuUtiFallingThreshold to cpuUtiRisingThreshold."
        ::= { ipecsEs3000TrapsPrefix 107 }

swCpuUtiFallingNotification NOTIFICATION-TYPE
        STATUS      current
        DESCRIPTION
              "This notification indicates that the CPU utilization has fallen
               from cpuUtiRisingThreshold to cpuUtiFallingThreshold."
        ::= { ipecsEs3000TrapsPrefix 108 }

swMemoryUtiRisingThresholdNotification NOTIFICATION-TYPE
        STATUS      current
        DESCRIPTION
              "This notification indicates that the memory utilization has risen
               from memoryUtiFallingThreshold to memoryUtiRisingThreshold."
        ::= { ipecsEs3000TrapsPrefix 109 }

swMemoryUtiFallingThresholdNotification NOTIFICATION-TYPE
        STATUS      current
        DESCRIPTION
              "This notification indicates that the memory utilization has fallen
               from memoryUtiRisingThreshold to memoryUtiFallingThreshold."
        ::= { ipecsEs3000TrapsPrefix 110 }

swIpFilterInetRejectTrap NOTIFICATION-TYPE
    OBJECTS {
                trapIpFilterRejectMode,
                trapIpFilterRejectInetAddressType,
                trapIpFilterRejectInetAddress
            }
    STATUS  current
    DESCRIPTION
            "This trap is sent when an incorrect IP address is rejected
             by the IP filter."
    ::= { ipecsEs3000TrapsPrefix 111 }

stpLoopbackDetectionPortShutdownTrap NOTIFICATION-TYPE
    OBJECTS     {
                    ifIndex
                }
    STATUS      current
    DESCRIPTION "This trap is sent when port is shut down by STP loopback
                 detection."
    ::= { ipecsEs3000TrapsPrefix 193 }

END
